a3c0fe7a: ndt_1c Msg: Querying if miniport is wireless
a3c0fe7a: ndt_1c Msg: Miniport AX88772B1 is ** NOT Wireless-LAN **
<TESTGROUP>

*** ==================================================================
*** SUITE INFORMATION
***
*** Suite Name:        N/A (built on the fly)
*** Suite Description: N/A
*** Number of Tests:   13
*** ==================================================================

*** ==================================================================
*** SYSTEM INFORMATION
***
*** Date and Time:          06/15/2010 10:19 AM (Tuesday)
***
*** Device Name:            CEPC
***
*** OS Version:             5.0
*** Build Number:           1400
*** Platform ID:            3 "Windows CE"
*** Version String:         ""
***
*** Processor Type:         0x000002AE (686) "Intel Pentium II"
*** Processor Architecture: 0x0000     (0) "Intel"
*** Page Size:              0x00001000 (4,096)
*** Minimum App Address:    0x00010000 (65,536)
*** Maximum App Address:    0x7FFFFFFF (2,147,483,647)
*** Active Processor Mask:  0x00000001
*** Number Of Processors:   1
*** Allocation Granularity: 0x00010000 (65,536)
*** Processor Level:        0x0003     (3)
*** Processor Revision:     0x0004     (4)
*** ==================================================================

*** ==================================================================
*** MEMORY INFO
***
*** Memory Total:    24,092,672 bytes
*** Memory Used:      5,693,440 bytes
*** Memory Free:     18,399,232 bytes
***
*** Kernel Used:        552,960 bytes
*** Water Mark:           4,491 pages
***
*** Store Total:     24,027,136 bytes
*** Store Used:         572,256 bytes
*** Store Free:      23,454,880 bytes
*** ==================================================================

BEGIN GROUP: ndt_1c.dll
<TESTCASE ID=1>
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
*** TEST STARTING
***
*** Test Name:      1c_OpenClose
*** Test ID:        1
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX88772B1
*** Random Seed:    6895
*** Thread Count:   0
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_OpenClose", Threads=0, Seed=6895
      a3c0fe7a: ndt_1c Msg: Start 1c_OpenClose test on the adapter AX88772B1
      a3c0fe7a: ndt_1c Msg: Opening adapter
      a3c0fe7a: ndt_1c Msg: Repeatedly binding and unbinding the adapter
      a3c0fe7a: ndt_1c Msg: Open and bind the adapter multiple times, then close each open instance
      a3c0fe7a: ndt_1c Msg: Opening 128 adapter instances (pass #0)
      a3c0fe7a: ndt_1c Msg: Closing all adapter instances
      a3c0fe7a: ndt_1c Msg: Opening 128 adapter instances (pass #1)
      a3c0fe7a: ndt_1c Msg: Closing all adapter instances
      a3c0fe7a: ndt_1c Msg: Opening 128 adapter instances (pass #2)
      a3c0fe7a: ndt_1c Msg: Closing all adapter instances
      a3c0fe7a: ndt_1c Msg: Opening 128 adapter instances (pass #3)
      a3c0fe7a: ndt_1c Msg: Closing all adapter instances
      a3c0fe7a: ndt_1c Msg: Opening 128 adapter instances (pass #4)
      a3c0fe7a: ndt_1c Msg: Closing all adapter instances
      a3c0fe7a: ndt_1c Msg: Opening 128 adapter instances (pass #5)
      a3c0fe7a: ndt_1c Msg: Closing all adapter instances
      a3c0fe7a: ndt_1c Msg: Opening 128 adapter instances (pass #6)
      a3c0fe7a: ndt_1c Msg: Closing all adapter instances
      a3c0fe7a: ndt_1c Msg: Opening 128 adapter instances (pass #7)
      a3c0fe7a: ndt_1c Msg: Closing all adapter instances
      a3c0fe7a: ndt_1c Msg: Opening 128 adapter instances (pass #8)
      a3c0fe7a: ndt_1c Msg: Closing all adapter instances
      a3c0fe7a: ndt_1c Msg: Opening 128 adapter instances (pass #9)
      a3c0fe7a: ndt_1c Msg: Closing all adapter instances
      a3c0fe7a: ndt_1c Msg: Opening 128 adapter instances (pass #10)
      a3c0fe7a: ndt_1c Msg: Closing all adapter instances
      a3c0fe7a: ndt_1c Msg: Opening 128 adapter instances (pass #11)
      a3c0fe7a: ndt_1c Msg: Closing all adapter instances
      a3c0fe7a: ndt_1c Msg: Opening 128 adapter instances (pass #12)
      a3c0fe7a: ndt_1c Msg: Closing all adapter instances
      a3c0fe7a: ndt_1c Msg: Opening 128 adapter instances (pass #13)
      a3c0fe7a: ndt_1c Msg: Closing all adapter instances
      a3c0fe7a: ndt_1c Msg: Opening 128 adapter instances (pass #14)
      a3c0fe7a: ndt_1c Msg: Closing all adapter instances
      a3c0fe7a: ndt_1c Msg: Opening 128 adapter instances (pass #15)
      a3c0fe7a: ndt_1c Msg: Closing all adapter instances
      a3c0fe7a: ndt_1c Msg: Test 1c_OpenClose on the adapter AX88772B1 PASS
   END TEST: "1c_OpenClose", PASSED, Time=8.920
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
*** TEST COMPLETED
***
*** Test Name:      1c_OpenClose
*** Test ID:        1
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX88772B1
*** Result:         Passed
*** Random Seed:    6895
*** Thread Count:   1
*** Execution Time: 0:00:08.920
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

</TESTCASE RESULT="PASSED">
<TESTCASE ID=2>
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
*** TEST STARTING
***
*** Test Name:      1c_Send
*** Test ID:        2
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX88772B1
*** Random Seed:    22554
*** Thread Count:   0
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_Send", Threads=0, Seed=22554
      a3c0fe7a: ndt_1c Msg: Start 1c_Send test on the adapter AX88772B1
      a3c0fe7a: ndt_1c Msg: Getting basic info about the adapter
      a3c0fe7a: ndt_1c Msg: Get OID_GEN_MAXIMUM_TOTAL_SIZE = 1514
      a3c0fe7a: ndt_1c Msg: Get OID_GEN_MAXIMUM_FRAME_SIZE = 1500
      a3c0fe7a: ndt_1c Msg: Testing sending to a (random) directed address
      a3c0fe7a: ndt_1c Msg: Sending: Send
      a3c0fe7a: ndt_1c Msg: Sending to a random address
      a3c0fe7a: ndt_1c Msg: Sending: Send
      a3c0fe7a: ndt_1c Msg: Sending to a broadcast address
      a3c0fe7a: ndt_1c Msg: Sending: Send
      a3c0fe7a: ndt_1c Msg: Sending to a multicast/functional address
      a3c0fe7a: ndt_1c Msg: Sending: Send
      a3c0fe7a: ndt_1c Msg: Testing sending to a group of addresses
   END TEST: "1c_Send", PASSED, Time=49.441
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
*** TEST COMPLETED
***
*** Test Name:      1c_Send
*** Test ID:        2
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX88772B1
*** Result:         Passed
*** Random Seed:    22554
*** Thread Count:   1
*** Execution Time: 0:00:49.441
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

</TESTCASE RESULT="PASSED">
<TESTCASE ID=3>
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
*** TEST STARTING
***
*** Test Name:      1c_LoopbackSend
*** Test ID:        3
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX88772B1
*** Random Seed:    8154
*** Thread Count:   0
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_LoopbackSend", Threads=0, Seed=8154
      a3c0fe7a: ndt_1c Msg: Start 1c_Loopback test
      a3c0fe7a: ndt_1c Msg: The test adapter is AX88772B1
      a3c0fe7a: ndt_1c Msg: Opening adapters
      a3c0fe7a: ndt_1c Msg: Binding adapters
      a3c0fe7a: ndt_1c Msg: Get basic adapter info
      a3c0fe7a: ndt_1c Msg: Possible filter settings:
      a3c0fe7a: ndt_1c Msg:   - Directed
      a3c0fe7a: ndt_1c Msg:   - Broadcast
      a3c0fe7a: ndt_1c Msg:   - Promiscuous
      a3c0fe7a: ndt_1c Msg:   - Multicast
      a3c0fe7a: ndt_1c Msg:   - All Multicast
      a3c0fe7a: ndt_1c Msg: Setting receiving filters
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_NONE for instance 0
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+ for instance 1
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_BROADCAST+ for instance 2
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+ for instance 3
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_PROMISCUOUS+ for instance 4
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_PROMISCUOUS+ for instance 5
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      a3c0fe7a: ndt_1c Msg: Start receiving
      a3c0fe7a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Test NIC's directed Addr
      a3c0fe7a: ndt_1c Msg: Stop receiving and checking results
      a3c0fe7a: ndt_1c Msg: Instance 0 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 1 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 2 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 3 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 4 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 5 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 6 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 7 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Setting receiving filters
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+ for instance 0
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+ for instance 1
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+ for instance 2
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+ for instance 3
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      a3c0fe7a: ndt_1c Msg: Start receiving
      a3c0fe7a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Test NIC's directed Addr
      a3c0fe7a: ndt_1c Msg: Stop receiving and checking results
      a3c0fe7a: ndt_1c Msg: Instance 0 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 1 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 2 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 3 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 4 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 5 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 6 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 7 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Setting receiving filters
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+ for instance 0
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+ for instance 1
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      a3c0fe7a: ndt_1c Msg: Start receiving
      a3c0fe7a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Test NIC's directed Addr
      a3c0fe7a: ndt_1c Msg: Stop receiving and checking results
      a3c0fe7a: ndt_1c Msg: Instance 0 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 1 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 2 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 3 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 4 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 5 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 6 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 7 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Setting receiving filters
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 0
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 1
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      a3c0fe7a: ndt_1c Msg: Start receiving
      a3c0fe7a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Test NIC's directed Addr
      a3c0fe7a: ndt_1c Msg: Stop receiving and checking results
      a3c0fe7a: ndt_1c Msg: Instance 0 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 1 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 2 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 3 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 4 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 5 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 6 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 7 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Setting receiving filters
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_NONE for instance 0
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+ for instance 1
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_BROADCAST+ for instance 2
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+ for instance 3
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_PROMISCUOUS+ for instance 4
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_PROMISCUOUS+ for instance 5
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      a3c0fe7a: ndt_1c Msg: Start receiving
      a3c0fe7a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Broadcast Addr
      a3c0fe7a: ndt_1c Msg: Stop receiving and checking results
      a3c0fe7a: ndt_1c Msg: Instance 0 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 1 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 2 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 3 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 4 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 5 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 6 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 7 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Setting receiving filters
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+ for instance 0
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+ for instance 1
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+ for instance 2
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+ for instance 3
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      a3c0fe7a: ndt_1c Msg: Start receiving
      a3c0fe7a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Broadcast Addr
      a3c0fe7a: ndt_1c Msg: Stop receiving and checking results
      a3c0fe7a: ndt_1c Msg: Instance 0 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 1 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 2 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 3 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 4 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 5 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 6 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 7 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Setting receiving filters
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+ for instance 0
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+ for instance 1
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      a3c0fe7a: ndt_1c Msg: Start receiving
      a3c0fe7a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Broadcast Addr
      a3c0fe7a: ndt_1c Msg: Stop receiving and checking results
      a3c0fe7a: ndt_1c Msg: Instance 0 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 1 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 2 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 3 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 4 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 5 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 6 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 7 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Setting receiving filters
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 0
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 1
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      a3c0fe7a: ndt_1c Msg: Start receiving
      a3c0fe7a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Broadcast Addr
      a3c0fe7a: ndt_1c Msg: Stop receiving and checking results
      a3c0fe7a: ndt_1c Msg: Instance 0 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 1 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 2 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 3 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 4 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 5 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 6 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 7 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Setting receiving filters
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_NONE for instance 0
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+ for instance 1
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_BROADCAST+ for instance 2
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+ for instance 3
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_PROMISCUOUS+ for instance 4
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_PROMISCUOUS+ for instance 5
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      a3c0fe7a: ndt_1c Msg: Start receiving
      a3c0fe7a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Any directed Random Addr
      a3c0fe7a: ndt_1c Msg: Stop receiving and checking results
      a3c0fe7a: ndt_1c Msg: Instance 0 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 1 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 2 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 3 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 4 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 5 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 6 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 7 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Setting receiving filters
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+ for instance 0
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+ for instance 1
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+ for instance 2
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+ for instance 3
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      a3c0fe7a: ndt_1c Msg: Start receiving
      a3c0fe7a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Any directed Random Addr
      a3c0fe7a: ndt_1c Msg: Stop receiving and checking results
      a3c0fe7a: ndt_1c Msg: Instance 0 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 1 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 2 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 3 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 4 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 5 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 6 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 7 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Setting receiving filters
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+ for instance 0
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+ for instance 1
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      a3c0fe7a: ndt_1c Msg: Start receiving
      a3c0fe7a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Any directed Random Addr
      a3c0fe7a: ndt_1c Msg: Stop receiving and checking results
      a3c0fe7a: ndt_1c Msg: Instance 0 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 1 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 2 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 3 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 4 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 5 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 6 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 7 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Setting receiving filters
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 0
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 1
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      a3c0fe7a: ndt_1c Msg: Start receiving
      a3c0fe7a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Any directed Random Addr
      a3c0fe7a: ndt_1c Msg: Stop receiving and checking results
      a3c0fe7a: ndt_1c Msg: Instance 0 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 1 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 2 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 3 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 4 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 5 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 6 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 7 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Setting receiving filters
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_NONE for instance 0
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+ for instance 1
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_BROADCAST+ for instance 2
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+ for instance 3
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_PROMISCUOUS+ for instance 4
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_PROMISCUOUS+ for instance 5
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      a3c0fe7a: ndt_1c Msg: Start receiving
      a3c0fe7a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Multicast Addr
      a3c0fe7a: ndt_1c Msg: Stop receiving and checking results
      a3c0fe7a: ndt_1c Msg: Instance 0 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 1 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 2 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 3 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 4 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 5 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 6 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 7 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Setting receiving filters
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+ for instance 0
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+ for instance 1
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+ for instance 2
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+ for instance 3
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      a3c0fe7a: ndt_1c Msg: Start receiving
      a3c0fe7a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Multicast Addr
      a3c0fe7a: ndt_1c Msg: Stop receiving and checking results
      a3c0fe7a: ndt_1c Msg: Instance 0 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 1 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 2 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 3 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 4 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 5 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 6 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 7 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Setting receiving filters
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+ for instance 0
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+ for instance 1
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      a3c0fe7a: ndt_1c Msg: Start receiving
      a3c0fe7a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Multicast Addr
      a3c0fe7a: ndt_1c Msg: Stop receiving and checking results
      a3c0fe7a: ndt_1c Msg: Instance 0 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 1 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 2 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 3 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 4 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 5 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 6 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 7 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Setting receiving filters
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 0
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 1
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      a3c0fe7a: ndt_1c Msg: Start receiving
      a3c0fe7a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Multicast Addr
      a3c0fe7a: ndt_1c Msg: Stop receiving and checking results
      a3c0fe7a: ndt_1c Msg: Instance 0 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 1 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 2 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 3 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 4 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 5 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 6 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 7 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Setting receiving filters
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_NONE for instance 0
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+ for instance 1
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_BROADCAST+ for instance 2
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+ for instance 3
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_PROMISCUOUS+ for instance 4
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_PROMISCUOUS+ for instance 5
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      a3c0fe7a: ndt_1c Msg: Start receiving
      a3c0fe7a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Bad Multicast Addr
      a3c0fe7a: ndt_1c Msg: Stop receiving and checking results
      a3c0fe7a: ndt_1c Msg: Instance 0 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 1 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 2 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 3 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 4 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 5 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 6 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 7 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Setting receiving filters
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+ for instance 0
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+ for instance 1
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+ for instance 2
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+ for instance 3
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      a3c0fe7a: ndt_1c Msg: Start receiving
      a3c0fe7a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Bad Multicast Addr
      a3c0fe7a: ndt_1c Msg: Stop receiving and checking results
      a3c0fe7a: ndt_1c Msg: Instance 0 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 1 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 2 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 3 properly didn't receive packets
      a3c0fe7a: ndt_1c Msg: Instance 4 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 5 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 6 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 7 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Setting receiving filters
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+ for instance 0
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+ for instance 1
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      a3c0fe7a: ndt_1c Msg: Start receiving
      a3c0fe7a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Bad Multicast Addr
      a3c0fe7a: ndt_1c Msg: Stop receiving and checking results
      a3c0fe7a: ndt_1c Msg: Instance 0 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 1 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 2 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 3 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 4 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 5 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 6 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 7 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Setting receiving filters
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 0
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 1
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      a3c0fe7a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      a3c0fe7a: ndt_1c Msg: Start receiving
      a3c0fe7a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Bad Multicast Addr
      a3c0fe7a: ndt_1c Msg: Stop receiving and checking results
      a3c0fe7a: ndt_1c Msg: Instance 0 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 1 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 2 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 3 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 4 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 5 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 6 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Instance 7 received expected 300 packets
      a3c0fe7a: ndt_1c Msg: Unbinding adapters
   END TEST: "1c_LoopbackSend", PASSED, Time=291.039
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
*** TEST COMPLETED
***
*** Test Name:      1c_LoopbackSend
*** Test ID:        3
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX88772B1
*** Result:         Passed
*** Random Seed:    8154
*** Thread Count:   1
*** Execution Time: 0:04:51.039
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

</TESTCASE RESULT="PASSED">
<TESTCASE ID=4>
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
*** TEST STARTING
***
*** Test Name:      1c_LoopbackStress
*** Test ID:        4
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX88772B1
*** Random Seed:    26666
*** Thread Count:   0
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_LoopbackStress", Threads=0, Seed=26666
      a3c0fe7a: ndt_1c Msg: Start 1c_LoopbackStess test on the adapter AX88772B1
      a3c0fe7a: ndt_1c Msg: Getting informations about the adapter
      a3c0fe7a: ndt_1c Msg: Opening adapters
      a3c0fe7a: ndt_1c Msg: Start Stress Tests
      a3c0fe7a: ndt_1c Msg: Test #0
      a3c0fe7a: ndt_1c Msg: Binding adapters
      a3c0fe7a: ndt_1c Msg: Start receiving
      a3c0fe7a: ndt_1c Msg: Start sending
      a3c0fe7a: ndt_1c Msg: Wait to finish with sending
      a3c0fe7a: ndt_1c Msg: Stop listening
      a3c0fe7a: ndt_1c Msg: Bind #0: Sent 10000 packets with total size 7803112 bytes in 12491 ms
      a3c0fe7a: ndt_1c Msg: Bind #0: Recv 10000 packets with total size 460000 bytes in 12491 ms
      a3c0fe7a: ndt_1c Msg: Bind #1: Recv 10000 packets with total size 7803112 bytes in 12491 ms
      a3c0fe7a: ndt_1c Msg: Bind #1: Sent 10000 packets with total size 460000 bytes in 12491 ms
      a3c0fe7a: ndt_1c Msg: Unbinding adapters
      a3c0fe7a: ndt_1c Msg: Test #1
      a3c0fe7a: ndt_1c Msg: Binding adapters
      a3c0fe7a: ndt_1c Msg: Start receiving
      a3c0fe7a: ndt_1c Msg: Start sending
      a3c0fe7a: ndt_1c Msg: Wait to finish with sending
      a3c0fe7a: ndt_1c Msg: Stop listening
      a3c0fe7a: ndt_1c Msg: Bind #0: Sent 10000 packets with total size 7798578 bytes in 12490 ms
      a3c0fe7a: ndt_1c Msg: Bind #0: Recv 10000 packets with total size 460000 bytes in 12490 ms
      a3c0fe7a: ndt_1c Msg: Bind #1: Recv 10000 packets with total size 7798578 bytes in 12490 ms
      a3c0fe7a: ndt_1c Msg: Bind #1: Sent 10000 packets with total size 460000 bytes in 12490 ms
      a3c0fe7a: ndt_1c Msg: Unbinding adapters
      a3c0fe7a: ndt_1c Msg: Test #2
      a3c0fe7a: ndt_1c Msg: Binding adapters
      a3c0fe7a: ndt_1c Msg: Start receiving
      a3c0fe7a: ndt_1c Msg: Start sending
      a3c0fe7a: ndt_1c Msg: Wait to finish with sending
      a3c0fe7a: ndt_1c Msg: Stop listening
      a3c0fe7a: ndt_1c Msg: Bind #0: Sent 10000 packets with total size 7784372 bytes in 12490 ms
      a3c0fe7a: ndt_1c Msg: Bind #0: Recv 10000 packets with total size 460000 bytes in 12490 ms
      a3c0fe7a: ndt_1c Msg: Bind #1: Recv 10000 packets with total size 7784372 bytes in 12490 ms
      a3c0fe7a: ndt_1c Msg: Bind #1: Sent 10000 packets with total size 460000 bytes in 12490 ms
      a3c0fe7a: ndt_1c Msg: Unbinding adapters
      a3c0fe7a: ndt_1c Msg: Test #3
      a3c0fe7a: ndt_1c Msg: Binding adapters
      a3c0fe7a: ndt_1c Msg: Start receiving
      a3c0fe7a: ndt_1c Msg: Start sending
      a3c0fe7a: ndt_1c Msg: Wait to finish with sending
      a3c0fe7a: ndt_1c Msg: Stop listening
      a3c0fe7a: ndt_1c Msg: Bind #0: Sent 100 packets with total size 9650 bytes in 120 ms
      a3c0fe7a: ndt_1c Msg: Bind #0: Recv 100 packets with total size 4600 bytes in 120 ms
      a3c0fe7a: ndt_1c Msg: Bind #1: Recv 100 packets with total size 9650 bytes in 120 ms
      a3c0fe7a: ndt_1c Msg: Bind #1: Sent 100 packets with total size 4600 bytes in 120 ms
      a3c0fe7a: ndt_1c Msg: Unbinding adapters
      a3c0fe7a: ndt_1c Msg: Test #4
      a3c0fe7a: ndt_1c Msg: Binding adapters
      a3c0fe7a: ndt_1c Msg: Start receiving
      a3c0fe7a: ndt_1c Msg: Start sending
      a3c0fe7a: ndt_1c Msg: Wait to finish with sending
      a3c0fe7a: ndt_1c Msg: Stop listening
      a3c0fe7a: ndt_1c Msg: Bind #0: Sent 53 packets with total size 3869 bytes in 60 ms
      a3c0fe7a: ndt_1c Msg: Bind #0: Recv 53 packets with total size 3869 bytes in 60 ms
      a3c0fe7a: ndt_1c Msg: Bind #1: Recv 53 packets with total size 3869 bytes in 60 ms
      a3c0fe7a: ndt_1c Msg: Bind #1: Sent 53 packets with total size 3869 bytes in 60 ms
      a3c0fe7a: ndt_1c Msg: Unbinding adapters
      a3c0fe7a: ndt_1c Msg: Test #5
      a3c0fe7a: ndt_1c Msg: Binding adapters
      a3c0fe7a: ndt_1c Msg: Start receiving
      a3c0fe7a: ndt_1c Msg: Start sending
      a3c0fe7a: ndt_1c Msg: Wait to finish with sending
      a3c0fe7a: ndt_1c Msg: Stop listening
      a3c0fe7a: ndt_1c Msg: Bind #0: Sent 10000 packets with total size 1140000 bytes in 12491 ms
      a3c0fe7a: ndt_1c Msg: Bind #0: Recv 10000 packets with total size 460000 bytes in 12491 ms
      a3c0fe7a: ndt_1c Msg: Bind #1: Recv 10000 packets with total size 1140000 bytes in 12491 ms
      a3c0fe7a: ndt_1c Msg: Bind #1: Sent 10000 packets with total size 460000 bytes in 12491 ms
      a3c0fe7a: ndt_1c Msg: Unbinding adapters
      a3c0fe7a: ndt_1c Msg: Test #6
      a3c0fe7a: ndt_1c Msg: Binding adapters
      a3c0fe7a: ndt_1c Msg: Start receiving
      a3c0fe7a: ndt_1c Msg: Start sending
      a3c0fe7a: ndt_1c Msg: Wait to finish with sending
      a3c0fe7a: ndt_1c Msg: Stop listening
      a3c0fe7a: ndt_1c Msg: Bind #0: Sent 10000 packets with total size 7728560 bytes in 12491 ms
      a3c0fe7a: ndt_1c Msg: Bind #0: Recv 10000 packets with total size 460000 bytes in 12491 ms
      a3c0fe7a: ndt_1c Msg: Bind #1: Recv 10000 packets with total size 7728560 bytes in 12491 ms
      a3c0fe7a: ndt_1c Msg: Bind #1: Sent 10000 packets with total size 460000 bytes in 12491 ms
      a3c0fe7a: ndt_1c Msg: Unbinding adapters
      a3c0fe7a: ndt_1c Msg: Test #7
      a3c0fe7a: ndt_1c Msg: Binding adapters
      a3c0fe7a: ndt_1c Msg: Start receiving
      a3c0fe7a: ndt_1c Msg: Start sending
      a3c0fe7a: ndt_1c Msg: Wait to finish with sending
      a3c0fe7a: ndt_1c Msg: Stop listening
      a3c0fe7a: ndt_1c Msg: Bind #0: Sent 10000 packets with total size 7760413 bytes in 12491 ms
      a3c0fe7a: ndt_1c Msg: Bind #0: Recv 10000 packets with total size 460000 bytes in 12491 ms
      a3c0fe7a: ndt_1c Msg: Bind #1: Recv 10000 packets with total size 7760413 bytes in 12491 ms
      a3c0fe7a: ndt_1c Msg: Bind #1: Sent 0 packets with total size 0 bytes in 12491 ms
      a3c0fe7a: ndt_1c Msg: Unbinding adapters
      a3c0fe7a: ndt_1c Msg: Test #8
      a3c0fe7a: ndt_1c Msg: Binding adapters
      a3c0fe7a: ndt_1c Msg: Start receiving
      a3c0fe7a: ndt_1c Msg: Start sending
      a3c0fe7a: ndt_1c Msg: Wait to finish with sending
      a3c0fe7a: ndt_1c Msg: Stop listening
      a3c0fe7a: ndt_1c Msg: Bind #0: Sent 10000 packets with total size 7850608 bytes in 12490 ms
      a3c0fe7a: ndt_1c Msg: Bind #0: Recv 10000 packets with total size 7850608 bytes in 12490 ms
      a3c0fe7a: ndt_1c Msg: Bind #1: Recv 10000 packets with total size 7850608 bytes in 12490 ms
      a3c0fe7a: ndt_1c Msg: Bind #1: Sent 10000 packets with total size 7850608 bytes in 12490 ms
      a3c0fe7a: ndt_1c Msg: Unbinding adapters
      a3c0fe7a: ndt_1c Msg: Test #9
      a3c0fe7a: ndt_1c Msg: Binding adapters
      a3c0fe7a: ndt_1c Msg: Start receiving
      a3c0fe7a: ndt_1c Msg: Start sending
      a3c0fe7a: ndt_1c Msg: Wait to finish with sending
      a3c0fe7a: ndt_1c Msg: Stop listening
      a3c0fe7a: ndt_1c Msg: Bind #0: Sent 10000 packets with total size 740000 bytes in 12490 ms
      a3c0fe7a: ndt_1c Msg: Bind #0: Recv 10000 packets with total size 740000 bytes in 12490 ms
      a3c0fe7a: ndt_1c Msg: Bind #1: Recv 10000 packets with total size 740000 bytes in 12490 ms
      a3c0fe7a: ndt_1c Msg: Bind #1: Sent 10000 packets with total size 740000 bytes in 12490 ms
      a3c0fe7a: ndt_1c Msg: Unbinding adapters
      a3c0fe7a: ndt_1c Msg: Start simultaneous stress tests
      a3c0fe7a: ndt_1c Msg: Binding to adapters
      a3c0fe7a: ndt_1c Msg: Start receiving
      a3c0fe7a: ndt_1c Msg: Start sending
      a3c0fe7a: ndt_1c Msg: Wait to finish with sending
      a3c0fe7a: ndt_1c Msg: Stop listening
      a3c0fe7a: ndt_1c Msg: Bind #0: Sent 6 packets with total size 297 bytes in 12490 ms
      a3c0fe7a: ndt_1c Msg: Bind #0: Recv 6 packets with total size 297 bytes in 12490 ms
      a3c0fe7a: ndt_1c Msg: Bind #1: Sent 6 packets with total size 297 bytes in 12490 ms
      a3c0fe7a: ndt_1c Msg: Bind #1: Recv 6 packets with total size 297 bytes in 12490 ms
      a3c0fe7a: ndt_1c Msg: Bind #2: Sent 6 packets with total size 297 bytes in 0 ms
      a3c0fe7a: ndt_1c Msg: Bind #2: Recv 6 packets with total size 297 bytes in 0 ms
      a3c0fe7a: ndt_1c Msg: Bind #3: Sent 6 packets with total size 297 bytes in 0 ms
      a3c0fe7a: ndt_1c Msg: Bind #3: Recv 6 packets with total size 297 bytes in 0 ms
      a3c0fe7a: ndt_1c Msg: Bind #4: Recv 6 packets with total size 297 bytes in 0 ms
      a3c0fe7a: ndt_1c Msg: Bind #4: Sent 6 packets with total size 297 bytes in 0 ms
      a3c0fe7a: ndt_1c Msg: Bind #5: Recv 6 packets with total size 297 bytes in 0 ms
      a3c0fe7a: ndt_1c Msg: Bind #5: Sent 6 packets with total size 297 bytes in 0 ms
      a3c0fe7a: ndt_1c Msg: Bind #6: Recv 6 packets with total size 297 bytes in 0 ms
      a3c0fe7a: ndt_1c Msg: Bind #6: Sent 6 packets with total size 297 bytes in 0 ms
      a3c0fe7a: ndt_1c Msg: Bind #7: Recv 6 packets with total size 297 bytes in 0 ms
      a3c0fe7a: ndt_1c Msg: Bind #7: Sent 6 packets with total size 297 bytes in 0 ms
      a3c0fe7a: ndt_1c Msg: Unbinding adapters
      a3c0fe7a: ndt_1c Msg: Closing adapters
   END TEST: "1c_LoopbackStress", PASSED, Time=125.610
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
*** TEST COMPLETED
***
*** Test Name:      1c_LoopbackStress
*** Test ID:        4
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX88772B1
*** Result:         Passed
*** Random Seed:    26666
*** Thread Count:   1
*** Execution Time: 0:02:05.610
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

</TESTCASE RESULT="PASSED">
<TESTCASE ID=5>
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
*** TEST STARTING
***
*** Test Name:      1c_SetMulticast
*** Test ID:        5
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX88772B1
*** Random Seed:    21582
*** Thread Count:   0
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_SetMulticast", Threads=0, Seed=21582
      a3c0fe7a: ndt_1c Msg: Start 1c_SetMulticast test
      a3c0fe7a: ndt_1c Msg: The test adapter is AX88772B1
      a3c0fe7a: ndt_1c Msg: Opening adapters
      a3c0fe7a: ndt_1c Msg: Binding to adapters
      a3c0fe7a: ndt_1c Msg: GetMaxListSize
      a3c0fe7a: ndt_1c Msg: Driver support 64 address in multicast list
      a3c0fe7a: ndt_1c Msg: 64 multicast addresses will be tested
      a3c0fe7a: ndt_1c Msg: Add/Delete a multicast address multiple times
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add as many multicast addresses as driver says it supports
      a3c0fe7a: ndt_1c Msg: Adding multicast address 1
      a3c0fe7a: ndt_1c Msg: Adding multicast address 2
      a3c0fe7a: ndt_1c Msg: Adding multicast address 3
      a3c0fe7a: ndt_1c Msg: Adding multicast address 4
      a3c0fe7a: ndt_1c Msg: Adding multicast address 5
      a3c0fe7a: ndt_1c Msg: Adding multicast address 6
      a3c0fe7a: ndt_1c Msg: Adding multicast address 7
      a3c0fe7a: ndt_1c Msg: Adding multicast address 8
      a3c0fe7a: ndt_1c Msg: Adding multicast address 9
      a3c0fe7a: ndt_1c Msg: Adding multicast address 10
      a3c0fe7a: ndt_1c Msg: Adding multicast address 11
      a3c0fe7a: ndt_1c Msg: Adding multicast address 12
      a3c0fe7a: ndt_1c Msg: Adding multicast address 13
      a3c0fe7a: ndt_1c Msg: Adding multicast address 14
      a3c0fe7a: ndt_1c Msg: Adding multicast address 15
      a3c0fe7a: ndt_1c Msg: Adding multicast address 16
      a3c0fe7a: ndt_1c Msg: Adding multicast address 17
      a3c0fe7a: ndt_1c Msg: Adding multicast address 18
      a3c0fe7a: ndt_1c Msg: Adding multicast address 19
      a3c0fe7a: ndt_1c Msg: Adding multicast address 20
      a3c0fe7a: ndt_1c Msg: Adding multicast address 21
      a3c0fe7a: ndt_1c Msg: Adding multicast address 22
      a3c0fe7a: ndt_1c Msg: Adding multicast address 23
      a3c0fe7a: ndt_1c Msg: Adding multicast address 24
      a3c0fe7a: ndt_1c Msg: Adding multicast address 25
      a3c0fe7a: ndt_1c Msg: Adding multicast address 26
      a3c0fe7a: ndt_1c Msg: Adding multicast address 27
      a3c0fe7a: ndt_1c Msg: Adding multicast address 28
      a3c0fe7a: ndt_1c Msg: Adding multicast address 29
      a3c0fe7a: ndt_1c Msg: Adding multicast address 30
      a3c0fe7a: ndt_1c Msg: Adding multicast address 31
      a3c0fe7a: ndt_1c Msg: Adding multicast address 32
      a3c0fe7a: ndt_1c Msg: Adding multicast address 33
      a3c0fe7a: ndt_1c Msg: Adding multicast address 34
      a3c0fe7a: ndt_1c Msg: Adding multicast address 35
      a3c0fe7a: ndt_1c Msg: Adding multicast address 36
      a3c0fe7a: ndt_1c Msg: Adding multicast address 37
      a3c0fe7a: ndt_1c Msg: Adding multicast address 38
      a3c0fe7a: ndt_1c Msg: Adding multicast address 39
      a3c0fe7a: ndt_1c Msg: Adding multicast address 40
      a3c0fe7a: ndt_1c Msg: Adding multicast address 41
      a3c0fe7a: ndt_1c Msg: Adding multicast address 42
      a3c0fe7a: ndt_1c Msg: Adding multicast address 43
      a3c0fe7a: ndt_1c Msg: Adding multicast address 44
      a3c0fe7a: ndt_1c Msg: Adding multicast address 45
      a3c0fe7a: ndt_1c Msg: Adding multicast address 46
      a3c0fe7a: ndt_1c Msg: Adding multicast address 47
      a3c0fe7a: ndt_1c Msg: Adding multicast address 48
      a3c0fe7a: ndt_1c Msg: Adding multicast address 49
      a3c0fe7a: ndt_1c Msg: Adding multicast address 50
      a3c0fe7a: ndt_1c Msg: Adding multicast address 51
      a3c0fe7a: ndt_1c Msg: Adding multicast address 52
      a3c0fe7a: ndt_1c Msg: Adding multicast address 53
      a3c0fe7a: ndt_1c Msg: Adding multicast address 54
      a3c0fe7a: ndt_1c Msg: Adding multicast address 55
      a3c0fe7a: ndt_1c Msg: Adding multicast address 56
      a3c0fe7a: ndt_1c Msg: Adding multicast address 57
      a3c0fe7a: ndt_1c Msg: Adding multicast address 58
      a3c0fe7a: ndt_1c Msg: Adding multicast address 59
      a3c0fe7a: ndt_1c Msg: Adding multicast address 60
      a3c0fe7a: ndt_1c Msg: Adding multicast address 61
      a3c0fe7a: ndt_1c Msg: Adding multicast address 62
      a3c0fe7a: ndt_1c Msg: Adding multicast address 63
      a3c0fe7a: ndt_1c Msg: Adding multicast address 64
      a3c0fe7a: ndt_1c Msg: Delete all these added multicast addresses
      a3c0fe7a: ndt_1c Msg: Add/Delete a multicast address multiple times on two instances
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add/Query Multicast
      a3c0fe7a: ndt_1c Msg: Delete/Query Multicast
      a3c0fe7a: ndt_1c Msg: Add half of the maximum list size multicast address to each open instance
      a3c0fe7a: ndt_1c Msg: Delete all these added multicast addresses
      a3c0fe7a: ndt_1c Msg: Unbinding adapters
      a3c0fe7a: ndt_1c Msg: Closing adapters
   END TEST: "1c_SetMulticast", PASSED, Time=3.432
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
*** TEST COMPLETED
***
*** Test Name:      1c_SetMulticast
*** Test ID:        5
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX88772B1
*** Result:         Passed
*** Random Seed:    21582
*** Thread Count:   1
*** Execution Time: 0:00:03.432
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

</TESTCASE RESULT="PASSED">
<TESTCASE ID=6>
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
*** TEST STARTING
***
*** Test Name:      1c_Reset
*** Test ID:        6
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX88772B1
*** Random Seed:    4980
*** Thread Count:   0
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_Reset", Threads=0, Seed=4980
      a3c0fe7a: ndt_1c Msg: Start 1c_Reset test on the adapter AX88772B1
      a3c0fe7a: ndt_1c Msg: Opening adapters
      a3c0fe7a: ndt_1c Msg: Getting basic info about the adapter
      a3c0fe7a: ndt_1c Msg: Querying if miniport is wireless
      a3c0fe7a: ndt_1c Msg: Binding adapters
      a3c0fe7a: ndt_1c Msg: Sending packets
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Reset
      a3c0fe7a: ndt_1c Msg: Querying connect status
      a3c0fe7a: ndt_1c Msg: Unbinding adapters
      a3c0fe7a: ndt_1c Msg: Closing adapters
   END TEST: "1c_Reset", PASSED, Time=60.227
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
*** TEST COMPLETED
***
*** Test Name:      1c_Reset
*** Test ID:        6
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX88772B1
*** Result:         Passed
*** Random Seed:    4980
*** Thread Count:   1
*** Execution Time: 0:01:00.227
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

</TESTCASE RESULT="PASSED">
<TESTCASE ID=7>
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
*** TEST STARTING
***
*** Test Name:      1c_CancelSend
*** Test ID:        7
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX88772B1
*** Random Seed:    16301
*** Thread Count:   0
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_CancelSend", Threads=0, Seed=16301
      a3c0fe7a: ndt_1c Msg: Start 1c_CancelSend test on the adapter AX88772B1
      a3c0fe7a: ndt_1c Msg: Opening adapters
      a3c0fe7a: ndt_1c Msg: Getting basic info about the adapter
      a3c0fe7a: ndt_1c Msg: Binding adapters
      a3c0fe7a: ndt_1c Msg: Sending and cancel packets
      a3c0fe7a: ndt_1c Msg: Unbind adapters
      a3c0fe7a: ndt_1c Msg: 1000 packets was sent. 900 packet wasn't canceled. 0 packet was.
      a3c0fe7a: ndt_1c Msg: Closing adapters
   END TEST: "1c_CancelSend", PASSED, Time=6.485
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
*** TEST COMPLETED
***
*** Test Name:      1c_CancelSend
*** Test ID:        7
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX88772B1
*** Result:         Passed
*** Random Seed:    16301
*** Thread Count:   1
*** Execution Time: 0:00:06.485
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

</TESTCASE RESULT="PASSED">
<TESTCASE ID=8>
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
*** TEST STARTING
***
*** Test Name:      1c_FaultHandling
*** Test ID:        8
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX88772B1
*** Random Seed:    20502
*** Thread Count:   0
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_FaultHandling", Threads=0, Seed=20502
   END TEST: "1c_FaultHandling", SKIPPED, Time=0.000
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
*** TEST COMPLETED
***
*** Test Name:      1c_FaultHandling
*** Test ID:        8
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX88772B1
*** Result:         Skipped
*** Random Seed:    20502
*** Thread Count:   1
*** Execution Time: 0:00:00.000
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

</TESTCASE RESULT="SKIPPED">
<TESTCASE ID=9>
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
*** TEST STARTING
***
*** Test Name:      1c_OIDs
*** Test ID:        9
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX88772B1
*** Random Seed:    1453
*** Thread Count:   0
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_OIDs", Threads=0, Seed=1453
      a3c0fe7a: ndt_1c Msg: Start 1c_TestOidsDeviceIoControl test on the adapter AX88772B1
      a3c0fe7a: ndt_1c Msg: Open adapter
      a3c0fe7a: ndt_1c Msg: Bind to adapter
      a3c0fe7a: ndt_1c Msg: Get Supported OIDs List
      a3c0fe7a: ndt_1c Msg: Check for all required OIDs
      a3c0fe7a: ndt_1c Msg: Check that listed OIDs really are supported
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0x00010101 should be queried
      a3c0fe7a: ndt_1c Msg: The OID 0x00010101 was skippen
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0x00010102 should be queried
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0x00010103 should be queried
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0x00010104 should be queried
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0x00010114 should be queried
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0x00010105 should be queried
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0x00010106 should be queried
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0x00010111 should be queried
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0x00010115 should be queried
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0x00010113 should be queried
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0x00010112 should be queried
      a3c0fe7a: ndt_1c Msg: The OID 0x00010112 was skippen
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0x00010107 should be queried
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0x00010108 should be queried
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0x0001010a should be queried
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0x0002020e should be queried
      a3c0fe7a: ndt_1c Msg: The OID 0x0002020e isn't required, and hence not checked
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0x00010109 should be queried
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0x0001010b should be queried
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0x0001010c should be queried
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0x0001010d should be queried
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0x00010116 should be queried
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0x0001010e should be queried
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0x0001010f should be queried
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0x00010110 should be queried
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0x00020101 should be queried
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0x00020103 should be queried
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0x00020102 should be queried
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0x00020104 should be queried
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0x00020105 should be queried
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0x01010101 should be queried
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0x01010102 should be queried
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0x01010103 should be queried
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0x01010104 should be queried
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0x01020101 should be queried
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0x01020102 should be queried
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0x01020103 should be queried
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0x00010117 should be queried
      a3c0fe7a: ndt_1c Msg: The OID 0x00010117 isn't required, and hence not checked
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0xfd010100 should be queried
      a3c0fe7a: ndt_1c Msg: The OID 0xfd010100 isn't required, and hence not checked
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0xfd010106 should be queried
      a3c0fe7a: ndt_1c Msg: The OID 0xfd010106 was skippen
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0xfd010102 should be queried
      a3c0fe7a: ndt_1c Msg: The OID 0xfd010102 was skippen
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0xfd010101 should be queried
      a3c0fe7a: ndt_1c Msg: The OID 0xfd010101 was skippen
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0xfd010103 should be queried
      a3c0fe7a: ndt_1c Msg: The OID 0xfd010103 was skippen
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0xfd010104 should be queried
      a3c0fe7a: ndt_1c Msg: The OID 0xfd010104 was skippen
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0xff000000 should be queried
      a3c0fe7a: ndt_1c Msg: The OID 0xff000000 isn't required, and hence not checked
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0xff000001 should be queried
      a3c0fe7a: ndt_1c Msg: The OID 0xff000001 isn't required, and hence not checked
      a3c0fe7a: ndt_1c Msg: Checking if an OID 0xfc010201 should be queried
      a3c0fe7a: ndt_1c Msg: The OID 0xfc010201 isn't required, and hence not checked
      a3c0fe7a: ndt_1c Msg: Close adapter
   END TEST: "1c_OIDs", PASSED, Time=1.267
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
*** TEST COMPLETED
***
*** Test Name:      1c_OIDs
*** Test ID:        9
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX88772B1
*** Result:         Passed
*** Random Seed:    1453
*** Thread Count:   1
*** Execution Time: 0:00:01.267
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

</TESTCASE RESULT="PASSED">
<TESTCASE ID=10>
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
*** TEST STARTING
***
*** Test Name:      1c_64BitOIDs
*** Test ID:        10
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX88772B1
*** Random Seed:    4783
*** Thread Count:   0
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_64BitOIDs", Threads=0, Seed=4783
      a3c0fe7a: ndt_1c Msg: Start 1c_64BitOID test on the adapter AX88772B1
      a3c0fe7a: ndt_1c Msg: Open adapter
      a3c0fe7a: ndt_1c Msg: Bind to adapter
      a3c0fe7a: ndt_1c Msg: Link speed is lower than 1.0Gbps
      a3c0fe7a: ndt_1c Msg: 64-bit statistics are optional
      a3c0fe7a: ndt_1c Msg: Querying 64bit OIDs
      a3c0fe7a: ndt_1c Msg: Query with a null buffer
      a3c0fe7a: ndt_1c Wrn: The miniport should have set BytesNeeded to 8 not to 4
      a3c0fe7a: ndt_1c Msg: Query with a four byte buffer
      a3c0fe7a: ndt_1c Wrn: The miniport should have set BytesNeeded to 8 not to 4
      a3c0fe7a: ndt_1c Msg: Query with an eight byte buffer
      a3c0fe7a: ndt_1c Wrn: The miniport should have set BytesWritten to 8 not to 4
      a3c0fe7a: ndt_1c Wrn: The miniport should have set BytesNeeded to 8 not to 4
      a3c0fe7a: ndt_1c Msg: Query with a null buffer
      a3c0fe7a: ndt_1c Wrn: The miniport should have set BytesNeeded to 8 not to 4
      a3c0fe7a: ndt_1c Msg: Query with a four byte buffer
      a3c0fe7a: ndt_1c Wrn: The miniport should have set BytesNeeded to 8 not to 4
      a3c0fe7a: ndt_1c Msg: Query with an eight byte buffer
      a3c0fe7a: ndt_1c Wrn: The miniport should have set BytesWritten to 8 not to 4
      a3c0fe7a: ndt_1c Wrn: The miniport should have set BytesNeeded to 8 not to 4
      a3c0fe7a: ndt_1c Msg: Unbind adapter
      a3c0fe7a: ndt_1c Msg: Close adapter
   END TEST: "1c_64BitOIDs", PASSED, Time=0.383
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
*** TEST COMPLETED
***
*** Test Name:      1c_64BitOIDs
*** Test ID:        10
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX88772B1
*** Result:         Passed
*** Random Seed:    4783
*** Thread Count:   1
*** Execution Time: 0:00:00.383
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

</TESTCASE RESULT="PASSED">
<TESTCASE ID=11>
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
*** TEST STARTING
***
*** Test Name:      1c_SuspendResume
*** Test ID:        11
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX88772B1
*** Random Seed:    15657
*** Thread Count:   0
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_SuspendResume", Threads=0, Seed=15657
      a3c0fe7a: ndt_1c Msg: Start 1c_SusRes (Suspend/Resume) test on the adapter AX88772B1
      a3c0fe7a: ndt_1c Msg: Enabling the Wake up source : SYSINTR_RTC_ALARM
      a3c0fe7a: ndt_1c Msg: Suspending the system 1 time
      a3c0fe7a: ndt_1c Msg: Resumed .....
      a3c0fe7a: ndt_1c Msg: Sleeping 5 sec .....
      a3c0fe7a: ndt_1c Msg: Suspending the system 2 time
      a3c0fe7a: ndt_1c Msg: Resumed .....
      a3c0fe7a: ndt_1c Msg: Sleeping 10 sec .....
      a3c0fe7a: ndt_1c Msg: Suspending the system 3 time
      a3c0fe7a: ndt_1c Msg: Resumed .....
      a3c0fe7a: ndt_1c Msg: Sleeping 15 sec .....
      a3c0fe7a: ndt_1c Msg: Suspending the system 4 time
      a3c0fe7a: ndt_1c Msg: Resumed .....
      a3c0fe7a: ndt_1c Msg: Sleeping 20 sec .....
      a3c0fe7a: ndt_1c Msg: Suspending the system 5 time
      a3c0fe7a: ndt_1c Msg: Resumed .....
      a3c0fe7a: ndt_1c Msg: Sleeping 25 sec .....
      a3c0fe7a: ndt_1c Msg: Testing if the adapter AX88772B1 is fine after suspend/resume
      a3c0fe7a: ndt_1c Msg: Getting basic info about the adapter
      a3c0fe7a: ndt_1c Msg: Get OID_GEN_MAXIMUM_TOTAL_SIZE = 1514
      a3c0fe7a: ndt_1c Msg: Get OID_GEN_MAXIMUM_FRAME_SIZE = 1500
      a3c0fe7a: ndt_1c Msg: Testing sending to a (random) directed address
      a3c0fe7a: ndt_1c Msg: Sending 100 packets each of 64 size to a random address
      a3c0fe7a: ndt_1c Msg: 100 packets were SendCompleted
      a3c0fe7a: ndt_1c Msg: Sending 100 packets each of 783 size to a random address
      a3c0fe7a: ndt_1c Msg: 100 packets were SendCompleted
      a3c0fe7a: ndt_1c Msg: Sending 100 packets each of 1500 size to a random address
      a3c0fe7a: ndt_1c Msg: 100 packets were SendCompleted
      a3c0fe7a: ndt_1c Msg: Disabling the Wake up source
   END TEST: "1c_SuspendResume", PASSED, Time=101.942
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
*** TEST COMPLETED
***
*** Test Name:      1c_SuspendResume
*** Test ID:        11
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX88772B1
*** Result:         Passed
*** Random Seed:    15657
*** Thread Count:   1
*** Execution Time: 0:01:41.942
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

</TESTCASE RESULT="PASSED">
<TESTCASE ID=12>
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
*** TEST STARTING
***
*** Test Name:      1c_StressSusRes
*** Test ID:        12
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX88772B1
*** Random Seed:    18399
*** Thread Count:   0
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_StressSusRes", Threads=0, Seed=18399
      a3c0fe7a: ndt_1c Msg: Start 1c_StressSusRes (Stress in Suspend/Resume) test on the adapter AX88772B1
      a3c0fe7a: ndt_1c Msg: Opening adapter
      a3c0fe7a: ndt_1c Msg: Binding to it
      a3c0fe7a: ndt_1c Msg: Checking if miniport is PM aware.
      a3c0fe7a: ndt_1c Msg: AX88772B1 supports only Power Management, but does not have wake-up capabilities
      e3d5a962: ndt_1c Msg: StressOIDs: AX88772B1 supports ** 45 ** OIDs
      e3beb002: ndt_1c Msg: StressSendRecv: stress started
      e3d5a962: ndt_1c Msg: StressOIDs: stress started
      e3beb002: ndt_1c Msg: StressSendRecv: Sending 1000 packets each of 64 size to a random address
      a3c0fe7a: ndt_1c Msg: Transitioning the adapter to D4 state 1 time
      a3c0fe7a: ndt_1c Msg: Transitioning back to D0 state 1 time
      a3c0fe7a: ndt_1c Msg: Waiting 1000 mili sec
      a3c0fe7a: ndt_1c Msg: Transitioning the adapter to D4 state 2 time
      a3c0fe7a: ndt_1c Msg: Transitioning back to D0 state 2 time
      a3c0fe7a: ndt_1c Msg: Waiting 1000 mili sec
      a3c0fe7a: ndt_1c Msg: Transitioning the adapter to D4 state 3 time
      a3c0fe7a: ndt_1c Msg: Transitioning back to D0 state 3 time
      a3c0fe7a: ndt_1c Msg: Waiting 1000 mili sec
      a3c0fe7a: ndt_1c Msg: Transitioning the adapter to D4 state 4 time
      a3c0fe7a: ndt_1c Msg: Transitioning back to D0 state 4 time
      a3c0fe7a: ndt_1c Msg: Waiting 1000 mili sec
      a3c0fe7a: ndt_1c Msg: Transitioning the adapter to D4 state 5 time
      a3c0fe7a: ndt_1c Msg: Transitioning back to D0 state 5 time
      a3c0fe7a: ndt_1c Msg: Waiting 1000 mili sec
      a3c0fe7a: ndt_1c Msg: Transitioning the adapter to D4 state 6 time
      a3c0fe7a: ndt_1c Msg: Transitioning back to D0 state 6 time
      a3c0fe7a: ndt_1c Msg: Waiting 2000 mili sec
      a3c0fe7a: ndt_1c Msg: Transitioning the adapter to D4 state 7 time
      a3c0fe7a: ndt_1c Msg: Transitioning back to D0 state 7 time
      a3c0fe7a: ndt_1c Msg: Waiting 2000 mili sec
      a3c0fe7a: ndt_1c Msg: Transitioning the adapter to D4 state 8 time
      a3c0fe7a: ndt_1c Msg: Transitioning back to D0 state 8 time
      a3c0fe7a: ndt_1c Msg: Waiting 2000 mili sec
      a3c0fe7a: ndt_1c Msg: Transitioning the adapter to D4 state 9 time
      a3c0fe7a: ndt_1c Msg: Transitioning back to D0 state 9 time
      a3c0fe7a: ndt_1c Msg: Waiting 2000 mili sec
      a3c0fe7a: ndt_1c Msg: Transitioning the adapter to D4 state 10 time
      a3c0fe7a: ndt_1c Msg: Transitioning back to D0 state 10 time
      a3c0fe7a: ndt_1c Msg: Waiting 2000 mili sec
      a3c0fe7a: ndt_1c Msg: Transitioning the adapter to D4 state 11 time
      a3c0fe7a: ndt_1c Msg: Transitioning back to D0 state 11 time
      a3c0fe7a: ndt_1c Msg: Waiting 4000 mili sec
      e3beb002: ndt_1c Msg: StressSendRecv: 21 packets each of 64 size were SendCompleted
      e3beb002: ndt_1c Msg: StressSendRecv: Sending 1000 packets each of 127 size to a random address
      a3c0fe7a: ndt_1c Msg: Transitioning the adapter to D4 state 12 time
      a3c0fe7a: ndt_1c Msg: Transitioning back to D0 state 12 time
      a3c0fe7a: ndt_1c Msg: Waiting 4000 mili sec
      a3c0fe7a: ndt_1c Msg: Transitioning the adapter to D4 state 13 time
      a3c0fe7a: ndt_1c Msg: Transitioning back to D0 state 13 time
      a3c0fe7a: ndt_1c Msg: Waiting 4000 mili sec
      a3c0fe7a: ndt_1c Msg: Transitioning the adapter to D4 state 14 time
      a3c0fe7a: ndt_1c Msg: Transitioning back to D0 state 14 time
      a3c0fe7a: ndt_1c Msg: Waiting 4000 mili sec
      a3c0fe7a: ndt_1c Msg: Transitioning the adapter to D4 state 15 time
      a3c0fe7a: ndt_1c Msg: Transitioning back to D0 state 15 time
      a3c0fe7a: ndt_1c Msg: Waiting 4000 mili sec
      a3c0fe7a: ndt_1c Msg: Transitioning the adapter to D4 state 16 time
      a3c0fe7a: ndt_1c Msg: Transitioning back to D0 state 16 time
      a3c0fe7a: ndt_1c Msg: Waiting 5000 mili sec
      a3c0fe7a: ndt_1c Msg: Transitioning the adapter to D4 state 17 time
      a3c0fe7a: ndt_1c Msg: Transitioning back to D0 state 17 time
      a3c0fe7a: ndt_1c Msg: Waiting 5000 mili sec
      a3c0fe7a: ndt_1c Msg: Transitioning the adapter to D4 state 18 time
      e3beb002: ndt_1c Msg: StressSendRecv: 382 packets each of 127 size were SendCompleted
      e3beb002: ndt_1c Msg: StressSendRecv: Sending 1000 packets each of 190 size to a random address
      a3c0fe7a: ndt_1c Msg: Transitioning back to D0 state 18 time
      a3c0fe7a: ndt_1c Msg: Waiting 5000 mili sec
      a3c0fe7a: ndt_1c Msg: Transitioning the adapter to D4 state 19 time
      a3c0fe7a: ndt_1c Msg: Transitioning back to D0 state 19 time
      a3c0fe7a: ndt_1c Msg: Waiting 5000 mili sec
      a3c0fe7a: ndt_1c Msg: Transitioning the adapter to D4 state 20 time
      a3c0fe7a: ndt_1c Msg: Transitioning back to D0 state 20 time
      a3c0fe7a: ndt_1c Msg: Waiting 5000 mili sec
      a3c0fe7a: ndt_1c Msg: Waiting for Stress OIDs thread to terminate
      e3d5a962: ndt_1c Msg: StressOIDs: signaled to stop
      e3d5a962: ndt_1c Msg: StressOIDs: Cleaned up & exiting.
      a3c0fe7a: ndt_1c Msg: Stress OIDs thread exited with exit value : PASS
      a3c0fe7a: ndt_1c Msg: Waiting for StressSendRecv thread to terminate
      e3beb002: ndt_1c Msg: StressSendRecv: 716 packets each of 190 size were SendCompleted
      e3beb002: ndt_1c Msg: StressSendRecv: signaled to stop
      e3beb002: ndt_1c Msg: StressSendRecv: Cleaned up & exiting.
      a3c0fe7a: ndt_1c Msg: Stress SendRecv thread exited with exit value : PASS
      a3c0fe7a: ndt_1c Msg: Unbinding to it
      a3c0fe7a: ndt_1c Msg: Closing adapter
   END TEST: "1c_StressSusRes", PASSED, Time=121.005
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
*** TEST COMPLETED
***
*** Test Name:      1c_StressSusRes
*** Test ID:        12
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX88772B1
*** Result:         Passed
*** Random Seed:    18399
*** Thread Count:   1
*** Execution Time: 0:02:01.005
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

</TESTCASE RESULT="PASSED">
<TESTCASE ID=13>
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
*** TEST STARTING
***
*** Test Name:      1c_ResetOnResume
*** Test ID:        13
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX88772B1
*** Random Seed:    27354
*** Thread Count:   0
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_ResetOnResume", Threads=0, Seed=27354
      a3c0fe7a: ndt_1c Msg: Start 1c_ResetOnResume (Reset on Resume) test on the adapter AX88772B1
      a3c0fe7a: ndt_1c Msg: This test will test if AX88772B1 restores its settings after Reset
      a3c0fe7a: ndt_1c Msg: AX88772B1 supports only Power Management, but does not have wake-up capabilities
      a3c0fe7a: ndt_1c Msg: Set CURRENT_PACKET_FILTER = NDIS_PACKET_TYPE_MULTICAST|NDIS_PACKET_TYPE_DIRECTED for adapter AX88772B1
      a3c0fe7a: ndt_1c Msg: AX88772B1 supports max 64 Multicast addresses
      a3c0fe7a: ndt_1c Msg: Got the current complete list of multicast addresses for AX88772B1
      a3c0fe7a: ndt_1c Msg: It has 0 multicast addresses set
      a3c0fe7a: ndt_1c Msg: Set 62 multicast addresses for AX88772B1
      a3c0fe7a: ndt_1c Msg: We'll RESET the device & at the end of every RESET we'll verify if AX88772B1 restores its settings or not
      a3c0fe7a: ndt_1c Msg: Reseting the network adapter AX88772B1 1 time
      a3c0fe7a: ndt_1c Msg: Waiting to receive NDIS_STATUS_RESET_END notification on the miniport adapter AX88772B1
      a3c0fe7a: ndt_1c Msg: Received NDIS_STATUS_RESET_END notification on AX88772B1
      a3c0fe7a: ndt_1c Msg: AX88772B1 has restored/retained its Packet Filter settings.
      a3c0fe7a: ndt_1c Msg: AX88772B1 has restored/retained its multicast addresses list.
      a3c0fe7a: ndt_1c Msg: AX88772B1 has passed ResetOnResume test
      a3c0fe7a: ndt_1c Msg: Reseting the network adapter AX88772B1 2 time
      a3c0fe7a: ndt_1c Msg: Waiting to receive NDIS_STATUS_RESET_END notification on the miniport adapter AX88772B1
      a3c0fe7a: ndt_1c Msg: Received NDIS_STATUS_RESET_END notification on AX88772B1
      a3c0fe7a: ndt_1c Msg: AX88772B1 has restored/retained its Packet Filter settings.
      a3c0fe7a: ndt_1c Msg: AX88772B1 has restored/retained its multicast addresses list.
      a3c0fe7a: ndt_1c Msg: AX88772B1 has passed ResetOnResume test
      a3c0fe7a: ndt_1c Msg: Reseting the network adapter AX88772B1 3 time
      a3c0fe7a: ndt_1c Msg: Waiting to receive NDIS_STATUS_RESET_END notification on the miniport adapter AX88772B1
      a3c0fe7a: ndt_1c Msg: Received NDIS_STATUS_RESET_END notification on AX88772B1
      a3c0fe7a: ndt_1c Msg: AX88772B1 has restored/retained its Packet Filter settings.
      a3c0fe7a: ndt_1c Msg: AX88772B1 has restored/retained its multicast addresses list.
      a3c0fe7a: ndt_1c Msg: AX88772B1 has passed ResetOnResume test
      a3c0fe7a: ndt_1c Msg: Reseting the network adapter AX88772B1 4 time
      a3c0fe7a: ndt_1c Msg: Waiting to receive NDIS_STATUS_RESET_END notification on the miniport adapter AX88772B1
      a3c0fe7a: ndt_1c Msg: Received NDIS_STATUS_RESET_END notification on AX88772B1
      a3c0fe7a: ndt_1c Msg: AX88772B1 has restored/retained its Packet Filter settings.
      a3c0fe7a: ndt_1c Msg: AX88772B1 has restored/retained its multicast addresses list.
      a3c0fe7a: ndt_1c Msg: AX88772B1 has passed ResetOnResume test
      a3c0fe7a: ndt_1c Msg: Reseting the network adapter AX88772B1 5 time
      a3c0fe7a: ndt_1c Msg: Waiting to receive NDIS_STATUS_RESET_END notification on the miniport adapter AX88772B1
      a3c0fe7a: ndt_1c Msg: Received NDIS_STATUS_RESET_END notification on AX88772B1
      a3c0fe7a: ndt_1c Msg: AX88772B1 has restored/retained its Packet Filter settings.
      a3c0fe7a: ndt_1c Msg: AX88772B1 has restored/retained its multicast addresses list.
      a3c0fe7a: ndt_1c Msg: AX88772B1 has passed ResetOnResume test
   END TEST: "1c_ResetOnResume", PASSED, Time=1.063
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
*** TEST COMPLETED
***
*** Test Name:      1c_ResetOnResume
*** Test ID:        13
*** Library Path:   \ndt_1c.dll
*** Command Line:   -t AX88772B1
*** Result:         Passed
*** Random Seed:    27354
*** Thread Count:   1
*** Execution Time: 0:00:01.063
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

</TESTCASE RESULT="PASSED">
END GROUP: ndt_1c.dll
*** ==================================================================
*** MEMORY INFO
***
*** Memory Total:    24,092,672 bytes
*** Memory Used:      8,454,144 bytes
*** Memory Free:     15,638,528 bytes
***
*** Kernel Used:        716,800 bytes
*** Water Mark:           3,762 pages
***
*** Store Total:     24,027,136 bytes
*** Store Used:         597,616 bytes
*** Store Free:      23,429,520 bytes
*** ==================================================================

*** ==================================================================
*** SUITE SUMMARY
***
*** Passed:         12
*** Failed:          0
*** Skipped:         1
*** Aborted:         0
*** -------- ---------
*** Total:          13
***
*** Cumulative Test Execution Time: 0:12:50.814
*** Total Tux Suite Execution Time: 0:12:54.003
*** CPU Idle Time:                  0:11:17.595
*** ==================================================================
</TESTGROUP>
@@@@@@0

