; @CESYSGEN IF BSP_NIC_AX88772B
;IF BSP_NIC_AX88772B
[HKEY_LOCAL_MACHINE\Drivers\USB\LoadClients\2965_30507\Default\Default\AX88772B]
   	"DLL"="AX88772B.DLL"
   	"Prefix"="ASX"

[HKEY_LOCAL_MACHINE\Drivers\USB\ClientDrivers\AX88772B]
   	"DLL"="AX88772B.DLL"
   	"Prefix"="ASX"

[HKEY_LOCAL_MACHINE\Comm\AX88772B]
   	"DisplayName"="ASIX AX88772B USB 2.0 Fast Ethernet Driver"
   	"Group"="NDIS"
   	"ImagePath"="AX88772B.dll"
  
[HKEY_LOCAL_MACHINE\Comm\AX88772B\Linkage]
   	"Route"=multi_sz:"AX88772B1","AX88772B2","AX88772B3","AX88772B4"

[HKEY_LOCAL_MACHINE\Comm\AX88772B1]
   	"DisplayName"="ASIX AX88772B USB 2.0 Fast Ethernet Driver"
   	"Group"="NDIS"
   	"ImagePath"="AX88772B.dll"
	
[HKEY_LOCAL_MACHINE\Comm\AX88772B1\Parms]
      	"BusNumber"=dword:0
   	"BusType"=dword:1   	
;      	"NetworkAddress"="02-12-34-56-78-9a" 	;Define an override MAC address 02-12-34-56-78-9a

;===========================================================================
; AX88772B Driver Parameters:
;===========================================================================
   	"ConnectionType"=dword:0                ; 0 = "AutoSense"; 2 = "10BaseT Half_Duplex"; 3 = "10BaseT Full_Duplex";
 		                                ; 8 = "100BaseTx Half_Duplex"; 9 = "100BaseTx Full_Duplex"
   	"FlowControl"=dword:3                   ; 0 = "Disable"; 1 = "TX PAUSE"; 2 = "RX PAUSE"; 3 = "Enable"
	"WakeUp"=dword:0                        ; 0 = "Disable"; 2 = "Link-Change"; 4 = "Magic Packet"; 8 = "Wakeup Frame";
                                                ; 6 = "Link-Change" & "Magic Packet"; a = "Link-Change" & "Wakeup Frame";
                                                ; c = "Magic Packet" & "Wakeup Frame"; e = "All"
	"WakeUpFrameType"=dword:3		; 1 = "Ping"; 2 = "ARP"; 3 = "All"
	"VlanEnable"=dword:0			; 0 = "Disable"; 1 = "Enable";
	"VlanId"=dword:0			; 0 - 4095
	"AutoDetach"=dword:2			; 0 = "Disable"; 1 = "Enable"; 2 = "Use EEPROM Setting"
	"WolLinkSpeed"=dword:1			; 0 = "10 Mpbs First"; 1 = "Use EEPROM Setting"
	"Checksum"=dword:1			; 0 = "Disable"; 1 = "Enable"

[HKEY_LOCAL_MACHINE\Comm\AX88772B1\Parms\TcpIp]
;	"EnableDHCP"=dword:0			;Disable DHCP function
;	"IpAddress"="xxx.xxx.xxx.aaa"		;Define your IP address (xxx.xxx.xxx.aaa)
;	"Subnetmask"="255.255.255.0"		;Define Submask IP address
;	"DefaultGateway"="xxx.xxx.xxx.bbb"	;Define Gateway IP address
;	"DNS"="xxx.xxx.xxx.ccc"			;Define DNS server IP address

   	"AutoCfg"=dword:1
   	"EnableDHCP"=dword:1			;Enable DHCP function
	"UseZeroBroadcast"=dword:0		;Use zero for broadcast address?

[HKEY_LOCAL_MACHINE\Comm\AX88772B2]
   	"DisplayName"="ASIX AX88772B USB 2.0 Fast Ethernet Driver"
   	"Group"="NDIS"
   	"ImagePath"="AX88772B.dll"
	
[HKEY_LOCAL_MACHINE\Comm\AX88772B2\Parms]
      	"BusNumber"=dword:0
   	"BusType"=dword:1   	
;      	"NetworkAddress"="02-12-34-56-78-9a" 	;Define an override MAC address 02-12-34-56-78-9a

;===========================================================================
; AX88772B Driver Parameters:
;===========================================================================
   	"ConnectionType"=dword:0                ; 0 = "AutoSense"; 2 = "10BaseT Half_Duplex"; 3 = "10BaseT Full_Duplex";
 		                                ; 8 = "100BaseTx Half_Duplex"; 9 = "100BaseTx Full_Duplex"
   	"FlowControl"=dword:3                   ; 0 = "Disable"; 1 = "TX PAUSE"; 2 = "RX PAUSE"; 3 = "Enable"
	"WakeUp"=dword:0                        ; 0 = "Disable"; 2 = "Link-Change"; 4 = "Magic Packet"; 8 = "Wakeup Frame";
                                                ; 6 = "Link-Change" & "Magic Packet"; a = "Link-Change" & "Wakeup Frame";
                                                ; c = "Magic Packet" & "Wakeup Frame"; e = "All"
	"WakeUpFrameType"=dword:3		; 1 = "Ping"; 2 = "ARP"; 3 = "All"
	"VlanEnable"=dword:0			; 0 = "Disable"; 1 = "Enable"
	"VlanId"=dword:0			; 0 - 4095
	"AutoDetach"=dword:2			; 0 = "Disable"; 1 = "Enable"; 2 = "Use EEPROM Setting"
	"WolLinkSpeed"=dword:1			; 0 = "10 Mpbs First"; 1 = "Use EEPROM Setting"
	"Checksum"=dword:1			; 0 = "Disable"; 1 = "Enable"

[HKEY_LOCAL_MACHINE\Comm\AX88772B2\Parms\TcpIp]
;	"EnableDHCP"=dword:0			;Disable DHCP function
;	"IpAddress"="xxx.xxx.xxx.aaa"		;Define your IP address (xxx.xxx.xxx.aaa)
;	"Subnetmask"="255.255.255.0"		;Define Submask IP address
;	"DefaultGateway"="xxx.xxx.xxx.bbb"	;Define Gateway IP address
;	"DNS"="xxx.xxx.xxx.ccc"			;Define DNS server IP address

   	"AutoCfg"=dword:1
   	"EnableDHCP"=dword:1			;Enable DHCP function
	"UseZeroBroadcast"=dword:0		;Use zero for broadcast address?

[HKEY_LOCAL_MACHINE\Comm\AX88772B3]
   	"DisplayName"="ASIX AX88772B USB 2.0 Fast Ethernet Driver"
   	"Group"="NDIS"
   	"ImagePath"="AX88772B.dll"
	
[HKEY_LOCAL_MACHINE\Comm\AX88772B3\Parms]
      	"BusNumber"=dword:0
   	"BusType"=dword:1   	
;      	"NetworkAddress"="02-12-34-56-78-9a" 	;Define an override MAC address 02-12-34-56-78-9a

;===========================================================================
; AX88772B Driver Parameters:
;===========================================================================
   	"ConnectionType"=dword:0                ; 0 = "AutoSense"; 2 = "10BaseT Half_Duplex"; 3 = "10BaseT Full_Duplex";
 		                                ; 8 = "100BaseTx Half_Duplex"; 9 = "100BaseTx Full_Duplex"
   	"FlowControl"=dword:3                   ; 0 = "Disable"; 1 = "TX PAUSE"; 2 = "RX PAUSE"; 3 = "Enable"
	"WakeUp"=dword:0                        ; 0 = "Disable"; 2 = "Link-Change"; 4 = "Magic Packet"; 8 = "Wakeup Frame";
                                                ; 6 = "Link-Change" & "Magic Packet"; a = "Link-Change" & "Wakeup Frame";
                                                ; c = "Magic Packet" & "Wakeup Frame"; e = "All"
	"WakeUpFrameType"=dword:3		; 1 = "Ping"; 2 = "ARP"; 3 = "All"
	"VlanEnable"=dword:0			; 0 = "Disable"; 1 = "Enable"
	"VlanId"=dword:0			; 0 - 4095
	"AutoDetach"=dword:1			; 0 = "Disable"; 1 = "Enable"; 2 = "Use EEPROM Setting"
	"WolLinkSpeed"=dword:1			; 0 = "10 Mpbs First"; 1 = "Use EEPROM Setting"
	"Checksum"=dword:1			; 0 = "Disable"; 1 = "Enable"

[HKEY_LOCAL_MACHINE\Comm\AX88772B3\Parms\TcpIp]
;	"EnableDHCP"=dword:0			;Disable DHCP function
;	"IpAddress"="xxx.xxx.xxx.aaa"		;Define your IP address (xxx.xxx.xxx.aaa)
;	"Subnetmask"="255.255.255.0"		;Define Submask IP address
;	"DefaultGateway"="xxx.xxx.xxx.bbb"	;Define Gateway IP address
;	"DNS"="xxx.xxx.xxx.ccc"			;Define DNS server IP address

   	"AutoCfg"=dword:1
   	"EnableDHCP"=dword:1			;Enable DHCP function
	"UseZeroBroadcast"=dword:0		;Use zero for broadcast address?

[HKEY_LOCAL_MACHINE\Comm\AX88772B4]
   	"DisplayName"="ASIX AX88772B USB 2.0 Fast Ethernet Driver"
   	"Group"="NDIS"
   	"ImagePath"="AX88772B.dll"
	
[HKEY_LOCAL_MACHINE\Comm\AX88772B4\Parms]
      	"BusNumber"=dword:0
   	"BusType"=dword:1   	
;      	"NetworkAddress"="02-12-34-56-78-9a" 	;Define an override MAC address 02-12-34-56-78-9a

;===========================================================================
; AX88772B Driver Parameters:
;===========================================================================
   	"ConnectionType"=dword:0                ; 0 = "AutoSense"; 2 = "10BaseT Half_Duplex"; 3 = "10BaseT Full_Duplex";
 		                                ; 8 = "100BaseTx Half_Duplex"; 9 = "100BaseTx Full_Duplex"
   	"FlowControl"=dword:3                   ; 0 = "Disable"; 1 = "TX PAUSE"; 2 = "RX PAUSE"; 3 = "Enable"
	"WakeUp"=dword:0                        ; 0 = "Disable"; 2 = "Link-Change"; 4 = "Magic Packet"; 8 = "Wakeup Frame";
                                                ; 6 = "Link-Change" & "Magic Packet"; a = "Link-Change" & "Wakeup Frame";
                                                ; c = "Magic Packet" & "Wakeup Frame"; e = "All"
	"WakeUpFrameType"=dword:3		; 1 = "Ping"; 2 = "ARP"; 3 = "All"
	"VlanEnable"=dword:0			; 0 = "Disable"; 1 = "Enable"
	"VlanId"=dword:0			; 0 - 4095
	"AutoDetach"=dword:2			; 0 = "Disable"; 1 = "Enable"; 2 = "Use EEPROM Setting"
	"WolLinkSpeed"=dword:1			; 0 = "10 Mpbs First"; 1 = "Use EEPROM Setting"
	"Checksum"=dword:1			; 0 = "Disable"; 1 = "Enable"

[HKEY_LOCAL_MACHINE\Comm\AX88772B4\Parms\TcpIp]
;	"EnableDHCP"=dword:0			;Disable DHCP function
;	"IpAddress"="xxx.xxx.xxx.aaa"		;Define your IP address (xxx.xxx.xxx.aaa)
;	"Subnetmask"="255.255.255.0"		;Define Submask IP address
;	"DefaultGateway"="xxx.xxx.xxx.bbb"	;Define Gateway IP address
;	"DNS"="xxx.xxx.xxx.ccc"			;Define DNS server IP address

   	"AutoCfg"=dword:1
   	"EnableDHCP"=dword:1			;Enable DHCP function
	"UseZeroBroadcast"=dword:0		;Use zero for broadcast address?
		
;ENDIF BSP_NIC_AX88772B
; @CESYSGEN ENDIF BSP_NIC_AX88772B

