==========================================
WIndows CE 6.0 Test Kit (CETK 6.0) 
Two-Card Network Card Miniport Driver Test
==========================================

REM tux -o -d ndt_2c -c "-s support_adapter -t test_adapter ..."
REM 
REM Parameters:
REM 
REM -t adapter : Adapter to test (e.g. NE20001)
REM -s adapter : Support adapter (e.g. NE20001@KARELD01)
REM -nounbind  : Do not unbind protocols from the test adapter
REM -cancel    : Check result for 1c_CancelSend (default false)
REM -nostress  : Skip stress tests (default false)
REM 
REM Adapter name is in form 'adapter@IP' for remote adapter
REM and in form 'adapter' for local one. E.g. NE20001@196.23.3.3
REM 
REM Do not use the Vmini network interface with this test. 
REM The Vmini interface disables your KITL connection to the Windows CE¡Vbased device.
REM 
REM Miniport NDIS Adapters
REM 
REM Name                 Medium
REM ======================================
REM AX887721             Ethernet 802.3
REM VMINI1               Ethernet 802.3

tux -o -d ndt_2c -c "-t AX887721 -s AX887721"


================================================================================
Test procedures:
	1. Make sure the CETK Clientside.exe program is NOT currently running on
	   your device.
	2. Start Windows CE Test Kit (CETK) on the desktop machine.
	3. Select "Start client..." from the "Connection" menu.
	4. On the "Device Connection" dialog, make sure the "Use Windows Sockets
	   for the client/server communication." checkbox is NOT checked.
	5. Click "Connect..." to get the connection to Windows CE target device.
	6. On the "Select a Windows CE Device" dialog, select the device you are
	   connecting to (typically "Default Device") and click OK.
	7. Select "Windows CE Device Driver Test Kit" and click right mouse key 
	   to select "Deselect All Tests".
	8. Expand the "Ethernet" test items under "Windows CE Device Driver Test Kit".
	9. Select "Two-Card Network Card Miniport Driver Test" and click right mouse key 
	   to select "Edit Command Line...". Enter <tux -o -d ndt_2c -c "-t AX887721 -s AX887721">
	   command on the Edit Command Line dialog and click OK.
	10.Select "Windows CE Device Driver Test Kit" and click right mouse key 
	   to select "Start Tests" to start the Ethernet testings.
================================================================================