0478013a: ndt_1c Msg: Querying if miniport is wireless
0478013a: ndt_1c Msg: Miniport AX88179_178A1 is ** NOT Wireless-LAN **
<TESTGROUP>

*** ==================================================================
*** SUITE INFORMATION
***
*** Suite Name:        N/A (built on the fly)
*** Suite Description: N/A
*** Number of Tests:   13
*** ==================================================================

*** ==================================================================
*** SYSTEM INFORMATION
***
*** Date and Time:          07/29/2013  8:40 PM (Monday)
***
*** Device Name:            CEPC28351
***
*** OS Version:             6.00
*** Build Number:           3122
*** Platform ID:            3 "Windows CE"
*** Version String:         ""
***
*** Processor Type:         0x000002AE (686) "Intel Pentium II"
*** Processor Architecture: 0x0000     (0) "Intel"
*** Page Size:              0x00001000 (4,096)
*** Minimum App Address:    0x00010000 (65,536)
*** Maximum App Address:    0x7FFFFFFF (2,147,483,647)
*** Active Processor Mask:  0x00000001
*** Number Of Processors:   1
*** Allocation Granularity: 0x00010000 (65,536)
*** Processor Level:        0x0002     (2)
*** Processor Revision:     0x0004     (4)
*** ==================================================================

*** ==================================================================
*** MEMORY INFO
***
*** Memory Total:    20,832,256 bytes
*** Memory Used:     16,576,512 bytes
*** Memory Free:      4,255,744 bytes
***
*** Kernel Used:        647,168 bytes
*** Water Mark:             306 pages
***
*** Store Total:     16,912,384 bytes
*** Store Used:         569,344 bytes
*** Store Free:      16,343,040 bytes
*** ==================================================================

BEGIN GROUP: ndt_1c.dll
   <TESTCASE ID=1>
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   *** TEST STARTING
   ***
   *** Test Name:      1c_OpenClose
   *** Test ID:        1
   *** Library Path:   \ndt_1c.dll
   *** Command Line:   -t AX88179_178A1
   *** Kernel Mode:    No
   *** Random Seed:    10409
   *** Thread Count:   0
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_OpenClose", Threads=0, Seed=10409
      0478013a: ndt_1c Msg: Start 1c_OpenClose test on the adapter AX88179_178A1
      0478013a: ndt_1c Msg: Opening adapter
      0478013a: ndt_1c Msg: Repeatedly binding and unbinding the adapter
      0478013a: ndt_1c Msg: Open and bind the adapter multiple times, then close each open instance
      0478013a: ndt_1c Msg: Opening 128 adapter instances (pass #0)
      0478013a: ndt_1c Msg: Closing all adapter instances
      0478013a: ndt_1c Msg: Opening 128 adapter instances (pass #1)
      0478013a: ndt_1c Msg: Closing all adapter instances
      0478013a: ndt_1c Msg: Opening 128 adapter instances (pass #2)
      0478013a: ndt_1c Msg: Closing all adapter instances
      0478013a: ndt_1c Msg: Opening 128 adapter instances (pass #3)
      0478013a: ndt_1c Msg: Closing all adapter instances
      0478013a: ndt_1c Msg: Opening 128 adapter instances (pass #4)
      0478013a: ndt_1c Msg: Closing all adapter instances
      0478013a: ndt_1c Msg: Opening 128 adapter instances (pass #5)
      0478013a: ndt_1c Msg: Closing all adapter instances
      0478013a: ndt_1c Msg: Opening 128 adapter instances (pass #6)
      0478013a: ndt_1c Msg: Closing all adapter instances
      0478013a: ndt_1c Msg: Opening 128 adapter instances (pass #7)
      0478013a: ndt_1c Msg: Closing all adapter instances
      0478013a: ndt_1c Msg: Opening 128 adapter instances (pass #8)
      0478013a: ndt_1c Msg: Closing all adapter instances
      0478013a: ndt_1c Msg: Opening 128 adapter instances (pass #9)
      0478013a: ndt_1c Msg: Closing all adapter instances
      0478013a: ndt_1c Msg: Opening 128 adapter instances (pass #10)
      0478013a: ndt_1c Msg: Closing all adapter instances
      0478013a: ndt_1c Msg: Opening 128 adapter instances (pass #11)
      0478013a: ndt_1c Msg: Closing all adapter instances
      0478013a: ndt_1c Msg: Opening 128 adapter instances (pass #12)
      0478013a: ndt_1c Msg: Closing all adapter instances
      0478013a: ndt_1c Msg: Opening 128 adapter instances (pass #13)
      0478013a: ndt_1c Msg: Closing all adapter instances
      0478013a: ndt_1c Msg: Opening 128 adapter instances (pass #14)
      0478013a: ndt_1c Msg: Closing all adapter instances
      0478013a: ndt_1c Msg: Opening 128 adapter instances (pass #15)
      0478013a: ndt_1c Msg: Closing all adapter instances
      0478013a: ndt_1c Msg: Test 1c_OpenClose on the adapter AX88179_178A1 PASS
   END TEST: "1c_OpenClose", PASSED, Time=7.003
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   *** TEST COMPLETED
   ***
   *** Test Name:      1c_OpenClose
   *** Test ID:        1
   *** Library Path:   \ndt_1c.dll
   *** Command Line:   -t AX88179_178A1
   *** Kernel Mode:    No
   *** Result:         Passed
   *** Random Seed:    10409
   *** Thread Count:   1
   *** Execution Time: 0:00:07.003
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   
   </TESTCASE RESULT="PASSED">
   <TESTCASE ID=2>
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   *** TEST STARTING
   ***
   *** Test Name:      1c_Send
   *** Test ID:        2
   *** Library Path:   \ndt_1c.dll
   *** Command Line:   -t AX88179_178A1
   *** Kernel Mode:    No
   *** Random Seed:    1262
   *** Thread Count:   0
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_Send", Threads=0, Seed=1262
      0478013a: ndt_1c Msg: Start 1c_Send test on the adapter AX88179_178A1
      0478013a: ndt_1c Msg: Getting basic info about the adapter
      0478013a: ndt_1c Msg: Get OID_GEN_MAXIMUM_TOTAL_SIZE = 1514
      0478013a: ndt_1c Msg: Get OID_GEN_MAXIMUM_FRAME_SIZE = 1500
      0478013a: ndt_1c Msg: Testing sending to a (random) directed address
      0478013a: ndt_1c Msg: Sending: Send
      0478013a: ndt_1c Msg: Sending to a random address
      0478013a: ndt_1c Msg: Sending: Send
      0478013a: ndt_1c Msg: Sending to a broadcast address
      0478013a: ndt_1c Msg: Sending: Send
      0478013a: ndt_1c Msg: Sending to a multicast/functional address
      0478013a: ndt_1c Msg: Sending: Send
      0478013a: ndt_1c Msg: Testing sending to a group of addresses
   END TEST: "1c_Send", PASSED, Time=49.231
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   *** TEST COMPLETED
   ***
   *** Test Name:      1c_Send
   *** Test ID:        2
   *** Library Path:   \ndt_1c.dll
   *** Command Line:   -t AX88179_178A1
   *** Kernel Mode:    No
   *** Result:         Passed
   *** Random Seed:    1262
   *** Thread Count:   1
   *** Execution Time: 0:00:49.231
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   
   </TESTCASE RESULT="PASSED">
   <TESTCASE ID=3>
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   *** TEST STARTING
   ***
   *** Test Name:      1c_LoopbackSend
   *** Test ID:        3
   *** Library Path:   \ndt_1c.dll
   *** Command Line:   -t AX88179_178A1
   *** Kernel Mode:    No
   *** Random Seed:    4159
   *** Thread Count:   0
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_LoopbackSend", Threads=0, Seed=4159
      0478013a: ndt_1c Msg: Start 1c_Loopback test
      0478013a: ndt_1c Msg: The test adapter is AX88179_178A1
      0478013a: ndt_1c Msg: Opening adapters
      0478013a: ndt_1c Msg: Binding adapters
      0478013a: ndt_1c Msg: Get basic adapter info
      0478013a: ndt_1c Msg: Maximum Frame size=1500
      0478013a: ndt_1c Msg: Possible filter settings:
      0478013a: ndt_1c Msg:   - Directed
      0478013a: ndt_1c Msg:   - Broadcast
      0478013a: ndt_1c Msg:   - Promiscuous
      0478013a: ndt_1c Msg:   - Multicast
      0478013a: ndt_1c Msg:   - All Multicast
      0478013a: ndt_1c Msg: Setting receiving filters
      0478013a: ndt_1c Msg: Set filter FILTER_NONE for instance 0
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+ for instance 1
      0478013a: ndt_1c Msg: Set filter FILTER_BROADCAST+ for instance 2
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+ for instance 3
      0478013a: ndt_1c Msg: Set filter FILTER_PROMISCUOUS+ for instance 4
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_PROMISCUOUS+ for instance 5
      0478013a: ndt_1c Msg: Set filter FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      0478013a: ndt_1c Msg: Start receiving
      0478013a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Test NIC's directed Addr
      0478013a: ndt_1c Msg: Stop receiving and checking results
      0478013a: ndt_1c Msg: Instance 0 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 1 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 2 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 3 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 4 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 5 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 6 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 7 received expected 300 packets
      0478013a: ndt_1c Msg: Setting receiving filters
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+ for instance 0
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+ for instance 1
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+ for instance 2
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+ for instance 3
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      0478013a: ndt_1c Msg: Start receiving
      0478013a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Test NIC's directed Addr
      0478013a: ndt_1c Msg: Stop receiving and checking results
      0478013a: ndt_1c Msg: Instance 0 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 1 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 2 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 3 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 4 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 5 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 6 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 7 received expected 300 packets
      0478013a: ndt_1c Msg: Setting receiving filters
      0478013a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+ for instance 0
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+ for instance 1
      0478013a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      0478013a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      0478013a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      0478013a: ndt_1c Msg: Start receiving
      0478013a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Test NIC's directed Addr
      0478013a: ndt_1c Msg: Stop receiving and checking results
      0478013a: ndt_1c Msg: Instance 0 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 1 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 2 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 3 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 4 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 5 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 6 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 7 received expected 300 packets
      0478013a: ndt_1c Msg: Setting receiving filters
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 0
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 1
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      0478013a: ndt_1c Msg: Start receiving
      0478013a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Test NIC's directed Addr
      0478013a: ndt_1c Msg: Stop receiving and checking results
      0478013a: ndt_1c Msg: Instance 0 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 1 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 2 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 3 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 4 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 5 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 6 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 7 received expected 300 packets
      0478013a: ndt_1c Msg: Setting receiving filters
      0478013a: ndt_1c Msg: Set filter FILTER_NONE for instance 0
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+ for instance 1
      0478013a: ndt_1c Msg: Set filter FILTER_BROADCAST+ for instance 2
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+ for instance 3
      0478013a: ndt_1c Msg: Set filter FILTER_PROMISCUOUS+ for instance 4
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_PROMISCUOUS+ for instance 5
      0478013a: ndt_1c Msg: Set filter FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      0478013a: ndt_1c Msg: Start receiving
      0478013a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Broadcast Addr
      0478013a: ndt_1c Msg: Stop receiving and checking results
      0478013a: ndt_1c Msg: Instance 0 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 1 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 2 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 3 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 4 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 5 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 6 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 7 received expected 300 packets
      0478013a: ndt_1c Msg: Setting receiving filters
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+ for instance 0
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+ for instance 1
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+ for instance 2
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+ for instance 3
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      0478013a: ndt_1c Msg: Start receiving
      0478013a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Broadcast Addr
      0478013a: ndt_1c Msg: Stop receiving and checking results
      0478013a: ndt_1c Msg: Instance 0 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 1 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 2 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 3 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 4 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 5 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 6 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 7 received expected 300 packets
      0478013a: ndt_1c Msg: Setting receiving filters
      0478013a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+ for instance 0
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+ for instance 1
      0478013a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      0478013a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      0478013a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      0478013a: ndt_1c Msg: Start receiving
      0478013a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Broadcast Addr
      0478013a: ndt_1c Msg: Stop receiving and checking results
      0478013a: ndt_1c Msg: Instance 0 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 1 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 2 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 3 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 4 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 5 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 6 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 7 received expected 300 packets
      0478013a: ndt_1c Msg: Setting receiving filters
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 0
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 1
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      0478013a: ndt_1c Msg: Start receiving
      0478013a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Broadcast Addr
      0478013a: ndt_1c Msg: Stop receiving and checking results
      0478013a: ndt_1c Msg: Instance 0 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 1 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 2 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 3 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 4 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 5 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 6 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 7 received expected 300 packets
      0478013a: ndt_1c Msg: Setting receiving filters
      0478013a: ndt_1c Msg: Set filter FILTER_NONE for instance 0
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+ for instance 1
      0478013a: ndt_1c Msg: Set filter FILTER_BROADCAST+ for instance 2
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+ for instance 3
      0478013a: ndt_1c Msg: Set filter FILTER_PROMISCUOUS+ for instance 4
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_PROMISCUOUS+ for instance 5
      0478013a: ndt_1c Msg: Set filter FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      0478013a: ndt_1c Msg: Start receiving
      0478013a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Any directed Random Addr
      0478013a: ndt_1c Msg: Stop receiving and checking results
      0478013a: ndt_1c Msg: Instance 0 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 1 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 2 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 3 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 4 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 5 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 6 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 7 received expected 300 packets
      0478013a: ndt_1c Msg: Setting receiving filters
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+ for instance 0
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+ for instance 1
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+ for instance 2
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+ for instance 3
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      0478013a: ndt_1c Msg: Start receiving
      0478013a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Any directed Random Addr
      0478013a: ndt_1c Msg: Stop receiving and checking results
      0478013a: ndt_1c Msg: Instance 0 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 1 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 2 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 3 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 4 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 5 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 6 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 7 received expected 300 packets
      0478013a: ndt_1c Msg: Setting receiving filters
      0478013a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+ for instance 0
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+ for instance 1
      0478013a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      0478013a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      0478013a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      0478013a: ndt_1c Msg: Start receiving
      0478013a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Any directed Random Addr
      0478013a: ndt_1c Msg: Stop receiving and checking results
      0478013a: ndt_1c Msg: Instance 0 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 1 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 2 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 3 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 4 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 5 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 6 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 7 received expected 300 packets
      0478013a: ndt_1c Msg: Setting receiving filters
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 0
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 1
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      0478013a: ndt_1c Msg: Start receiving
      0478013a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Any directed Random Addr
      0478013a: ndt_1c Msg: Stop receiving and checking results
      0478013a: ndt_1c Msg: Instance 0 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 1 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 2 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 3 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 4 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 5 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 6 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 7 received expected 300 packets
      0478013a: ndt_1c Msg: Setting receiving filters
      0478013a: ndt_1c Msg: Set filter FILTER_NONE for instance 0
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+ for instance 1
      0478013a: ndt_1c Msg: Set filter FILTER_BROADCAST+ for instance 2
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+ for instance 3
      0478013a: ndt_1c Msg: Set filter FILTER_PROMISCUOUS+ for instance 4
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_PROMISCUOUS+ for instance 5
      0478013a: ndt_1c Msg: Set filter FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      0478013a: ndt_1c Msg: Start receiving
      0478013a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Multicast Addr
      0478013a: ndt_1c Msg: Stop receiving and checking results
      0478013a: ndt_1c Msg: Instance 0 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 1 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 2 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 3 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 4 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 5 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 6 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 7 received expected 300 packets
      0478013a: ndt_1c Msg: Setting receiving filters
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+ for instance 0
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+ for instance 1
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+ for instance 2
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+ for instance 3
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      0478013a: ndt_1c Msg: Start receiving
      0478013a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Multicast Addr
      0478013a: ndt_1c Msg: Stop receiving and checking results
      0478013a: ndt_1c Msg: Instance 0 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 1 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 2 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 3 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 4 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 5 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 6 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 7 received expected 300 packets
      0478013a: ndt_1c Msg: Setting receiving filters
      0478013a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+ for instance 0
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+ for instance 1
      0478013a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      0478013a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      0478013a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      0478013a: ndt_1c Msg: Start receiving
      0478013a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Multicast Addr
      0478013a: ndt_1c Msg: Stop receiving and checking results
      0478013a: ndt_1c Msg: Instance 0 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 1 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 2 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 3 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 4 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 5 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 6 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 7 received expected 300 packets
      0478013a: ndt_1c Msg: Setting receiving filters
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 0
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 1
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      0478013a: ndt_1c Msg: Start receiving
      0478013a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Multicast Addr
      0478013a: ndt_1c Msg: Stop receiving and checking results
      0478013a: ndt_1c Msg: Instance 0 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 1 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 2 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 3 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 4 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 5 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 6 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 7 received expected 300 packets
      0478013a: ndt_1c Msg: Setting receiving filters
      0478013a: ndt_1c Msg: Set filter FILTER_NONE for instance 0
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+ for instance 1
      0478013a: ndt_1c Msg: Set filter FILTER_BROADCAST+ for instance 2
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+ for instance 3
      0478013a: ndt_1c Msg: Set filter FILTER_PROMISCUOUS+ for instance 4
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_PROMISCUOUS+ for instance 5
      0478013a: ndt_1c Msg: Set filter FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      0478013a: ndt_1c Msg: Start receiving
      0478013a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Bad Multicast Addr
      0478013a: ndt_1c Msg: Stop receiving and checking results
      0478013a: ndt_1c Msg: Instance 0 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 1 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 2 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 3 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 4 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 5 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 6 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 7 received expected 300 packets
      0478013a: ndt_1c Msg: Setting receiving filters
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+ for instance 0
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+ for instance 1
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+ for instance 2
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+ for instance 3
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      0478013a: ndt_1c Msg: Start receiving
      0478013a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Bad Multicast Addr
      0478013a: ndt_1c Msg: Stop receiving and checking results
      0478013a: ndt_1c Msg: Instance 0 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 1 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 2 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 3 properly didn't receive packets
      0478013a: ndt_1c Msg: Instance 4 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 5 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 6 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 7 received expected 300 packets
      0478013a: ndt_1c Msg: Setting receiving filters
      0478013a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+ for instance 0
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+ for instance 1
      0478013a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      0478013a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      0478013a: ndt_1c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      0478013a: ndt_1c Msg: Start receiving
      0478013a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Bad Multicast Addr
      0478013a: ndt_1c Msg: Stop receiving and checking results
      0478013a: ndt_1c Msg: Instance 0 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 1 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 2 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 3 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 4 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 5 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 6 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 7 received expected 300 packets
      0478013a: ndt_1c Msg: Setting receiving filters
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 0
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 1
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      0478013a: ndt_1c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      0478013a: ndt_1c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      0478013a: ndt_1c Msg: Start receiving
      0478013a: ndt_1c Msg: Sending 300 packets with size 128 bytes to Bad Multicast Addr
      0478013a: ndt_1c Msg: Stop receiving and checking results
      0478013a: ndt_1c Msg: Instance 0 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 1 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 2 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 3 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 4 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 5 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 6 received expected 300 packets
      0478013a: ndt_1c Msg: Instance 7 received expected 300 packets
      0478013a: ndt_1c Msg: Unbinding adapters
   END TEST: "1c_LoopbackSend", PASSED, Time=282.707
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   *** TEST COMPLETED
   ***
   *** Test Name:      1c_LoopbackSend
   *** Test ID:        3
   *** Library Path:   \ndt_1c.dll
   *** Command Line:   -t AX88179_178A1
   *** Kernel Mode:    No
   *** Result:         Passed
   *** Random Seed:    4159
   *** Thread Count:   1
   *** Execution Time: 0:04:42.707
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   
   </TESTCASE RESULT="PASSED">
   <TESTCASE ID=4>
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   *** TEST STARTING
   ***
   *** Test Name:      1c_LoopbackStress
   *** Test ID:        4
   *** Library Path:   \ndt_1c.dll
   *** Command Line:   -t AX88179_178A1
   *** Kernel Mode:    No
   *** Random Seed:    13620
   *** Thread Count:   0
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_LoopbackStress", Threads=0, Seed=13620
      0478013a: ndt_1c Msg: Start 1c_LoopbackStess test on the adapter AX88179_178A1
      0478013a: ndt_1c Msg: Getting informations about the adapter
      0478013a: ndt_1c Msg: Opening adapters
      0478013a: ndt_1c Msg: Start Stress Tests
      0478013a: ndt_1c Msg: Test #0
      0478013a: ndt_1c Msg: Binding adapters
      0478013a: ndt_1c Msg: Start receiving
      0478013a: ndt_1c Msg: Start sending
      0478013a: ndt_1c Msg: Wait to finish with sending
      0478013a: ndt_1c Msg: Stop listening
      0478013a: ndt_1c Msg: Bind #0: Sent 10000 packets with total size 7624989 bytes in 12490 ms
      0478013a: ndt_1c Msg: Bind #0: Recv 10000 packets with total size 460000 bytes in 12490 ms
      0478013a: ndt_1c Msg: Bind #1: Recv 10000 packets with total size 7764989 bytes in 12490 ms
      0478013a: ndt_1c Msg: Bind #1: Sent 10000 packets with total size 460000 bytes in 12490 ms
      0478013a: ndt_1c Msg: Unbinding adapters
      0478013a: ndt_1c Msg: Test #1
      0478013a: ndt_1c Msg: Binding adapters
      0478013a: ndt_1c Msg: Start receiving
      0478013a: ndt_1c Msg: Start sending
      0478013a: ndt_1c Msg: Wait to finish with sending
      0478013a: ndt_1c Msg: Stop listening
      0478013a: ndt_1c Msg: Bind #0: Sent 10000 packets with total size 7693008 bytes in 12491 ms
      0478013a: ndt_1c Msg: Bind #0: Recv 10000 packets with total size 460000 bytes in 12491 ms
      0478013a: ndt_1c Msg: Bind #1: Recv 10000 packets with total size 7833008 bytes in 12491 ms
      0478013a: ndt_1c Msg: Bind #1: Sent 10000 packets with total size 460000 bytes in 12491 ms
      0478013a: ndt_1c Msg: Unbinding adapters
      0478013a: ndt_1c Msg: Test #2
      0478013a: ndt_1c Msg: Binding adapters
      0478013a: ndt_1c Msg: Start receiving
      0478013a: ndt_1c Msg: Start sending
      0478013a: ndt_1c Msg: Wait to finish with sending
      0478013a: ndt_1c Msg: Stop listening
      0478013a: ndt_1c Msg: Bind #0: Sent 10000 packets with total size 7759467 bytes in 12490 ms
      0478013a: ndt_1c Msg: Bind #0: Recv 10000 packets with total size 460000 bytes in 12490 ms
      0478013a: ndt_1c Msg: Bind #1: Recv 10000 packets with total size 7899467 bytes in 12490 ms
      0478013a: ndt_1c Msg: Bind #1: Sent 10000 packets with total size 460000 bytes in 12490 ms
      0478013a: ndt_1c Msg: Unbinding adapters
      0478013a: ndt_1c Msg: Test #3
      0478013a: ndt_1c Msg: Binding adapters
      0478013a: ndt_1c Msg: Start receiving
      0478013a: ndt_1c Msg: Start sending
      0478013a: ndt_1c Msg: Wait to finish with sending
      0478013a: ndt_1c Msg: Stop listening
      0478013a: ndt_1c Msg: Bind #0: Sent 100 packets with total size 8250 bytes in 120 ms
      0478013a: ndt_1c Msg: Bind #0: Recv 100 packets with total size 4600 bytes in 120 ms
      0478013a: ndt_1c Msg: Bind #1: Recv 100 packets with total size 9650 bytes in 120 ms
      0478013a: ndt_1c Msg: Bind #1: Sent 100 packets with total size 4600 bytes in 120 ms
      0478013a: ndt_1c Msg: Unbinding adapters
      0478013a: ndt_1c Msg: Test #4
      0478013a: ndt_1c Msg: Binding adapters
      0478013a: ndt_1c Msg: Start receiving
      0478013a: ndt_1c Msg: Start sending
      0478013a: ndt_1c Msg: Wait to finish with sending
      0478013a: ndt_1c Msg: Stop listening
      0478013a: ndt_1c Msg: Bind #0: Sent 53 packets with total size 3127 bytes in 60 ms
      0478013a: ndt_1c Msg: Bind #0: Recv 53 packets with total size 3869 bytes in 60 ms
      0478013a: ndt_1c Msg: Bind #1: Recv 53 packets with total size 3869 bytes in 60 ms
      0478013a: ndt_1c Msg: Bind #1: Sent 53 packets with total size 3869 bytes in 60 ms
      0478013a: ndt_1c Msg: Unbinding adapters
      0478013a: ndt_1c Msg: Test #5
      0478013a: ndt_1c Msg: Binding adapters
      0478013a: ndt_1c Msg: Start receiving
      0478013a: ndt_1c Msg: Start sending
      0478013a: ndt_1c Msg: Wait to finish with sending
      0478013a: ndt_1c Msg: Stop listening
      0478013a: ndt_1c Msg: Bind #0: Sent 10000 packets with total size 1000000 bytes in 12491 ms
      0478013a: ndt_1c Msg: Bind #0: Recv 10000 packets with total size 460000 bytes in 12491 ms
      0478013a: ndt_1c Msg: Bind #1: Recv 10000 packets with total size 1140000 bytes in 12491 ms
      0478013a: ndt_1c Msg: Bind #1: Sent 10000 packets with total size 460000 bytes in 12491 ms
      0478013a: ndt_1c Msg: Unbinding adapters
      0478013a: ndt_1c Msg: Test #6
      0478013a: ndt_1c Msg: Binding adapters
      0478013a: ndt_1c Msg: Start receiving
      0478013a: ndt_1c Msg: Start sending
      0478013a: ndt_1c Msg: Wait to finish with sending
      0478013a: ndt_1c Msg: Stop listening
      0478013a: ndt_1c Msg: Bind #0: Sent 10000 packets with total size 7652859 bytes in 12490 ms
      0478013a: ndt_1c Msg: Bind #0: Recv 10000 packets with total size 460000 bytes in 12490 ms
      0478013a: ndt_1c Msg: Bind #1: Recv 10000 packets with total size 7792859 bytes in 12490 ms
      0478013a: ndt_1c Msg: Bind #1: Sent 10000 packets with total size 460000 bytes in 12490 ms
      0478013a: ndt_1c Msg: Unbinding adapters
      0478013a: ndt_1c Msg: Test #7
      0478013a: ndt_1c Msg: Binding adapters
      0478013a: ndt_1c Msg: Start receiving
      0478013a: ndt_1c Msg: Start sending
      0478013a: ndt_1c Msg: Wait to finish with sending
      0478013a: ndt_1c Msg: Stop listening
      0478013a: ndt_1c Msg: Bind #0: Sent 10000 packets with total size 7641814 bytes in 12490 ms
      0478013a: ndt_1c Msg: Bind #0: Recv 0 packets with total size 0 bytes in 12490 ms
      0478013a: ndt_1c Msg: Bind #1: Recv 10000 packets with total size 7781814 bytes in 12490 ms
      0478013a: ndt_1c Msg: Bind #1: Sent 0 packets with total size 0 bytes in 12490 ms
      0478013a: ndt_1c Msg: Unbinding adapters
      0478013a: ndt_1c Msg: Test #8
      0478013a: ndt_1c Msg: Binding adapters
      0478013a: ndt_1c Msg: Start receiving
      0478013a: ndt_1c Msg: Start sending
      0478013a: ndt_1c Msg: Wait to finish with sending
      0478013a: ndt_1c Msg: Stop listening
      0478013a: ndt_1c Msg: Bind #0: Sent 10000 packets with total size 7631628 bytes in 12491 ms
      0478013a: ndt_1c Msg: Bind #0: Recv 10000 packets with total size 7771628 bytes in 12491 ms
      0478013a: ndt_1c Msg: Bind #1: Recv 10000 packets with total size 7771628 bytes in 12491 ms
      0478013a: ndt_1c Msg: Bind #1: Sent 10000 packets with total size 7771628 bytes in 12491 ms
      0478013a: ndt_1c Msg: Unbinding adapters
      0478013a: ndt_1c Msg: Test #9
      0478013a: ndt_1c Msg: Binding adapters
      0478013a: ndt_1c Msg: Start receiving
      0478013a: ndt_1c Msg: Start sending
      0478013a: ndt_1c Msg: Wait to finish with sending
      0478013a: ndt_1c Msg: Stop listening
      0478013a: ndt_1c Msg: Bind #0: Sent 10000 packets with total size 600000 bytes in 12490 ms
      0478013a: ndt_1c Msg: Bind #0: Recv 10000 packets with total size 740000 bytes in 12490 ms
      0478013a: ndt_1c Msg: Bind #1: Recv 10000 packets with total size 740000 bytes in 12490 ms
      0478013a: ndt_1c Msg: Bind #1: Sent 10000 packets with total size 740000 bytes in 12490 ms
      0478013a: ndt_1c Msg: Unbinding adapters
      0478013a: ndt_1c Msg: Start simultaneous stress tests
      0478013a: ndt_1c Msg: Binding to adapters
      0478013a: ndt_1c Msg: Start receiving
      0478013a: ndt_1c Msg: Start sending
      0478013a: ndt_1c Msg: Wait to finish with sending
      0478013a: ndt_1c Msg: Stop listening
      0478013a: ndt_1c Msg: Bind #0: Sent 6 packets with total size 213 bytes in 0 ms
      0478013a: ndt_1c Msg: Bind #0: Recv 6 packets with total size 297 bytes in 0 ms
      0478013a: ndt_1c Msg: Bind #1: Sent 6 packets with total size 213 bytes in 0 ms
      0478013a: ndt_1c Msg: Bind #1: Recv 6 packets with total size 297 bytes in 0 ms
      0478013a: ndt_1c Msg: Bind #2: Sent 6 packets with total size 213 bytes in 0 ms
      0478013a: ndt_1c Msg: Bind #2: Recv 6 packets with total size 297 bytes in 0 ms
      0478013a: ndt_1c Msg: Bind #3: Sent 6 packets with total size 213 bytes in 0 ms
      0478013a: ndt_1c Msg: Bind #3: Recv 6 packets with total size 297 bytes in 0 ms
      0478013a: ndt_1c Msg: Bind #4: Recv 6 packets with total size 297 bytes in 0 ms
      0478013a: ndt_1c Msg: Bind #4: Sent 6 packets with total size 297 bytes in 0 ms
      0478013a: ndt_1c Msg: Bind #5: Recv 6 packets with total size 297 bytes in 0 ms
      0478013a: ndt_1c Msg: Bind #5: Sent 6 packets with total size 297 bytes in 0 ms
      0478013a: ndt_1c Msg: Bind #6: Recv 6 packets with total size 297 bytes in 0 ms
      0478013a: ndt_1c Msg: Bind #6: Sent 6 packets with total size 297 bytes in 0 ms
      0478013a: ndt_1c Msg: Bind #7: Recv 6 packets with total size 297 bytes in 0 ms
      0478013a: ndt_1c Msg: Bind #7: Sent 6 packets with total size 297 bytes in 0 ms
      0478013a: ndt_1c Msg: Unbinding adapters
      0478013a: ndt_1c Msg: Closing adapters
   END TEST: "1c_LoopbackStress", PASSED, Time=123.545
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   *** TEST COMPLETED
   ***
   *** Test Name:      1c_LoopbackStress
   *** Test ID:        4
   *** Library Path:   \ndt_1c.dll
   *** Command Line:   -t AX88179_178A1
   *** Kernel Mode:    No
   *** Result:         Passed
   *** Random Seed:    13620
   *** Thread Count:   1
   *** Execution Time: 0:02:03.545
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   
   </TESTCASE RESULT="PASSED">
   <TESTCASE ID=5>
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   *** TEST STARTING
   ***
   *** Test Name:      1c_SetMulticast
   *** Test ID:        5
   *** Library Path:   \ndt_1c.dll
   *** Command Line:   -t AX88179_178A1
   *** Kernel Mode:    No
   *** Random Seed:    11747
   *** Thread Count:   0
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_SetMulticast", Threads=0, Seed=11747
      0478013a: ndt_1c Msg: Start 1c_SetMulticast test
      0478013a: ndt_1c Msg: The test adapter is AX88179_178A1
      0478013a: ndt_1c Msg: Opening adapters
      0478013a: ndt_1c Msg: Binding to adapters
      0478013a: ndt_1c Msg: GetMaxListSize
      0478013a: ndt_1c Msg: Driver support 64 address in multicast list
      0478013a: ndt_1c Msg: 64 multicast addresses will be tested
      0478013a: ndt_1c Msg: Add/Delete a multicast address multiple times
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add as many multicast addresses as driver says it supports
      0478013a: ndt_1c Msg: Adding multicast address 1
      0478013a: ndt_1c Msg: Adding multicast address 2
      0478013a: ndt_1c Msg: Adding multicast address 3
      0478013a: ndt_1c Msg: Adding multicast address 4
      0478013a: ndt_1c Msg: Adding multicast address 5
      0478013a: ndt_1c Msg: Adding multicast address 6
      0478013a: ndt_1c Msg: Adding multicast address 7
      0478013a: ndt_1c Msg: Adding multicast address 8
      0478013a: ndt_1c Msg: Adding multicast address 9
      0478013a: ndt_1c Msg: Adding multicast address 10
      0478013a: ndt_1c Msg: Adding multicast address 11
      0478013a: ndt_1c Msg: Adding multicast address 12
      0478013a: ndt_1c Msg: Adding multicast address 13
      0478013a: ndt_1c Msg: Adding multicast address 14
      0478013a: ndt_1c Msg: Adding multicast address 15
      0478013a: ndt_1c Msg: Adding multicast address 16
      0478013a: ndt_1c Msg: Adding multicast address 17
      0478013a: ndt_1c Msg: Adding multicast address 18
      0478013a: ndt_1c Msg: Adding multicast address 19
      0478013a: ndt_1c Msg: Adding multicast address 20
      0478013a: ndt_1c Msg: Adding multicast address 21
      0478013a: ndt_1c Msg: Adding multicast address 22
      0478013a: ndt_1c Msg: Adding multicast address 23
      0478013a: ndt_1c Msg: Adding multicast address 24
      0478013a: ndt_1c Msg: Adding multicast address 25
      0478013a: ndt_1c Msg: Adding multicast address 26
      0478013a: ndt_1c Msg: Adding multicast address 27
      0478013a: ndt_1c Msg: Adding multicast address 28
      0478013a: ndt_1c Msg: Adding multicast address 29
      0478013a: ndt_1c Msg: Adding multicast address 30
      0478013a: ndt_1c Msg: Adding multicast address 31
      0478013a: ndt_1c Msg: Adding multicast address 32
      0478013a: ndt_1c Msg: Adding multicast address 33
      0478013a: ndt_1c Msg: Adding multicast address 34
      0478013a: ndt_1c Msg: Adding multicast address 35
      0478013a: ndt_1c Msg: Adding multicast address 36
      0478013a: ndt_1c Msg: Adding multicast address 37
      0478013a: ndt_1c Msg: Adding multicast address 38
      0478013a: ndt_1c Msg: Adding multicast address 39
      0478013a: ndt_1c Msg: Adding multicast address 40
      0478013a: ndt_1c Msg: Adding multicast address 41
      0478013a: ndt_1c Msg: Adding multicast address 42
      0478013a: ndt_1c Msg: Adding multicast address 43
      0478013a: ndt_1c Msg: Adding multicast address 44
      0478013a: ndt_1c Msg: Adding multicast address 45
      0478013a: ndt_1c Msg: Adding multicast address 46
      0478013a: ndt_1c Msg: Adding multicast address 47
      0478013a: ndt_1c Msg: Adding multicast address 48
      0478013a: ndt_1c Msg: Adding multicast address 49
      0478013a: ndt_1c Msg: Adding multicast address 50
      0478013a: ndt_1c Msg: Adding multicast address 51
      0478013a: ndt_1c Msg: Adding multicast address 52
      0478013a: ndt_1c Msg: Adding multicast address 53
      0478013a: ndt_1c Msg: Adding multicast address 54
      0478013a: ndt_1c Msg: Adding multicast address 55
      0478013a: ndt_1c Msg: Adding multicast address 56
      0478013a: ndt_1c Msg: Adding multicast address 57
      0478013a: ndt_1c Msg: Adding multicast address 58
      0478013a: ndt_1c Msg: Adding multicast address 59
      0478013a: ndt_1c Msg: Adding multicast address 60
      0478013a: ndt_1c Msg: Adding multicast address 61
      0478013a: ndt_1c Msg: Adding multicast address 62
      0478013a: ndt_1c Msg: Adding multicast address 63
      0478013a: ndt_1c Msg: Adding multicast address 64
      0478013a: ndt_1c Msg: Delete all these added multicast addresses
      0478013a: ndt_1c Msg: Add/Delete a multicast address multiple times on two instances
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add/Query Multicast
      0478013a: ndt_1c Msg: Delete/Query Multicast
      0478013a: ndt_1c Msg: Add half of the maximum allowed list size multicast address to each open instance
      0478013a: ndt_1c Msg: Delete all these added multicast addresses
      0478013a: ndt_1c Msg: Unbinding adapters
      0478013a: ndt_1c Msg: Closing adapters
   END TEST: "1c_SetMulticast", PASSED, Time=0.697
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   *** TEST COMPLETED
   ***
   *** Test Name:      1c_SetMulticast
   *** Test ID:        5
   *** Library Path:   \ndt_1c.dll
   *** Command Line:   -t AX88179_178A1
   *** Kernel Mode:    No
   *** Result:         Passed
   *** Random Seed:    11747
   *** Thread Count:   1
   *** Execution Time: 0:00:00.697
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   
   </TESTCASE RESULT="PASSED">
   <TESTCASE ID=6>
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   *** TEST STARTING
   ***
   *** Test Name:      1c_Reset
   *** Test ID:        6
   *** Library Path:   \ndt_1c.dll
   *** Command Line:   -t AX88179_178A1
   *** Kernel Mode:    No
   *** Random Seed:    5631
   *** Thread Count:   0
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_Reset", Threads=0, Seed=5631
      0478013a: ndt_1c Msg: Start 1c_Reset test on the adapter AX88179_178A1
      0478013a: ndt_1c Msg: Opening adapters
      0478013a: ndt_1c Msg: Getting basic info about the adapter
      0478013a: ndt_1c Msg: Querying if miniport is wireless
      0478013a: ndt_1c Msg: Binding adapters
      0478013a: ndt_1c Msg: Sending packets
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Reset
      0478013a: ndt_1c Msg: Querying connect status
      0478013a: ndt_1c Msg: Unbinding adapters
      0478013a: ndt_1c Msg: Closing adapters
   END TEST: "1c_Reset", PASSED, Time=60.114
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   *** TEST COMPLETED
   ***
   *** Test Name:      1c_Reset
   *** Test ID:        6
   *** Library Path:   \ndt_1c.dll
   *** Command Line:   -t AX88179_178A1
   *** Kernel Mode:    No
   *** Result:         Passed
   *** Random Seed:    5631
   *** Thread Count:   1
   *** Execution Time: 0:01:00.114
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   
   </TESTCASE RESULT="PASSED">
   <TESTCASE ID=7>
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   *** TEST STARTING
   ***
   *** Test Name:      1c_CancelSend
   *** Test ID:        7
   *** Library Path:   \ndt_1c.dll
   *** Command Line:   -t AX88179_178A1
   *** Kernel Mode:    No
   *** Random Seed:    18427
   *** Thread Count:   0
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_CancelSend", Threads=0, Seed=18427
      0478013a: ndt_1c Msg: Start 1c_CancelSend test on the adapter AX88179_178A1
      0478013a: ndt_1c Msg: Opening adapters
      0478013a: ndt_1c Msg: Getting basic info about the adapter
      0478013a: ndt_1c Msg: Binding adapters
      0478013a: ndt_1c Msg: Sending and cancel packets
      0478013a: ndt_1c Msg: Unbind adapters
      0478013a: ndt_1c Msg: 1000 packets was sent. 0 packet wasn't canceled. 900 packet was.
      0478013a: ndt_1c Msg: Closing adapters
   END TEST: "1c_CancelSend", PASSED, Time=6.446
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   *** TEST COMPLETED
   ***
   *** Test Name:      1c_CancelSend
   *** Test ID:        7
   *** Library Path:   \ndt_1c.dll
   *** Command Line:   -t AX88179_178A1
   *** Kernel Mode:    No
   *** Result:         Passed
   *** Random Seed:    18427
   *** Thread Count:   1
   *** Execution Time: 0:00:06.446
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   
   </TESTCASE RESULT="PASSED">
   <TESTCASE ID=8>
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   *** TEST STARTING
   ***
   *** Test Name:      1c_FaultHandling
   *** Test ID:        8
   *** Library Path:   \ndt_1c.dll
   *** Command Line:   -t AX88179_178A1
   *** Kernel Mode:    No
   *** Random Seed:    27445
   *** Thread Count:   0
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_FaultHandling", Threads=0, Seed=27445
   END TEST: "1c_FaultHandling", SKIPPED, Time=0.000
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   *** TEST COMPLETED
   ***
   *** Test Name:      1c_FaultHandling
   *** Test ID:        8
   *** Library Path:   \ndt_1c.dll
   *** Command Line:   -t AX88179_178A1
   *** Kernel Mode:    No
   *** Result:         Skipped
   *** Random Seed:    27445
   *** Thread Count:   1
   *** Execution Time: 0:00:00.000
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   
   </TESTCASE RESULT="SKIPPED">
   <TESTCASE ID=9>
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   *** TEST STARTING
   ***
   *** Test Name:      1c_OIDs
   *** Test ID:        9
   *** Library Path:   \ndt_1c.dll
   *** Command Line:   -t AX88179_178A1
   *** Kernel Mode:    No
   *** Random Seed:    24126
   *** Thread Count:   0
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_OIDs", Threads=0, Seed=24126
      0478013a: ndt_1c Msg: Start 1c_TestOidsDeviceIoControl test on the adapter AX88179_178A1
      0478013a: ndt_1c Msg: Open adapter
      0478013a: ndt_1c Msg: Bind to adapter
      0478013a: ndt_1c Msg: Get Supported OIDs List
      0478013a: ndt_1c Msg: Check for all required OIDs
      0478013a: ndt_1c Msg: Check that listed OIDs really are supported
      0478013a: ndt_1c Msg: Checking if an OID 0x00010101 should be queried
      0478013a: ndt_1c Msg: The OID 0x00010101 was skippen
      0478013a: ndt_1c Msg: Checking if an OID 0x00010102 should be queried
      0478013a: ndt_1c Msg: Checking if an OID 0x00010103 should be queried
      0478013a: ndt_1c Msg: Checking if an OID 0x00010104 should be queried
      0478013a: ndt_1c Msg: Checking if an OID 0x00010114 should be queried
      0478013a: ndt_1c Msg: Checking if an OID 0x00010105 should be queried
      0478013a: ndt_1c Msg: Checking if an OID 0x00010106 should be queried
      0478013a: ndt_1c Msg: Checking if an OID 0x00010111 should be queried
      0478013a: ndt_1c Msg: Checking if an OID 0x00010115 should be queried
      0478013a: ndt_1c Msg: Checking if an OID 0x00010113 should be queried
      0478013a: ndt_1c Msg: Checking if an OID 0x00010107 should be queried
      0478013a: ndt_1c Msg: Checking if an OID 0x00010108 should be queried
      0478013a: ndt_1c Msg: Checking if an OID 0x0001010a should be queried
      0478013a: ndt_1c Msg: Checking if an OID 0x0002020e should be queried
      0478013a: ndt_1c Msg: The OID 0x0002020e isn't required, and hence not checked
      0478013a: ndt_1c Msg: Checking if an OID 0x00010109 should be queried
      0478013a: ndt_1c Msg: Checking if an OID 0x0001010b should be queried
      0478013a: ndt_1c Msg: Checking if an OID 0x0001010c should be queried
      0478013a: ndt_1c Msg: Checking if an OID 0x0001010d should be queried
      0478013a: ndt_1c Msg: Checking if an OID 0x00010116 should be queried
      0478013a: ndt_1c Msg: Checking if an OID 0x0001010e should be queried
      0478013a: ndt_1c Msg: Checking if an OID 0x0001010f should be queried
      0478013a: ndt_1c Msg: Checking if an OID 0x00010110 should be queried
      0478013a: ndt_1c Msg: Checking if an OID 0x00020101 should be queried
      0478013a: ndt_1c Msg: Checking if an OID 0x00020103 should be queried
      0478013a: ndt_1c Msg: Checking if an OID 0x00020102 should be queried
      0478013a: ndt_1c Msg: Checking if an OID 0x00020104 should be queried
      0478013a: ndt_1c Msg: Checking if an OID 0x00020105 should be queried
      0478013a: ndt_1c Msg: Checking if an OID 0x01010101 should be queried
      0478013a: ndt_1c Msg: Checking if an OID 0x01010102 should be queried
      0478013a: ndt_1c Msg: Checking if an OID 0x01010103 should be queried
      0478013a: ndt_1c Msg: Checking if an OID 0x01010104 should be queried
      0478013a: ndt_1c Msg: Checking if an OID 0x01020101 should be queried
      0478013a: ndt_1c Msg: Checking if an OID 0x01020102 should be queried
      0478013a: ndt_1c Msg: Checking if an OID 0x01020103 should be queried
      0478013a: ndt_1c Msg: Checking if an OID 0xfc010201 should be queried
      0478013a: ndt_1c Msg: The OID 0xfc010201 isn't required, and hence not checked
      0478013a: ndt_1c Msg: Checking if an OID 0xfd010100 should be queried
      0478013a: ndt_1c Msg: The OID 0xfd010100 isn't required, and hence not checked
      0478013a: ndt_1c Msg: Checking if an OID 0xfd010106 should be queried
      0478013a: ndt_1c Msg: The OID 0xfd010106 was skippen
      0478013a: ndt_1c Msg: Checking if an OID 0xfd010102 should be queried
      0478013a: ndt_1c Msg: The OID 0xfd010102 was skippen
      0478013a: ndt_1c Msg: Checking if an OID 0xfd010101 should be queried
      0478013a: ndt_1c Msg: The OID 0xfd010101 was skippen
      0478013a: ndt_1c Msg: Checking if an OID 0xfd010103 should be queried
      0478013a: ndt_1c Msg: The OID 0xfd010103 was skippen
      0478013a: ndt_1c Msg: Checking if an OID 0xfd010104 should be queried
      0478013a: ndt_1c Msg: The OID 0xfd010104 was skippen
      0478013a: ndt_1c Msg: Checking if an OID 0x0001021c should be queried
      0478013a: ndt_1c Msg: The OID 0x0001021c isn't required, and hence not checked
      0478013a: ndt_1c Msg: Close adapter
   END TEST: "1c_OIDs", PASSED, Time=0.101
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   *** TEST COMPLETED
   ***
   *** Test Name:      1c_OIDs
   *** Test ID:        9
   *** Library Path:   \ndt_1c.dll
   *** Command Line:   -t AX88179_178A1
   *** Kernel Mode:    No
   *** Result:         Passed
   *** Random Seed:    24126
   *** Thread Count:   1
   *** Execution Time: 0:00:00.101
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   
   </TESTCASE RESULT="PASSED">
   <TESTCASE ID=10>
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   *** TEST STARTING
   ***
   *** Test Name:      1c_64BitOIDs
   *** Test ID:        10
   *** Library Path:   \ndt_1c.dll
   *** Command Line:   -t AX88179_178A1
   *** Kernel Mode:    No
   *** Random Seed:    13287
   *** Thread Count:   0
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_64BitOIDs", Threads=0, Seed=13287
      0478013a: ndt_1c Msg: Start 1c_64BitOID test on the adapter AX88179_178A1
      0478013a: ndt_1c Msg: Open adapter
      0478013a: ndt_1c Msg: Bind to adapter
      0478013a: ndt_1c Msg: Link speed is equal or higher than 1.0Gbps
      0478013a: ndt_1c Msg: 64-bit statistics are required
      0478013a: ndt_1c Msg: Querying 64bit OIDs
      0478013a: ndt_1c Msg: Query with a null buffer
      0478013a: ndt_1c Msg: Query with a four byte buffer
      0478013a: ndt_1c Msg: Query with an eight byte buffer
      0478013a: ndt_1c Msg: Query with a null buffer
      0478013a: ndt_1c Msg: Query with a four byte buffer
      0478013a: ndt_1c Msg: Query with an eight byte buffer
      0478013a: ndt_1c Msg: Unbind adapter
      0478013a: ndt_1c Msg: Close adapter
   END TEST: "1c_64BitOIDs", PASSED, Time=0.234
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   *** TEST COMPLETED
   ***
   *** Test Name:      1c_64BitOIDs
   *** Test ID:        10
   *** Library Path:   \ndt_1c.dll
   *** Command Line:   -t AX88179_178A1
   *** Kernel Mode:    No
   *** Result:         Passed
   *** Random Seed:    13287
   *** Thread Count:   1
   *** Execution Time: 0:00:00.234
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   
   </TESTCASE RESULT="PASSED">
   <TESTCASE ID=11>
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   *** TEST STARTING
   ***
   *** Test Name:      1c_SuspendResume
   *** Test ID:        11
   *** Library Path:   \ndt_1c.dll
   *** Command Line:   -t AX88179_178A1
   *** Kernel Mode:    No
   *** Random Seed:    10660
   *** Thread Count:   0
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_SuspendResume", Threads=0, Seed=10660
      0478013a: ndt_1c Msg: Start 1c_SusRes (Suspend/Resume) test on the adapter AX88179_178A1
      0478013a: ndt_1c Msg: Enabling the Wake up source : SYSINTR_RTC_ALARM
      0478013a: ndt_1c Wrn: SKIPPING TEST: The system does not support enabling waking up from suspend (IOCTL_HAL_ENABLE_WAKE)
   END TEST: "1c_SuspendResume", SKIPPED, Time=0.001
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   *** TEST COMPLETED
   ***
   *** Test Name:      1c_SuspendResume
   *** Test ID:        11
   *** Library Path:   \ndt_1c.dll
   *** Command Line:   -t AX88179_178A1
   *** Kernel Mode:    No
   *** Result:         Skipped
   *** Random Seed:    10660
   *** Thread Count:   1
   *** Execution Time: 0:00:00.001
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   
   </TESTCASE RESULT="SKIPPED">
   <TESTCASE ID=12>
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   *** TEST STARTING
   ***
   *** Test Name:      1c_StressSusRes
   *** Test ID:        12
   *** Library Path:   \ndt_1c.dll
   *** Command Line:   -t AX88179_178A1
   *** Kernel Mode:    No
   *** Random Seed:    2081
   *** Thread Count:   0
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_StressSusRes", Threads=0, Seed=2081
      0478013a: ndt_1c Msg: Start 1c_StressSusRes (Stress in Suspend/Resume) test on the adapter AX88179_178A1
      0478013a: ndt_1c Msg: Opening adapter
      0478013a: ndt_1c Msg: Binding to it
      0478013a: ndt_1c Msg: Checking if miniport is PM aware.
      0478013a: ndt_1c Msg: AX88179_178A1 supports Power Management and one or more wake-up capabilities
      011ea216: ndt_1c Msg: StressOIDs: AX88179_178A1 supports ** 42 ** OIDs
      011ea216: ndt_1c Msg: StressOIDs: stress started
      05f107a6: ndt_1c Msg: StressSendRecv: stress started
      05f107a6: ndt_1c Msg: StressSendRecv: Sending 1000 packets each of 64 size to a random address
      0478013a: ndt_1c Msg: Transitioning the adapter to D4 state 1 time
      0478013a: ndt_1c Msg: Transitioning back to D0 state 1 time
      0478013a: ndt_1c Msg: Waiting 1000 mili sec
      0478013a: ndt_1c Msg: Transitioning the adapter to D4 state 2 time
      0478013a: ndt_1c Msg: Transitioning back to D0 state 2 time
      0478013a: ndt_1c Msg: Waiting 1000 mili sec
      0478013a: ndt_1c Msg: Transitioning the adapter to D4 state 3 time
      0478013a: ndt_1c Msg: Transitioning back to D0 state 3 time
      0478013a: ndt_1c Msg: Waiting 1000 mili sec
      0478013a: ndt_1c Msg: Transitioning the adapter to D4 state 4 time
      0478013a: ndt_1c Msg: Transitioning back to D0 state 4 time
      0478013a: ndt_1c Msg: Waiting 1000 mili sec
      0478013a: ndt_1c Msg: Transitioning the adapter to D4 state 5 time
      0478013a: ndt_1c Msg: Transitioning back to D0 state 5 time
      0478013a: ndt_1c Msg: Waiting 1000 mili sec
      0478013a: ndt_1c Msg: Transitioning the adapter to D4 state 6 time
      0478013a: ndt_1c Msg: Transitioning back to D0 state 6 time
      0478013a: ndt_1c Msg: Waiting 2000 mili sec
      0478013a: ndt_1c Msg: Transitioning the adapter to D4 state 7 time
      0478013a: ndt_1c Msg: Transitioning back to D0 state 7 time
      0478013a: ndt_1c Msg: Waiting 2000 mili sec
      0478013a: ndt_1c Msg: Transitioning the adapter to D4 state 8 time
      0478013a: ndt_1c Msg: Transitioning back to D0 state 8 time
      0478013a: ndt_1c Msg: Waiting 2000 mili sec
      0478013a: ndt_1c Msg: Transitioning the adapter to D4 state 9 time
      0478013a: ndt_1c Msg: Transitioning back to D0 state 9 time
      0478013a: ndt_1c Msg: Waiting 2000 mili sec
      0478013a: ndt_1c Msg: Transitioning the adapter to D4 state 10 time
      0478013a: ndt_1c Msg: Transitioning back to D0 state 10 time
      0478013a: ndt_1c Msg: Waiting 2000 mili sec
      0478013a: ndt_1c Msg: Transitioning the adapter to D4 state 11 time
      0478013a: ndt_1c Msg: Transitioning back to D0 state 11 time
      0478013a: ndt_1c Msg: Waiting 4000 mili sec
      0478013a: ndt_1c Msg: Transitioning the adapter to D4 state 12 time
      0478013a: ndt_1c Msg: Transitioning back to D0 state 12 time
      0478013a: ndt_1c Msg: Waiting 4000 mili sec
      05f107a6: ndt_1c Msg: StressSendRecv: 71 packets each of 64 size were SendCompleted
      05f107a6: ndt_1c Msg: StressSendRecv: Sending 1000 packets each of 127 size to a random address
      0478013a: ndt_1c Msg: Transitioning the adapter to D4 state 13 time
      0478013a: ndt_1c Msg: Transitioning back to D0 state 13 time
      0478013a: ndt_1c Msg: Waiting 4000 mili sec
      0478013a: ndt_1c Msg: Transitioning the adapter to D4 state 14 time
      0478013a: ndt_1c Msg: Transitioning back to D0 state 14 time
      0478013a: ndt_1c Msg: Waiting 4000 mili sec
      0478013a: ndt_1c Msg: Transitioning the adapter to D4 state 15 time
      0478013a: ndt_1c Msg: Transitioning back to D0 state 15 time
      0478013a: ndt_1c Msg: Waiting 4000 mili sec
      0478013a: ndt_1c Msg: Transitioning the adapter to D4 state 16 time
      0478013a: ndt_1c Msg: Transitioning back to D0 state 16 time
      0478013a: ndt_1c Msg: Waiting 5000 mili sec
      0478013a: ndt_1c Msg: Transitioning the adapter to D4 state 17 time
      0478013a: ndt_1c Msg: Transitioning back to D0 state 17 time
      0478013a: ndt_1c Msg: Waiting 5000 mili sec
      0478013a: ndt_1c Msg: Transitioning the adapter to D4 state 18 time
      0478013a: ndt_1c Msg: Transitioning back to D0 state 18 time
      0478013a: ndt_1c Msg: Waiting 5000 mili sec
      0478013a: ndt_1c Msg: Transitioning the adapter to D4 state 19 time
      0478013a: ndt_1c Msg: Transitioning back to D0 state 19 time
      0478013a: ndt_1c Msg: Waiting 5000 mili sec
      05f107a6: ndt_1c Msg: StressSendRecv: 341 packets each of 127 size were SendCompleted
      05f107a6: ndt_1c Msg: StressSendRecv: Sending 1000 packets each of 190 size to a random address
      0478013a: ndt_1c Msg: Transitioning the adapter to D4 state 20 time
      0478013a: ndt_1c Msg: Transitioning back to D0 state 20 time
      0478013a: ndt_1c Msg: Waiting 5000 mili sec
      0478013a: ndt_1c Msg: Waiting for Stress OIDs thread to terminate
      011ea216: ndt_1c Msg: StressOIDs: signaled to stop
      011ea216: ndt_1c Msg: StressOIDs: Cleaned up & exiting.
      0478013a: ndt_1c Msg: Stress OIDs thread exited with exit value : PASS
      0478013a: ndt_1c Msg: Waiting for StressSendRecv thread to terminate
      05f107a6: ndt_1c Msg: StressSendRecv: 897 packets each of 190 size were SendCompleted
      05f107a6: ndt_1c Msg: StressSendRecv: signaled to stop
      05f107a6: ndt_1c Msg: StressSendRecv: Cleaned up & exiting.
      0478013a: ndt_1c Msg: Stress SendRecv thread exited with exit value : PASS
      0478013a: ndt_1c Msg: Unbinding to it
      0478013a: ndt_1c Msg: Closing adapter
   END TEST: "1c_StressSusRes", PASSED, Time=120.337
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   *** TEST COMPLETED
   ***
   *** Test Name:      1c_StressSusRes
   *** Test ID:        12
   *** Library Path:   \ndt_1c.dll
   *** Command Line:   -t AX88179_178A1
   *** Kernel Mode:    No
   *** Result:         Passed
   *** Random Seed:    2081
   *** Thread Count:   1
   *** Execution Time: 0:02:00.337
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   
   </TESTCASE RESULT="PASSED">
   <TESTCASE ID=13>
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   *** TEST STARTING
   ***
   *** Test Name:      1c_ResetOnResume
   *** Test ID:        13
   *** Library Path:   \ndt_1c.dll
   *** Command Line:   -t AX88179_178A1
   *** Kernel Mode:    No
   *** Random Seed:    6834
   *** Thread Count:   0
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "1c_ResetOnResume", Threads=0, Seed=6834
      0478013a: ndt_1c Msg: Start 1c_ResetOnResume (Reset on Resume) test on the adapter AX88179_178A1
      0478013a: ndt_1c Msg: This test will test if AX88179_178A1 restores its settings after Reset
      0478013a: ndt_1c Msg: AX88179_178A1 supports Power Management and one or more wake-up capabilities
      0478013a: ndt_1c Msg: Set CURRENT_PACKET_FILTER = NDIS_PACKET_TYPE_MULTICAST|NDIS_PACKET_TYPE_DIRECTED for adapter AX88179_178A1
      0478013a: ndt_1c Msg: AX88179_178A1 supports max 64 Multicast addresses
      0478013a: ndt_1c Msg: Got the current complete list of multicast addresses for AX88179_178A1
      0478013a: ndt_1c Msg: It has 0 multicast addresses set
      0478013a: ndt_1c Msg: Set 4 multicast addresses for AX88179_178A1
      0478013a: ndt_1c Msg: We'll RESET the device & at the end of every RESET we'll verify if AX88179_178A1 restores its settings or not
      0478013a: ndt_1c Msg: Reseting the network adapter AX88179_178A1 1 time
      0478013a: ndt_1c Msg: Waiting to receive NDIS_STATUS_RESET_END notification on the miniport adapter AX88179_178A1
      0478013a: ndt_1c Msg: Received NDIS_STATUS_RESET_END notification on AX88179_178A1
      0478013a: ndt_1c Msg: AX88179_178A1 has restored/retained its Packet Filter settings.
      0478013a: ndt_1c Msg: AX88179_178A1 has restored/retained its multicast addresses list.
      0478013a: ndt_1c Msg: AX88179_178A1 has passed ResetOnResume test
      0478013a: ndt_1c Msg: Reseting the network adapter AX88179_178A1 2 time
      0478013a: ndt_1c Msg: Waiting to receive NDIS_STATUS_RESET_END notification on the miniport adapter AX88179_178A1
      0478013a: ndt_1c Msg: Received NDIS_STATUS_RESET_END notification on AX88179_178A1
      0478013a: ndt_1c Msg: AX88179_178A1 has restored/retained its Packet Filter settings.
      0478013a: ndt_1c Msg: AX88179_178A1 has restored/retained its multicast addresses list.
      0478013a: ndt_1c Msg: AX88179_178A1 has passed ResetOnResume test
      0478013a: ndt_1c Msg: Reseting the network adapter AX88179_178A1 3 time
      0478013a: ndt_1c Msg: Waiting to receive NDIS_STATUS_RESET_END notification on the miniport adapter AX88179_178A1
      0478013a: ndt_1c Msg: Received NDIS_STATUS_RESET_END notification on AX88179_178A1
      0478013a: ndt_1c Msg: AX88179_178A1 has restored/retained its Packet Filter settings.
      0478013a: ndt_1c Msg: AX88179_178A1 has restored/retained its multicast addresses list.
      0478013a: ndt_1c Msg: AX88179_178A1 has passed ResetOnResume test
      0478013a: ndt_1c Msg: Reseting the network adapter AX88179_178A1 4 time
      0478013a: ndt_1c Msg: Waiting to receive NDIS_STATUS_RESET_END notification on the miniport adapter AX88179_178A1
      0478013a: ndt_1c Msg: Received NDIS_STATUS_RESET_END notification on AX88179_178A1
      0478013a: ndt_1c Msg: AX88179_178A1 has restored/retained its Packet Filter settings.
      0478013a: ndt_1c Msg: AX88179_178A1 has restored/retained its multicast addresses list.
      0478013a: ndt_1c Msg: AX88179_178A1 has passed ResetOnResume test
      0478013a: ndt_1c Msg: Reseting the network adapter AX88179_178A1 5 time
      0478013a: ndt_1c Msg: Waiting to receive NDIS_STATUS_RESET_END notification on the miniport adapter AX88179_178A1
      0478013a: ndt_1c Msg: Received NDIS_STATUS_RESET_END notification on AX88179_178A1
      0478013a: ndt_1c Msg: AX88179_178A1 has restored/retained its Packet Filter settings.
      0478013a: ndt_1c Msg: AX88179_178A1 has restored/retained its multicast addresses list.
      0478013a: ndt_1c Msg: AX88179_178A1 has passed ResetOnResume test
   END TEST: "1c_ResetOnResume", PASSED, Time=0.058
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   *** TEST COMPLETED
   ***
   *** Test Name:      1c_ResetOnResume
   *** Test ID:        13
   *** Library Path:   \ndt_1c.dll
   *** Command Line:   -t AX88179_178A1
   *** Kernel Mode:    No
   *** Result:         Passed
   *** Random Seed:    6834
   *** Thread Count:   1
   *** Execution Time: 0:00:00.058
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   
   </TESTCASE RESULT="PASSED">
END GROUP: ndt_1c.dll
*** ==================================================================
*** MEMORY INFO
***
*** Memory Total:    20,832,256 bytes
*** Memory Used:     16,805,888 bytes
*** Memory Free:      4,026,368 bytes
***
*** Kernel Used:        802,816 bytes
*** Water Mark:             306 pages
***
*** Store Total:     16,912,384 bytes
*** Store Used:         651,264 bytes
*** Store Free:      16,261,120 bytes
*** ==================================================================

*** ==================================================================
*** SUITE SUMMARY
***
*** Passed:         11
*** Failed:          0
*** Skipped:         2
*** Aborted:         0
*** -------- ---------
*** Total:          13
***
*** Cumulative Test Execution Time: 0:10:50.474
*** Total Tux Suite Execution Time: 0:10:51.668
*** CPU Idle Time:                  0:09:55.717
*** ==================================================================
</TESTGROUP>
@@@@@@0

