04050466: ndt_2c Msg: Querying if test miniport is wireless
04050466: ndt_2c Msg: Miniport AX88772C_772B1 is ** NOT Wireless-LAN **
<TESTGROUP>

*** ==================================================================
*** SUITE INFORMATION
***
*** Suite Name:        N/A (built on the fly)
*** Suite Description: N/A
*** Number of Tests:   6
*** ==================================================================

*** ==================================================================
*** SYSTEM INFORMATION
***
*** Date and Time:          08/09/2013 10:40 AM (Friday)
***
*** Device Name:            CEPC13475
***
*** OS Version:             7.00
*** Build Number:           2806
*** Platform ID:            3 "Windows CE"
*** Version String:         ""
***
*** Processor Type:         0x000002AE (686) "Intel Pentium II"
*** Processor Architecture: 0x0000     (0) "Intel"
*** Page Size:              0x00001000 (4,096)
*** Minimum App Address:    0x00010000 (65,536)
*** Maximum App Address:    0x7FFFFFFF (2,147,483,647)
*** Active Processor Mask:  0x00000001
*** Number Of Processors:   1
*** Allocation Granularity: 0x00010000 (65,536)
*** Processor Level:        0x000F     (15)
*** Processor Revision:     0x000D     (13)
*** ==================================================================

*** ==================================================================
*** MEMORY INFO
***
*** Memory Total:   746,651,648 bytes
*** Memory Used:     25,341,952 bytes
*** Memory Free:    721,309,696 bytes
***
*** Kernel Used:        753,664 bytes
*** Water Mark:         175,864 pages
***
*** Store Total:    133,971,968 bytes
*** Store Used:       1,241,088 bytes
*** Store Free:     132,730,880 bytes
*** ==================================================================

BEGIN GROUP: ndt_2c.dll
   <TESTCASE ID=1>
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   *** TEST STARTING
   ***
   *** Test Name:      2c_SendPackets
   *** Test ID:        1
   *** Library Path:   \ndt_2c.dll
   *** Command Line:   -t AX88772C_772B1 -s AX88772C_772B2
   *** Kernel Mode:    No
   *** Random Seed:    30629
   *** Thread Count:   0
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "2c_SendPackets", Threads=0, Seed=30629
      04050466: ndt_2c Msg: Start 2c_SendPackets test
      04050466: ndt_2c Msg: The test adapter is AX88772C_772B1
      04050466: ndt_2c Msg: The support adapter is AX88772C_772B2
      04050466: ndt_2c Msg: Setting conversation id to 1921358663
      04050466: ndt_2c Msg: Opening adapters
      04050466: ndt_2c Msg: Binding adapters
      04050466: ndt_2c Msg: Get basic adapters info
      04050466: ndt_2c Msg: Set adapter filters
      04050466: ndt_2c Msg: Sending 300 packets with size 64 bytes to 1 address
      04050466: ndt_2c Msg: Sent 300 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Received 300 packets
      04050466: ndt_2c Msg: Sending 300 packets with size 783 bytes to 1 address
      04050466: ndt_2c Msg: Sent 300 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Received 300 packets
      04050466: ndt_2c Msg: Sending 300 packets with size 1500 bytes to 1 address
      04050466: ndt_2c Msg: Sent 300 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Received 300 packets
      04050466: ndt_2c Msg: Sending 600 packets with size 64 bytes to 1 address
      04050466: ndt_2c Msg: Sent 600 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Received 600 packets
      04050466: ndt_2c Msg: Sending 600 packets with size 783 bytes to 1 address
      04050466: ndt_2c Msg: Sent 600 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Received 600 packets
      04050466: ndt_2c Msg: Sending 600 packets with size 1500 bytes to 1 address
      04050466: ndt_2c Msg: Sent 600 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Received 600 packets
      04050466: ndt_2c Msg: Sending 900 packets with size 64 bytes to 1 address
      04050466: ndt_2c Msg: Sent 900 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Received 900 packets
      04050466: ndt_2c Msg: Sending 900 packets with size 783 bytes to 1 address
      04050466: ndt_2c Msg: Sent 900 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Received 900 packets
      04050466: ndt_2c Msg: Sending 900 packets with size 1500 bytes to 1 address
      04050466: ndt_2c Msg: Sent 900 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Received 900 packets
      04050466: ndt_2c Msg: Sending 1200 packets with size 64 bytes to 1 address
      04050466: ndt_2c Msg: Sent 1200 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Received 1200 packets
      04050466: ndt_2c Msg: Sending 1200 packets with size 783 bytes to 1 address
      04050466: ndt_2c Msg: Sent 1200 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Received 1200 packets
      04050466: ndt_2c Msg: Sending 1200 packets with size 1500 bytes to 1 address
      04050466: ndt_2c Msg: Sent 1200 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Received 1200 packets
      04050466: ndt_2c Msg: Sending 1500 packets with size 64 bytes to 1 address
      04050466: ndt_2c Msg: Sent 1500 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Received 1500 packets
      04050466: ndt_2c Msg: Sending 1500 packets with size 783 bytes to 1 address
      04050466: ndt_2c Msg: Sent 1500 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Received 1500 packets
      04050466: ndt_2c Msg: Sending 1500 packets with size 1500 bytes to 1 address
      04050466: ndt_2c Msg: Sent 1500 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Received 1500 packets
      04050466: ndt_2c Msg: Sending 1800 packets with size 64 bytes to 1 address
      04050466: ndt_2c Msg: Sent 1800 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Received 1800 packets
      04050466: ndt_2c Msg: Sending 1800 packets with size 783 bytes to 1 address
      04050466: ndt_2c Msg: Sent 1800 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Received 1800 packets
      04050466: ndt_2c Msg: Sending 1800 packets with size 1500 bytes to 1 address
      04050466: ndt_2c Msg: Sent 1800 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Received 1800 packets
      04050466: ndt_2c Msg: Sending 2100 packets with size 64 bytes to 1 address
      04050466: ndt_2c Msg: Sent 2100 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Received 2100 packets
      04050466: ndt_2c Msg: Sending 2100 packets with size 783 bytes to 1 address
      04050466: ndt_2c Msg: Sent 2100 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Received 2100 packets
      04050466: ndt_2c Msg: Sending 2100 packets with size 1500 bytes to 1 address
      04050466: ndt_2c Msg: Sent 2100 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Received 2100 packets
      04050466: ndt_2c Msg: Sending 2400 packets with size 64 bytes to 1 address
      04050466: ndt_2c Msg: Sent 2400 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Received 2400 packets
      04050466: ndt_2c Msg: Sending 2400 packets with size 783 bytes to 1 address
      04050466: ndt_2c Msg: Sent 2400 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Received 2400 packets
      04050466: ndt_2c Msg: Sending 2400 packets with size 1500 bytes to 1 address
      04050466: ndt_2c Msg: Sent 2400 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Received 2400 packets
      04050466: ndt_2c Msg: Unbinding adapters
   END TEST: "2c_SendPackets", PASSED, Time=338.545
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   *** TEST COMPLETED
   ***
   *** Test Name:      2c_SendPackets
   *** Test ID:        1
   *** Library Path:   \ndt_2c.dll
   *** Command Line:   -t AX88772C_772B1 -s AX88772C_772B2
   *** Kernel Mode:    No
   *** Result:         Passed
   *** Random Seed:    30629
   *** Thread Count:   1
   *** Execution Time: 0:05:38.545
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   
   </TESTCASE RESULT="PASSED">
   <TESTCASE ID=2>
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   *** TEST STARTING
   ***
   *** Test Name:      2c_ReceivePackets
   *** Test ID:        2
   *** Library Path:   \ndt_2c.dll
   *** Command Line:   -t AX88772C_772B1 -s AX88772C_772B2
   *** Kernel Mode:    No
   *** Random Seed:    1756
   *** Thread Count:   0
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "2c_ReceivePackets", Threads=0, Seed=1756
      04050466: ndt_2c Msg: Start 2c_ReceivePackets test
      04050466: ndt_2c Msg: The test adapter is AX88772C_772B1
      04050466: ndt_2c Msg: The support adapter is AX88772C_772B2
      04050466: ndt_2c Msg: Opening adapters
      04050466: ndt_2c Msg: Binding adapters
      04050466: ndt_2c Msg: Get basic adapters info
      04050466: ndt_2c Msg: Set adapter filters
      04050466: ndt_2c Msg: Sending 2400 packets with size 64 bytes to 1 address
      04050466: ndt_2c Msg: Sent 2400 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Received 2400 packets
      04050466: ndt_2c Msg: Sending 2400 packets with size 783 bytes to 1 address
      04050466: ndt_2c Msg: Sent 2400 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Received 2400 packets
      04050466: ndt_2c Msg: Sending 2400 packets with size 1500 bytes to 1 address
      04050466: ndt_2c Msg: Sent 2400 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Received 2400 packets
      04050466: ndt_2c Msg: Unbinding adapters
   END TEST: "2c_ReceivePackets", PASSED, Time=42.319
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   *** TEST COMPLETED
   ***
   *** Test Name:      2c_ReceivePackets
   *** Test ID:        2
   *** Library Path:   \ndt_2c.dll
   *** Command Line:   -t AX88772C_772B1 -s AX88772C_772B2
   *** Kernel Mode:    No
   *** Result:         Passed
   *** Random Seed:    1756
   *** Thread Count:   1
   *** Execution Time: 0:00:42.319
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   
   </TESTCASE RESULT="PASSED">
   <TESTCASE ID=3>
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   *** TEST STARTING
   ***
   *** Test Name:      2c_FilterReceive
   *** Test ID:        3
   *** Library Path:   \ndt_2c.dll
   *** Command Line:   -t AX88772C_772B1 -s AX88772C_772B2
   *** Kernel Mode:    No
   *** Random Seed:    5772
   *** Thread Count:   0
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "2c_FilterReceive", Threads=0, Seed=5772
      04050466: ndt_2c Msg: Start 2c_FilterReceive test
      04050466: ndt_2c Msg: The test adapter is AX88772C_772B1
      04050466: ndt_2c Msg: The support adapter is AX88772C_772B2
      04050466: ndt_2c Msg: Opening adapters
      04050466: ndt_2c Msg: Binding adapters
      04050466: ndt_2c Msg: Get basic adapters info
      04050466: ndt_2c Msg: Possible filter settings:
      04050466: ndt_2c Msg:   - Directed
      04050466: ndt_2c Msg:   - Broadcast
      04050466: ndt_2c Msg:   - Promiscuous
      04050466: ndt_2c Msg:   - Multicast
      04050466: ndt_2c Msg:   - All Multicast
      04050466: ndt_2c Msg: Setting receiving filters
      04050466: ndt_2c Msg: Set filter FILTER_NONE for instance 0
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+ for instance 1
      04050466: ndt_2c Msg: Set filter FILTER_BROADCAST+ for instance 2
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+ for instance 3
      04050466: ndt_2c Msg: Set filter FILTER_PROMISCUOUS+ for instance 4
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_PROMISCUOUS+ for instance 5
      04050466: ndt_2c Msg: Set filter FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      04050466: ndt_2c Msg: Start receiving
      04050466: ndt_2c Msg: Sending 300 packets with size 128 bytes to Test NIC's directed Addr
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Instance 0 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 1 received expected 300 packets
      04050466: ndt_2c Msg: Instance 2 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 3 received expected 300 packets
      04050466: ndt_2c Msg: Instance 4 received expected 300 packets
      04050466: ndt_2c Msg: Instance 5 received expected 300 packets
      04050466: ndt_2c Msg: Instance 6 received expected 300 packets
      04050466: ndt_2c Msg: Instance 7 received expected 300 packets
      04050466: ndt_2c Msg: Setting receiving filters
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+ for instance 0
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+ for instance 1
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+ for instance 2
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+ for instance 3
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      04050466: ndt_2c Msg: Start receiving
      04050466: ndt_2c Msg: Sending 300 packets with size 128 bytes to Test NIC's directed Addr
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Instance 0 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 1 received expected 300 packets
      04050466: ndt_2c Msg: Instance 2 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 3 received expected 300 packets
      04050466: ndt_2c Msg: Instance 4 received expected 300 packets
      04050466: ndt_2c Msg: Instance 5 received expected 300 packets
      04050466: ndt_2c Msg: Instance 6 received expected 300 packets
      04050466: ndt_2c Msg: Instance 7 received expected 300 packets
      04050466: ndt_2c Msg: Setting receiving filters
      04050466: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+ for instance 0
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+ for instance 1
      04050466: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      04050466: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      04050466: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      04050466: ndt_2c Msg: Start receiving
      04050466: ndt_2c Msg: Sending 300 packets with size 128 bytes to Test NIC's directed Addr
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Instance 0 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 1 received expected 300 packets
      04050466: ndt_2c Msg: Instance 2 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 3 received expected 300 packets
      04050466: ndt_2c Msg: Instance 4 received expected 300 packets
      04050466: ndt_2c Msg: Instance 5 received expected 300 packets
      04050466: ndt_2c Msg: Instance 6 received expected 300 packets
      04050466: ndt_2c Msg: Instance 7 received expected 300 packets
      04050466: ndt_2c Msg: Setting receiving filters
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 0
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 1
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      04050466: ndt_2c Msg: Start receiving
      04050466: ndt_2c Msg: Sending 300 packets with size 128 bytes to Test NIC's directed Addr
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Instance 0 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 1 received expected 300 packets
      04050466: ndt_2c Msg: Instance 2 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 3 received expected 300 packets
      04050466: ndt_2c Msg: Instance 4 received expected 300 packets
      04050466: ndt_2c Msg: Instance 5 received expected 300 packets
      04050466: ndt_2c Msg: Instance 6 received expected 300 packets
      04050466: ndt_2c Msg: Instance 7 received expected 300 packets
      04050466: ndt_2c Msg: Setting receiving filters
      04050466: ndt_2c Msg: Set filter FILTER_NONE for instance 0
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+ for instance 1
      04050466: ndt_2c Msg: Set filter FILTER_BROADCAST+ for instance 2
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+ for instance 3
      04050466: ndt_2c Msg: Set filter FILTER_PROMISCUOUS+ for instance 4
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_PROMISCUOUS+ for instance 5
      04050466: ndt_2c Msg: Set filter FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      04050466: ndt_2c Msg: Start receiving
      04050466: ndt_2c Msg: Sending 300 packets with size 128 bytes to Broadcast Addr
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Instance 0 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 1 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 2 received expected 300 packets
      04050466: ndt_2c Msg: Instance 3 received expected 300 packets
      04050466: ndt_2c Msg: Instance 4 received expected 300 packets
      04050466: ndt_2c Msg: Instance 5 received expected 300 packets
      04050466: ndt_2c Msg: Instance 6 received expected 300 packets
      04050466: ndt_2c Msg: Instance 7 received expected 300 packets
      04050466: ndt_2c Msg: Setting receiving filters
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+ for instance 0
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+ for instance 1
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+ for instance 2
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+ for instance 3
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      04050466: ndt_2c Msg: Start receiving
      04050466: ndt_2c Msg: Sending 300 packets with size 128 bytes to Broadcast Addr
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Instance 0 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 1 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 2 received expected 300 packets
      04050466: ndt_2c Msg: Instance 3 received expected 300 packets
      04050466: ndt_2c Msg: Instance 4 received expected 300 packets
      04050466: ndt_2c Msg: Instance 5 received expected 300 packets
      04050466: ndt_2c Msg: Instance 6 received expected 300 packets
      04050466: ndt_2c Msg: Instance 7 received expected 300 packets
      04050466: ndt_2c Msg: Setting receiving filters
      04050466: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+ for instance 0
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+ for instance 1
      04050466: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      04050466: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      04050466: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      04050466: ndt_2c Msg: Start receiving
      04050466: ndt_2c Msg: Sending 300 packets with size 128 bytes to Broadcast Addr
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Instance 0 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 1 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 2 received expected 300 packets
      04050466: ndt_2c Msg: Instance 3 received expected 300 packets
      04050466: ndt_2c Msg: Instance 4 received expected 300 packets
      04050466: ndt_2c Msg: Instance 5 received expected 300 packets
      04050466: ndt_2c Msg: Instance 6 received expected 300 packets
      04050466: ndt_2c Msg: Instance 7 received expected 300 packets
      04050466: ndt_2c Msg: Setting receiving filters
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 0
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 1
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      04050466: ndt_2c Msg: Start receiving
      04050466: ndt_2c Msg: Sending 300 packets with size 128 bytes to Broadcast Addr
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Instance 0 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 1 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 2 received expected 300 packets
      04050466: ndt_2c Msg: Instance 3 received expected 300 packets
      04050466: ndt_2c Msg: Instance 4 received expected 300 packets
      04050466: ndt_2c Msg: Instance 5 received expected 300 packets
      04050466: ndt_2c Msg: Instance 6 received expected 300 packets
      04050466: ndt_2c Msg: Instance 7 received expected 300 packets
      04050466: ndt_2c Msg: Setting receiving filters
      04050466: ndt_2c Msg: Set filter FILTER_NONE for instance 0
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+ for instance 1
      04050466: ndt_2c Msg: Set filter FILTER_BROADCAST+ for instance 2
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+ for instance 3
      04050466: ndt_2c Msg: Set filter FILTER_PROMISCUOUS+ for instance 4
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_PROMISCUOUS+ for instance 5
      04050466: ndt_2c Msg: Set filter FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      04050466: ndt_2c Msg: Start receiving
      04050466: ndt_2c Msg: Sending 300 packets with size 128 bytes to Any directed Random Addr
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Instance 0 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 1 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 2 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 3 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 4 received expected 300 packets
      04050466: ndt_2c Msg: Instance 5 received expected 300 packets
      04050466: ndt_2c Msg: Instance 6 received expected 300 packets
      04050466: ndt_2c Msg: Instance 7 received expected 300 packets
      04050466: ndt_2c Msg: Setting receiving filters
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+ for instance 0
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+ for instance 1
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+ for instance 2
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+ for instance 3
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      04050466: ndt_2c Msg: Start receiving
      04050466: ndt_2c Msg: Sending 300 packets with size 128 bytes to Any directed Random Addr
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Instance 0 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 1 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 2 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 3 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 4 received expected 300 packets
      04050466: ndt_2c Msg: Instance 5 received expected 300 packets
      04050466: ndt_2c Msg: Instance 6 received expected 300 packets
      04050466: ndt_2c Msg: Instance 7 received expected 300 packets
      04050466: ndt_2c Msg: Setting receiving filters
      04050466: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+ for instance 0
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+ for instance 1
      04050466: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      04050466: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      04050466: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      04050466: ndt_2c Msg: Start receiving
      04050466: ndt_2c Msg: Sending 300 packets with size 128 bytes to Any directed Random Addr
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Instance 0 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 1 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 2 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 3 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 4 received expected 300 packets
      04050466: ndt_2c Msg: Instance 5 received expected 300 packets
      04050466: ndt_2c Msg: Instance 6 received expected 300 packets
      04050466: ndt_2c Msg: Instance 7 received expected 300 packets
      04050466: ndt_2c Msg: Setting receiving filters
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 0
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 1
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      04050466: ndt_2c Msg: Start receiving
      04050466: ndt_2c Msg: Sending 300 packets with size 128 bytes to Any directed Random Addr
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Instance 0 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 1 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 2 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 3 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 4 received expected 300 packets
      04050466: ndt_2c Msg: Instance 5 received expected 300 packets
      04050466: ndt_2c Msg: Instance 6 received expected 300 packets
      04050466: ndt_2c Msg: Instance 7 received expected 300 packets
      04050466: ndt_2c Msg: Setting receiving filters
      04050466: ndt_2c Msg: Set filter FILTER_NONE for instance 0
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+ for instance 1
      04050466: ndt_2c Msg: Set filter FILTER_BROADCAST+ for instance 2
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+ for instance 3
      04050466: ndt_2c Msg: Set filter FILTER_PROMISCUOUS+ for instance 4
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_PROMISCUOUS+ for instance 5
      04050466: ndt_2c Msg: Set filter FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      04050466: ndt_2c Msg: Start receiving
      04050466: ndt_2c Msg: Sending 300 packets with size 128 bytes to Multicast Addr
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Instance 0 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 1 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 2 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 3 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 4 received expected 300 packets
      04050466: ndt_2c Msg: Instance 5 received expected 300 packets
      04050466: ndt_2c Msg: Instance 6 received expected 300 packets
      04050466: ndt_2c Msg: Instance 7 received expected 300 packets
      04050466: ndt_2c Msg: Setting receiving filters
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+ for instance 0
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+ for instance 1
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+ for instance 2
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+ for instance 3
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      04050466: ndt_2c Msg: Start receiving
      04050466: ndt_2c Msg: Sending 300 packets with size 128 bytes to Multicast Addr
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Instance 0 received expected 300 packets
      04050466: ndt_2c Msg: Instance 1 received expected 300 packets
      04050466: ndt_2c Msg: Instance 2 received expected 300 packets
      04050466: ndt_2c Msg: Instance 3 received expected 300 packets
      04050466: ndt_2c Msg: Instance 4 received expected 300 packets
      04050466: ndt_2c Msg: Instance 5 received expected 300 packets
      04050466: ndt_2c Msg: Instance 6 received expected 300 packets
      04050466: ndt_2c Msg: Instance 7 received expected 300 packets
      04050466: ndt_2c Msg: Setting receiving filters
      04050466: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+ for instance 0
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+ for instance 1
      04050466: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      04050466: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      04050466: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      04050466: ndt_2c Msg: Start receiving
      04050466: ndt_2c Msg: Sending 300 packets with size 128 bytes to Multicast Addr
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Instance 0 received expected 300 packets
      04050466: ndt_2c Msg: Instance 1 received expected 300 packets
      04050466: ndt_2c Msg: Instance 2 received expected 300 packets
      04050466: ndt_2c Msg: Instance 3 received expected 300 packets
      04050466: ndt_2c Msg: Instance 4 received expected 300 packets
      04050466: ndt_2c Msg: Instance 5 received expected 300 packets
      04050466: ndt_2c Msg: Instance 6 received expected 300 packets
      04050466: ndt_2c Msg: Instance 7 received expected 300 packets
      04050466: ndt_2c Msg: Setting receiving filters
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 0
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 1
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      04050466: ndt_2c Msg: Start receiving
      04050466: ndt_2c Msg: Sending 300 packets with size 128 bytes to Multicast Addr
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Instance 0 received expected 300 packets
      04050466: ndt_2c Msg: Instance 1 received expected 300 packets
      04050466: ndt_2c Msg: Instance 2 received expected 300 packets
      04050466: ndt_2c Msg: Instance 3 received expected 300 packets
      04050466: ndt_2c Msg: Instance 4 received expected 300 packets
      04050466: ndt_2c Msg: Instance 5 received expected 300 packets
      04050466: ndt_2c Msg: Instance 6 received expected 300 packets
      04050466: ndt_2c Msg: Instance 7 received expected 300 packets
      04050466: ndt_2c Msg: Setting receiving filters
      04050466: ndt_2c Msg: Set filter FILTER_NONE for instance 0
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+ for instance 1
      04050466: ndt_2c Msg: Set filter FILTER_BROADCAST+ for instance 2
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+ for instance 3
      04050466: ndt_2c Msg: Set filter FILTER_PROMISCUOUS+ for instance 4
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_PROMISCUOUS+ for instance 5
      04050466: ndt_2c Msg: Set filter FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      04050466: ndt_2c Msg: Start receiving
      04050466: ndt_2c Msg: Sending 300 packets with size 128 bytes to Bad Multicast Addr
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Instance 0 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 1 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 2 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 3 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 4 received expected 300 packets
      04050466: ndt_2c Msg: Instance 5 received expected 300 packets
      04050466: ndt_2c Msg: Instance 6 received expected 300 packets
      04050466: ndt_2c Msg: Instance 7 received expected 300 packets
      04050466: ndt_2c Msg: Setting receiving filters
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+ for instance 0
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+ for instance 1
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+ for instance 2
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+ for instance 3
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      04050466: ndt_2c Msg: Start receiving
      04050466: ndt_2c Msg: Sending 300 packets with size 128 bytes to Bad Multicast Addr
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Instance 0 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 1 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 2 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 3 properly didn't receive packets
      04050466: ndt_2c Msg: Instance 4 received expected 300 packets
      04050466: ndt_2c Msg: Instance 5 received expected 300 packets
      04050466: ndt_2c Msg: Instance 6 received expected 300 packets
      04050466: ndt_2c Msg: Instance 7 received expected 300 packets
      04050466: ndt_2c Msg: Setting receiving filters
      04050466: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+ for instance 0
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+ for instance 1
      04050466: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      04050466: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      04050466: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      04050466: ndt_2c Msg: Start receiving
      04050466: ndt_2c Msg: Sending 300 packets with size 128 bytes to Bad Multicast Addr
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Instance 0 received expected 300 packets
      04050466: ndt_2c Msg: Instance 1 received expected 300 packets
      04050466: ndt_2c Msg: Instance 2 received expected 300 packets
      04050466: ndt_2c Msg: Instance 3 received expected 300 packets
      04050466: ndt_2c Msg: Instance 4 received expected 300 packets
      04050466: ndt_2c Msg: Instance 5 received expected 300 packets
      04050466: ndt_2c Msg: Instance 6 received expected 300 packets
      04050466: ndt_2c Msg: Instance 7 received expected 300 packets
      04050466: ndt_2c Msg: Setting receiving filters
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 0
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 1
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      04050466: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      04050466: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      04050466: ndt_2c Msg: Start receiving
      04050466: ndt_2c Msg: Sending 300 packets with size 128 bytes to Bad Multicast Addr
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Instance 0 received expected 300 packets
      04050466: ndt_2c Msg: Instance 1 received expected 300 packets
      04050466: ndt_2c Msg: Instance 2 received expected 300 packets
      04050466: ndt_2c Msg: Instance 3 received expected 300 packets
      04050466: ndt_2c Msg: Instance 4 received expected 300 packets
      04050466: ndt_2c Msg: Instance 5 received expected 300 packets
      04050466: ndt_2c Msg: Instance 6 received expected 300 packets
      04050466: ndt_2c Msg: Instance 7 received expected 300 packets
      04050466: ndt_2c Msg: Unbinding adapters
   END TEST: "2c_FilterReceive", PASSED, Time=282.549
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   *** TEST COMPLETED
   ***
   *** Test Name:      2c_FilterReceive
   *** Test ID:        3
   *** Library Path:   \ndt_2c.dll
   *** Command Line:   -t AX88772C_772B1 -s AX88772C_772B2
   *** Kernel Mode:    No
   *** Result:         Passed
   *** Random Seed:    5772
   *** Thread Count:   1
   *** Execution Time: 0:04:42.549
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   
   </TESTCASE RESULT="PASSED">
   <TESTCASE ID=4>
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   *** TEST STARTING
   ***
   *** Test Name:      2c_MulticastReceive
   *** Test ID:        4
   *** Library Path:   \ndt_2c.dll
   *** Command Line:   -t AX88772C_772B1 -s AX88772C_772B2
   *** Kernel Mode:    No
   *** Random Seed:    18887
   *** Thread Count:   0
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "2c_MulticastReceive", Threads=0, Seed=18887
      04050466: ndt_2c Msg: Start 1c_MulticastReceive test
      04050466: ndt_2c Msg: The test adapter is AX88772C_772B1
      04050466: ndt_2c Msg: The support adapter is AX88772C_772B2
      04050466: ndt_2c Msg: Opening adapters
      04050466: ndt_2c Msg: Binding adapters
      04050466: ndt_2c Msg: Get basic adapters info
      04050466: ndt_2c Msg: AX88772C_772B1 driver supports 64 multicast addresses
      04050466: ndt_2c Msg: Add multicast addresses
      04050466: ndt_2c Msg: Set multicast filter
      04050466: ndt_2c Msg: Sending 10 packets on 8 unused multicast addresses
      04050466: ndt_2c Msg: Sent 80 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Properly didn't receive packets
      04050466: ndt_2c Msg: Sending 10 packets on 64 multicast addresses
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Properly received 640 packets
      04050466: ndt_2c Msg: Removing randomly 8 multicast addresses
      04050466: ndt_2c Msg: Sending 10 packets on 16 unused multicast addresses
      04050466: ndt_2c Msg: Sent 160 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Wrn: Improperly received 80 packets
      04050466: ndt_2c Msg: Sending 10 packets on 56 multicast addresses
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Properly received 560 packets
      04050466: ndt_2c Msg: Removing randomly 8 multicast addresses
      04050466: ndt_2c Msg: Sending 10 packets on 24 unused multicast addresses
      04050466: ndt_2c Msg: Sent 240 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Wrn: Improperly received 160 packets
      04050466: ndt_2c Msg: Sending 10 packets on 48 multicast addresses
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Properly received 480 packets
      04050466: ndt_2c Msg: Removing randomly 8 multicast addresses
      04050466: ndt_2c Msg: Sending 10 packets on 32 unused multicast addresses
      04050466: ndt_2c Msg: Sent 320 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Wrn: Improperly received 200 packets
      04050466: ndt_2c Msg: Sending 10 packets on 40 multicast addresses
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Properly received 400 packets
      04050466: ndt_2c Msg: Removing randomly 8 multicast addresses
      04050466: ndt_2c Msg: Sending 10 packets on 40 unused multicast addresses
      04050466: ndt_2c Msg: Sent 400 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Wrn: Improperly received 280 packets
      04050466: ndt_2c Msg: Sending 10 packets on 32 multicast addresses
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Properly received 320 packets
      04050466: ndt_2c Msg: Removing randomly 4 multicast addresses
      04050466: ndt_2c Msg: Sending 10 packets on 44 unused multicast addresses
      04050466: ndt_2c Msg: Sent 440 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Wrn: Improperly received 280 packets
      04050466: ndt_2c Msg: Sending 10 packets on 28 multicast addresses
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Properly received 280 packets
      04050466: ndt_2c Msg: Removing randomly 4 multicast addresses
      04050466: ndt_2c Msg: Sending 10 packets on 48 unused multicast addresses
      04050466: ndt_2c Msg: Sent 480 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Wrn: Improperly received 240 packets
      04050466: ndt_2c Msg: Sending 10 packets on 24 multicast addresses
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Properly received 240 packets
      04050466: ndt_2c Msg: Removing randomly 4 multicast addresses
      04050466: ndt_2c Msg: Sending 10 packets on 52 unused multicast addresses
      04050466: ndt_2c Msg: Sent 520 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Wrn: Improperly received 280 packets
      04050466: ndt_2c Msg: Sending 10 packets on 20 multicast addresses
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Properly received 200 packets
      04050466: ndt_2c Msg: Removing randomly 4 multicast addresses
      04050466: ndt_2c Msg: Sending 10 packets on 56 unused multicast addresses
      04050466: ndt_2c Msg: Sent 560 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Wrn: Improperly received 280 packets
      04050466: ndt_2c Msg: Sending 10 packets on 16 multicast addresses
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Properly received 160 packets
      04050466: ndt_2c Msg: Removing randomly 1 multicast addresses
      04050466: ndt_2c Msg: Sending 10 packets on 57 unused multicast addresses
      04050466: ndt_2c Msg: Sent 570 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Wrn: Improperly received 290 packets
      04050466: ndt_2c Msg: Sending 10 packets on 15 multicast addresses
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Properly received 150 packets
      04050466: ndt_2c Msg: Removing randomly 1 multicast addresses
      04050466: ndt_2c Msg: Sending 10 packets on 58 unused multicast addresses
      04050466: ndt_2c Msg: Sent 580 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Wrn: Improperly received 300 packets
      04050466: ndt_2c Msg: Sending 10 packets on 14 multicast addresses
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Properly received 140 packets
      04050466: ndt_2c Msg: Removing randomly 1 multicast addresses
      04050466: ndt_2c Msg: Sending 10 packets on 59 unused multicast addresses
      04050466: ndt_2c Msg: Sent 590 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Wrn: Improperly received 270 packets
      04050466: ndt_2c Msg: Sending 10 packets on 13 multicast addresses
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Properly received 130 packets
      04050466: ndt_2c Msg: Removing randomly 1 multicast addresses
      04050466: ndt_2c Msg: Sending 10 packets on 60 unused multicast addresses
      04050466: ndt_2c Msg: Sent 600 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Wrn: Improperly received 240 packets
      04050466: ndt_2c Msg: Sending 10 packets on 12 multicast addresses
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Properly received 120 packets
      04050466: ndt_2c Msg: Removing randomly 1 multicast addresses
      04050466: ndt_2c Msg: Sending 10 packets on 61 unused multicast addresses
      04050466: ndt_2c Msg: Sent 610 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Wrn: Improperly received 210 packets
      04050466: ndt_2c Msg: Sending 10 packets on 11 multicast addresses
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Properly received 110 packets
      04050466: ndt_2c Msg: Removing randomly 1 multicast addresses
      04050466: ndt_2c Msg: Sending 10 packets on 62 unused multicast addresses
      04050466: ndt_2c Msg: Sent 620 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Wrn: Improperly received 180 packets
      04050466: ndt_2c Msg: Sending 10 packets on 10 multicast addresses
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Properly received 100 packets
      04050466: ndt_2c Msg: Removing randomly 1 multicast addresses
      04050466: ndt_2c Msg: Sending 10 packets on 63 unused multicast addresses
      04050466: ndt_2c Msg: Sent 630 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Wrn: Improperly received 190 packets
      04050466: ndt_2c Msg: Sending 10 packets on 9 multicast addresses
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Properly received 90 packets
      04050466: ndt_2c Msg: Removing randomly 1 multicast addresses
      04050466: ndt_2c Msg: Sending 10 packets on 64 unused multicast addresses
      04050466: ndt_2c Msg: Sent 640 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Wrn: Improperly received 160 packets
      04050466: ndt_2c Msg: Sending 10 packets on 8 multicast addresses
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Properly received 80 packets
      04050466: ndt_2c Msg: Removing randomly 1 multicast addresses
      04050466: ndt_2c Msg: Sending 10 packets on 65 unused multicast addresses
      04050466: ndt_2c Msg: Sent 650 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Wrn: Improperly received 130 packets
      04050466: ndt_2c Msg: Sending 10 packets on 7 multicast addresses
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Properly received 70 packets
      04050466: ndt_2c Msg: Removing randomly 1 multicast addresses
      04050466: ndt_2c Msg: Sending 10 packets on 66 unused multicast addresses
      04050466: ndt_2c Msg: Sent 660 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Wrn: Improperly received 100 packets
      04050466: ndt_2c Msg: Sending 10 packets on 6 multicast addresses
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Properly received 60 packets
      04050466: ndt_2c Msg: Removing randomly 1 multicast addresses
      04050466: ndt_2c Msg: Sending 10 packets on 67 unused multicast addresses
      04050466: ndt_2c Msg: Sent 670 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Wrn: Improperly received 110 packets
      04050466: ndt_2c Msg: Sending 10 packets on 5 multicast addresses
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Properly received 50 packets
      04050466: ndt_2c Msg: Removing randomly 1 multicast addresses
      04050466: ndt_2c Msg: Sending 10 packets on 68 unused multicast addresses
      04050466: ndt_2c Msg: Sent 680 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Wrn: Improperly received 80 packets
      04050466: ndt_2c Msg: Sending 10 packets on 4 multicast addresses
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Properly received 40 packets
      04050466: ndt_2c Msg: Removing randomly 1 multicast addresses
      04050466: ndt_2c Msg: Sending 10 packets on 69 unused multicast addresses
      04050466: ndt_2c Msg: Sent 690 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Wrn: Improperly received 90 packets
      04050466: ndt_2c Msg: Sending 10 packets on 3 multicast addresses
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Properly received 30 packets
      04050466: ndt_2c Msg: Removing randomly 1 multicast addresses
      04050466: ndt_2c Msg: Sending 10 packets on 70 unused multicast addresses
      04050466: ndt_2c Msg: Sent 700 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Wrn: Improperly received 60 packets
      04050466: ndt_2c Msg: Sending 10 packets on 2 multicast addresses
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Properly received 20 packets
      04050466: ndt_2c Msg: Removing randomly 1 multicast addresses
      04050466: ndt_2c Msg: Sending 10 packets on 71 unused multicast addresses
      04050466: ndt_2c Msg: Sent 710 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Wrn: Improperly received 30 packets
      04050466: ndt_2c Msg: Sending 10 packets on 1 multicast addresses
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Properly received 10 packets
      04050466: ndt_2c Msg: Removing randomly 1 multicast addresses
      04050466: ndt_2c Msg: Sending 10 packets on 72 unused multicast addresses
      04050466: ndt_2c Msg: Sent 720 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Properly didn't receive packets
      04050466: ndt_2c Wrn: WARNING: Adapter AX88772C_772B1 indicates unwanted multicast packets up the stack
      04050466: ndt_2c Wrn: It indicates packets sent to multicast addresses not set in its multicast address list
      04050466: ndt_2c Msg: Closing adapters
   END TEST: "2c_MulticastReceive", PASSED, Time=218.826
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   *** TEST COMPLETED
   ***
   *** Test Name:      2c_MulticastReceive
   *** Test ID:        4
   *** Library Path:   \ndt_2c.dll
   *** Command Line:   -t AX88772C_772B1 -s AX88772C_772B2
   *** Kernel Mode:    No
   *** Result:         Passed
   *** Random Seed:    18887
   *** Thread Count:   1
   *** Execution Time: 0:03:38.826
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   
   </TESTCASE RESULT="PASSED">
   <TESTCASE ID=5>
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   *** TEST STARTING
   ***
   *** Test Name:      2c_StressSend
   *** Test ID:        5
   *** Library Path:   \ndt_2c.dll
   *** Command Line:   -t AX88772C_772B1 -s AX88772C_772B2
   *** Kernel Mode:    No
   *** Random Seed:    28947
   *** Thread Count:   0
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "2c_StressSend", Threads=0, Seed=28947
      04050466: ndt_2c Msg: Start 2c_StressSend test
      04050466: ndt_2c Msg: The test adapter is AX88772C_772B1
      04050466: ndt_2c Msg: The support adapter is AX88772C_772B2
      04050466: ndt_2c Msg: Opening adapters
      04050466: ndt_2c Msg: Binding adapters
      04050466: ndt_2c Msg: Get basic adapters info
      04050466: ndt_2c Msg: Seting direct receive filters
      04050466: ndt_2c Msg: Test Pass #0
      04050466: ndt_2c Msg: Start sending 10000 packets
      04050466: ndt_2c Msg: Sent 10000 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Test: Sent 10000 packets with total size 7738987 bytes in 12689 ms
      04050466: ndt_2c Msg: Test: Recv 10000 packets with total size 523400 bytes in 12689 ms
      04050466: ndt_2c Msg: Support: Recv 10013 packets with total size 7885735 bytes in 12688 ms
      04050466: ndt_2c Msg: Support: Sent 10013 packets with total size 500650 bytes in 12688 ms
      04050466: ndt_2c Msg: Test Pass #1
      04050466: ndt_2c Msg: Start sending 10000 packets
      04050466: ndt_2c Msg: Sent 10000 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Test: Sent 10000 packets with total size 7736540 bytes in 12718 ms
      04050466: ndt_2c Msg: Test: Recv 10000 packets with total size 535450 bytes in 12718 ms
      04050466: ndt_2c Msg: Support: Recv 10005 packets with total size 7879933 bytes in 12722 ms
      04050466: ndt_2c Msg: Support: Sent 10005 packets with total size 500250 bytes in 12722 ms
      04050466: ndt_2c Msg: Test Pass #2
      04050466: ndt_2c Msg: Start sending 10000 packets
      04050466: ndt_2c Msg: Sent 10000 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Test: Sent 10000 packets with total size 7661269 bytes in 12710 ms
      04050466: ndt_2c Msg: Test: Recv 10000 packets with total size 545400 bytes in 12710 ms
      04050466: ndt_2c Msg: Support: Recv 10009 packets with total size 7810301 bytes in 12710 ms
      04050466: ndt_2c Msg: Support: Sent 10009 packets with total size 500450 bytes in 12710 ms
      04050466: ndt_2c Msg: Test Pass #3
      04050466: ndt_2c Msg: Start sending 100 packets
      04050466: ndt_2c Msg: Sent 100 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Test: Sent 100 packets with total size 8650 bytes in 120 ms
      04050466: ndt_2c Msg: Test: Recv 100 packets with total size 5750 bytes in 120 ms
      04050466: ndt_2c Msg: Support: Recv 100 packets with total size 10050 bytes in 120 ms
      04050466: ndt_2c Msg: Support: Sent 100 packets with total size 5000 bytes in 120 ms
      04050466: ndt_2c Msg: Test Pass #4
      04050466: ndt_2c Msg: Start sending 53 packets
      04050466: ndt_2c Msg: Sent 53 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Test: Sent 53 packets with total size 3339 bytes in 60 ms
      04050466: ndt_2c Msg: Test: Recv 53 packets with total size 4131 bytes in 60 ms
      04050466: ndt_2c Msg: Support: Recv 53 packets with total size 4081 bytes in 60 ms
      04050466: ndt_2c Msg: Support: Sent 53 packets with total size 4081 bytes in 60 ms
      04050466: ndt_2c Msg: Test Pass #5
      04050466: ndt_2c Msg: Start sending 10000 packets
      04050466: ndt_2c Msg: Sent 10000 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Test: Sent 10000 packets with total size 1000000 bytes in 12515 ms
      04050466: ndt_2c Msg: Test: Recv 10000 packets with total size 564322 bytes in 12515 ms
      04050466: ndt_2c Msg: Support: Recv 10000 packets with total size 1140000 bytes in 12515 ms
      04050466: ndt_2c Msg: Support: Sent 10000 packets with total size 500000 bytes in 12515 ms
      04050466: ndt_2c Msg: Test Pass #6
      04050466: ndt_2c Msg: Start sending 10000 packets
      04050466: ndt_2c Msg: Sent 10000 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Test: Sent 10000 packets with total size 7677557 bytes in 12685 ms
      04050466: ndt_2c Msg: Test: Recv 10000 packets with total size 574974 bytes in 12685 ms
      04050466: ndt_2c Msg: Support: Recv 10008 packets with total size 7822207 bytes in 12686 ms
      04050466: ndt_2c Msg: Support: Sent 10008 packets with total size 500400 bytes in 12686 ms
      04050466: ndt_2c Msg: Test Pass #7
      04050466: ndt_2c Msg: Start sending 10000 packets
      04050466: ndt_2c Msg: Sent 10000 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Test: Sent 10000 packets with total size 7676969 bytes in 12510 ms
      04050466: ndt_2c Msg: Test: Recv 0 packets with total size 0 bytes in 12510 ms
      04050466: ndt_2c Msg: Support: Recv 10006 packets with total size 7819856 bytes in 12509 ms
      04050466: ndt_2c Msg: Support: Sent 0 packets with total size 0 bytes in 12509 ms
      04050466: ndt_2c Msg: Test Pass #8
      04050466: ndt_2c Msg: Start sending 10000 packets
      04050466: ndt_2c Msg: Sent 10000 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Test: Sent 10000 packets with total size 7701734 bytes in 12792 ms
      04050466: ndt_2c Msg: Test: Recv 10000 packets with total size 7844593 bytes in 12792 ms
      04050466: ndt_2c Msg: Support: Recv 10003 packets with total size 7844593 bytes in 12792 ms
      04050466: ndt_2c Msg: Support: Sent 10003 packets with total size 7844593 bytes in 12792 ms
      04050466: ndt_2c Msg: Test Pass #9
      04050466: ndt_2c Msg: Start sending 10000 packets
      04050466: ndt_2c Msg: Sent 10000 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Test: Sent 10000 packets with total size 600000 bytes in 12511 ms
      04050466: ndt_2c Msg: Test: Recv 10000 packets with total size 740000 bytes in 12511 ms
      04050466: ndt_2c Msg: Support: Recv 10000 packets with total size 740000 bytes in 12511 ms
      04050466: ndt_2c Msg: Support: Sent 10000 packets with total size 740000 bytes in 12511 ms
      04050466: ndt_2c Msg: Unbinding adapters
      04050466: ndt_2c Msg: Closing adapters
   END TEST: "2c_StressSend", PASSED, Time=122.444
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   *** TEST COMPLETED
   ***
   *** Test Name:      2c_StressSend
   *** Test ID:        5
   *** Library Path:   \ndt_2c.dll
   *** Command Line:   -t AX88772C_772B1 -s AX88772C_772B2
   *** Kernel Mode:    No
   *** Result:         Passed
   *** Random Seed:    28947
   *** Thread Count:   1
   *** Execution Time: 0:02:02.444
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   
   </TESTCASE RESULT="PASSED">
   <TESTCASE ID=6>
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   *** TEST STARTING
   ***
   *** Test Name:      2c_StressReceive
   *** Test ID:        6
   *** Library Path:   \ndt_2c.dll
   *** Command Line:   -t AX88772C_772B1 -s AX88772C_772B2
   *** Kernel Mode:    No
   *** Random Seed:    29031
   *** Thread Count:   0
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "2c_StressReceive", Threads=0, Seed=29031
      04050466: ndt_2c Msg: Start 2c_StessReceive test
      04050466: ndt_2c Msg: The test adapter is AX88772C_772B1
      04050466: ndt_2c Msg: The support adapter is AX88772C_772B2
      04050466: ndt_2c Msg: Opening adapters
      04050466: ndt_2c Msg: Binding adapters
      04050466: ndt_2c Msg: Get basic adapters info
      04050466: ndt_2c Msg: Seting direct receive filters
      04050466: ndt_2c Msg: Test Pass #0
      04050466: ndt_2c Msg: Start sending 10000 packets
      04050466: ndt_2c Msg: Sent 10000 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Support: Sent 10000 packets with total size 7710960 bytes in 12683 ms
      04050466: ndt_2c Msg: Support: Recv 10000 packets with total size 509650 bytes in 12683 ms
      04050466: ndt_2c Msg: Test: Recv 10005 packets with total size 7855010 bytes in 12683 ms
      04050466: ndt_2c Msg: Test: Sent 10005 packets with total size 500250 bytes in 12683 ms
      04050466: ndt_2c Msg: Test Pass #1
      04050466: ndt_2c Msg: Start sending 10000 packets
      04050466: ndt_2c Msg: Sent 10000 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Support: Sent 10000 packets with total size 7688114 bytes in 12687 ms
      04050466: ndt_2c Msg: Support: Recv 10000 packets with total size 529350 bytes in 12687 ms
      04050466: ndt_2c Msg: Test: Recv 10009 packets with total size 7834564 bytes in 12687 ms
      04050466: ndt_2c Msg: Test: Sent 10009 packets with total size 500450 bytes in 12687 ms
      04050466: ndt_2c Msg: Test Pass #2
      04050466: ndt_2c Msg: Start sending 10000 packets
      04050466: ndt_2c Msg: Sent 10000 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Support: Sent 10000 packets with total size 7662622 bytes in 12693 ms
      04050466: ndt_2c Msg: Support: Recv 10000 packets with total size 550950 bytes in 12693 ms
      04050466: ndt_2c Msg: Test: Recv 10010 packets with total size 7810132 bytes in 12694 ms
      04050466: ndt_2c Msg: Test: Sent 10010 packets with total size 500500 bytes in 12694 ms
      04050466: ndt_2c Msg: Test Pass #3
      04050466: ndt_2c Msg: Start sending 100 packets
      04050466: ndt_2c Msg: Sent 100 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Support: Sent 100 packets with total size 8650 bytes in 120 ms
      04050466: ndt_2c Msg: Support: Recv 100 packets with total size 5400 bytes in 120 ms
      04050466: ndt_2c Msg: Test: Recv 100 packets with total size 10050 bytes in 120 ms
      04050466: ndt_2c Msg: Test: Sent 100 packets with total size 5000 bytes in 120 ms
      04050466: ndt_2c Msg: Test Pass #4
      04050466: ndt_2c Msg: Start sending 53 packets
      04050466: ndt_2c Msg: Sent 53 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Support: Sent 53 packets with total size 3339 bytes in 60 ms
      04050466: ndt_2c Msg: Support: Recv 53 packets with total size 4281 bytes in 60 ms
      04050466: ndt_2c Msg: Test: Recv 53 packets with total size 4081 bytes in 60 ms
      04050466: ndt_2c Msg: Test: Sent 53 packets with total size 4081 bytes in 60 ms
      04050466: ndt_2c Msg: Test Pass #5
      04050466: ndt_2c Msg: Start sending 10000 packets
      04050466: ndt_2c Msg: Sent 10000 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Support: Sent 10000 packets with total size 1000000 bytes in 12514 ms
      04050466: ndt_2c Msg: Support: Recv 10000 packets with total size 548722 bytes in 12514 ms
      04050466: ndt_2c Msg: Test: Recv 10000 packets with total size 1140000 bytes in 12515 ms
      04050466: ndt_2c Msg: Test: Sent 10000 packets with total size 500000 bytes in 12515 ms
      04050466: ndt_2c Msg: Test Pass #6
      04050466: ndt_2c Msg: Start sending 10000 packets
      04050466: ndt_2c Msg: Sent 10000 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Support: Sent 10000 packets with total size 7746623 bytes in 12720 ms
      04050466: ndt_2c Msg: Support: Recv 10000 packets with total size 567172 bytes in 12720 ms
      04050466: ndt_2c Msg: Test: Recv 10013 packets with total size 7895779 bytes in 12720 ms
      04050466: ndt_2c Msg: Test: Sent 10013 packets with total size 500650 bytes in 12720 ms
      04050466: ndt_2c Msg: Test Pass #7
      04050466: ndt_2c Msg: Start sending 10000 packets
      04050466: ndt_2c Msg: Sent 10000 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Support: Sent 10000 packets with total size 7680119 bytes in 12511 ms
      04050466: ndt_2c Msg: Support: Recv 0 packets with total size 0 bytes in 12511 ms
      04050466: ndt_2c Msg: Test: Recv 10002 packets with total size 7821143 bytes in 12511 ms
      04050466: ndt_2c Msg: Test: Sent 0 packets with total size 0 bytes in 12511 ms
      04050466: ndt_2c Msg: Test Pass #8
      04050466: ndt_2c Msg: Start sending 10000 packets
      04050466: ndt_2c Msg: Sent 10000 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Support: Sent 10000 packets with total size 7747917 bytes in 12803 ms
      04050466: ndt_2c Msg: Support: Recv 10000 packets with total size 7887917 bytes in 12803 ms
      04050466: ndt_2c Msg: Test: Recv 10000 packets with total size 7887917 bytes in 12804 ms
      04050466: ndt_2c Msg: Test: Sent 10000 packets with total size 7887917 bytes in 12804 ms
      04050466: ndt_2c Msg: Test Pass #9
      04050466: ndt_2c Msg: Start sending 10000 packets
      04050466: ndt_2c Msg: Sent 10000 packets
      04050466: ndt_2c Msg: Stop receiving and checking results
      04050466: ndt_2c Msg: Support: Sent 10000 packets with total size 600000 bytes in 12511 ms
      04050466: ndt_2c Msg: Support: Recv 10000 packets with total size 740000 bytes in 12511 ms
      04050466: ndt_2c Msg: Test: Recv 10000 packets with total size 740000 bytes in 12511 ms
      04050466: ndt_2c Msg: Test: Sent 10000 packets with total size 740000 bytes in 12511 ms
      04050466: ndt_2c Msg: Unbinding adapters
      04050466: ndt_2c Msg: Closing adapters
   END TEST: "2c_StressReceive", PASSED, Time=122.433
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   *** TEST COMPLETED
   ***
   *** Test Name:      2c_StressReceive
   *** Test ID:        6
   *** Library Path:   \ndt_2c.dll
   *** Command Line:   -t AX88772C_772B1 -s AX88772C_772B2
   *** Kernel Mode:    No
   *** Result:         Passed
   *** Random Seed:    29031
   *** Thread Count:   1
   *** Execution Time: 0:02:02.433
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   
   </TESTCASE RESULT="PASSED">
END GROUP: ndt_2c.dll
*** ==================================================================
*** MEMORY INFO
***
*** Memory Total:   746,651,648 bytes
*** Memory Used:     27,013,120 bytes
*** Memory Free:    719,638,528 bytes
***
*** Kernel Used:        761,856 bytes
*** Water Mark:         175,475 pages
***
*** Store Total:    133,971,968 bytes
*** Store Used:       1,314,816 bytes
*** Store Free:     132,657,152 bytes
*** ==================================================================

*** ==================================================================
*** SUITE SUMMARY
***
*** Passed:          6
*** Failed:          0
*** Skipped:         0
*** Aborted:         0
*** -------- ---------
*** Total:           6
***
*** Cumulative Test Execution Time: 0:18:47.116
*** Total Tux Suite Execution Time: 0:18:49.170
*** CPU Idle Time:                  0:18:32.492
*** ==================================================================
</TESTGROUP>
@@@@@@0

