05be0212: ndt_2c Msg: Querying if test miniport is wireless
05be0212: ndt_2c Msg: Miniport AX88179_178A1 is ** NOT Wireless-LAN **
<TESTGROUP>

*** ==================================================================
*** SUITE INFORMATION
***
*** Suite Name:        N/A (built on the fly)
*** Suite Description: N/A
*** Number of Tests:   6
*** ==================================================================

*** ==================================================================
*** SYSTEM INFORMATION
***
*** Date and Time:          10/25/2013 11:12 AM (Friday)
***
*** Device Name:            CEPC32108
***
*** OS Version:             7.00
*** Build Number:           2806
*** Platform ID:            3 "Windows CE"
*** Version String:         ""
***
*** Processor Type:         0x000002AE (686) "Intel Pentium II"
*** Processor Architecture: 0x0000     (0) "Intel"
*** Page Size:              0x00001000 (4,096)
*** Minimum App Address:    0x00010000 (65,536)
*** Maximum App Address:    0x7FFFFFFF (2,147,483,647)
*** Active Processor Mask:  0x00000001
*** Number Of Processors:   1
*** Allocation Granularity: 0x00010000 (65,536)
*** Processor Level:        0x000F     (15)
*** Processor Revision:     0x000D     (13)
*** ==================================================================

*** ==================================================================
*** MEMORY INFO
***
*** Memory Total:   746,651,648 bytes
*** Memory Used:     25,890,816 bytes
*** Memory Free:    720,760,832 bytes
***
*** Kernel Used:        749,568 bytes
*** Water Mark:         175,583 pages
***
*** Store Total:    133,971,968 bytes
*** Store Used:       1,241,088 bytes
*** Store Free:     132,730,880 bytes
*** ==================================================================

BEGIN GROUP: ndt_2c.dll
   <TESTCASE ID=1>
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   *** TEST STARTING
   ***
   *** Test Name:      2c_SendPackets
   *** Test ID:        1
   *** Library Path:   \ndt_2c.dll
   *** Command Line:   -t AX88179_178A1 -s AX88179_178A2
   *** Kernel Mode:    No
   *** Random Seed:    27225
   *** Thread Count:   0
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "2c_SendPackets", Threads=0, Seed=27225
      05be0212: ndt_2c Msg: Start 2c_SendPackets test
      05be0212: ndt_2c Msg: The test adapter is AX88179_178A1
      05be0212: ndt_2c Msg: The support adapter is AX88179_178A2
      05be0212: ndt_2c Msg: Setting conversation id to 2004587627
      05be0212: ndt_2c Msg: Opening adapters
      05be0212: ndt_2c Msg: Binding adapters
      05be0212: ndt_2c Msg: Get basic adapters info
      05be0212: ndt_2c Msg: Set adapter filters
      05be0212: ndt_2c Msg: Sending 300 packets with size 64 bytes to 1 address
      05be0212: ndt_2c Msg: Sent 300 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Received 300 packets
      05be0212: ndt_2c Msg: Sending 300 packets with size 783 bytes to 1 address
      05be0212: ndt_2c Msg: Sent 300 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Received 300 packets
      05be0212: ndt_2c Msg: Sending 300 packets with size 1500 bytes to 1 address
      05be0212: ndt_2c Msg: Sent 300 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Received 300 packets
      05be0212: ndt_2c Msg: Sending 600 packets with size 64 bytes to 1 address
      05be0212: ndt_2c Msg: Sent 600 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Received 600 packets
      05be0212: ndt_2c Msg: Sending 600 packets with size 783 bytes to 1 address
      05be0212: ndt_2c Msg: Sent 600 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Received 600 packets
      05be0212: ndt_2c Msg: Sending 600 packets with size 1500 bytes to 1 address
      05be0212: ndt_2c Msg: Sent 600 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Received 600 packets
      05be0212: ndt_2c Msg: Sending 900 packets with size 64 bytes to 1 address
      05be0212: ndt_2c Msg: Sent 900 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Received 900 packets
      05be0212: ndt_2c Msg: Sending 900 packets with size 783 bytes to 1 address
      05be0212: ndt_2c Msg: Sent 900 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Received 900 packets
      05be0212: ndt_2c Msg: Sending 900 packets with size 1500 bytes to 1 address
      05be0212: ndt_2c Msg: Sent 900 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Received 900 packets
      05be0212: ndt_2c Msg: Sending 1200 packets with size 64 bytes to 1 address
      05be0212: ndt_2c Msg: Sent 1200 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Received 1200 packets
      05be0212: ndt_2c Msg: Sending 1200 packets with size 783 bytes to 1 address
      05be0212: ndt_2c Msg: Sent 1200 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Received 1200 packets
      05be0212: ndt_2c Msg: Sending 1200 packets with size 1500 bytes to 1 address
      05be0212: ndt_2c Msg: Sent 1200 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Received 1200 packets
      05be0212: ndt_2c Msg: Sending 1500 packets with size 64 bytes to 1 address
      05be0212: ndt_2c Msg: Sent 1500 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Received 1500 packets
      05be0212: ndt_2c Msg: Sending 1500 packets with size 783 bytes to 1 address
      05be0212: ndt_2c Msg: Sent 1500 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Received 1500 packets
      05be0212: ndt_2c Msg: Sending 1500 packets with size 1500 bytes to 1 address
      05be0212: ndt_2c Msg: Sent 1500 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Received 1500 packets
      05be0212: ndt_2c Msg: Sending 1800 packets with size 64 bytes to 1 address
      05be0212: ndt_2c Msg: Sent 1800 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Received 1800 packets
      05be0212: ndt_2c Msg: Sending 1800 packets with size 783 bytes to 1 address
      05be0212: ndt_2c Msg: Sent 1800 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Received 1800 packets
      05be0212: ndt_2c Msg: Sending 1800 packets with size 1500 bytes to 1 address
      05be0212: ndt_2c Msg: Sent 1800 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Received 1800 packets
      05be0212: ndt_2c Msg: Sending 2100 packets with size 64 bytes to 1 address
      05be0212: ndt_2c Msg: Sent 2100 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Received 2100 packets
      05be0212: ndt_2c Msg: Sending 2100 packets with size 783 bytes to 1 address
      05be0212: ndt_2c Msg: Sent 2100 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Received 2100 packets
      05be0212: ndt_2c Msg: Sending 2100 packets with size 1500 bytes to 1 address
      05be0212: ndt_2c Msg: Sent 2100 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Received 2100 packets
      05be0212: ndt_2c Msg: Sending 2400 packets with size 64 bytes to 1 address
      05be0212: ndt_2c Msg: Sent 2400 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Received 2400 packets
      05be0212: ndt_2c Msg: Sending 2400 packets with size 783 bytes to 1 address
      05be0212: ndt_2c Msg: Sent 2400 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Received 2400 packets
      05be0212: ndt_2c Msg: Sending 2400 packets with size 1500 bytes to 1 address
      05be0212: ndt_2c Msg: Sent 2400 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Received 2400 packets
      05be0212: ndt_2c Msg: Unbinding adapters
   END TEST: "2c_SendPackets", PASSED, Time=338.455
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   *** TEST COMPLETED
   ***
   *** Test Name:      2c_SendPackets
   *** Test ID:        1
   *** Library Path:   \ndt_2c.dll
   *** Command Line:   -t AX88179_178A1 -s AX88179_178A2
   *** Kernel Mode:    No
   *** Result:         Passed
   *** Random Seed:    27225
   *** Thread Count:   1
   *** Execution Time: 0:05:38.455
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   
   </TESTCASE RESULT="PASSED">
   <TESTCASE ID=2>
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   *** TEST STARTING
   ***
   *** Test Name:      2c_ReceivePackets
   *** Test ID:        2
   *** Library Path:   \ndt_2c.dll
   *** Command Line:   -t AX88179_178A1 -s AX88179_178A2
   *** Kernel Mode:    No
   *** Random Seed:    23408
   *** Thread Count:   0
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "2c_ReceivePackets", Threads=0, Seed=23408
      05be0212: ndt_2c Msg: Start 2c_ReceivePackets test
      05be0212: ndt_2c Msg: The test adapter is AX88179_178A1
      05be0212: ndt_2c Msg: The support adapter is AX88179_178A2
      05be0212: ndt_2c Msg: Opening adapters
      05be0212: ndt_2c Msg: Binding adapters
      05be0212: ndt_2c Msg: Get basic adapters info
      05be0212: ndt_2c Msg: Set adapter filters
      05be0212: ndt_2c Msg: Sending 2400 packets with size 64 bytes to 1 address
      05be0212: ndt_2c Msg: Sent 2400 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Received 2400 packets
      05be0212: ndt_2c Msg: Sending 2400 packets with size 783 bytes to 1 address
      05be0212: ndt_2c Msg: Sent 2400 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Received 2400 packets
      05be0212: ndt_2c Msg: Sending 2400 packets with size 1500 bytes to 1 address
      05be0212: ndt_2c Msg: Sent 2400 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Received 2400 packets
      05be0212: ndt_2c Msg: Unbinding adapters
   END TEST: "2c_ReceivePackets", PASSED, Time=42.312
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   *** TEST COMPLETED
   ***
   *** Test Name:      2c_ReceivePackets
   *** Test ID:        2
   *** Library Path:   \ndt_2c.dll
   *** Command Line:   -t AX88179_178A1 -s AX88179_178A2
   *** Kernel Mode:    No
   *** Result:         Passed
   *** Random Seed:    23408
   *** Thread Count:   1
   *** Execution Time: 0:00:42.312
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   
   </TESTCASE RESULT="PASSED">
   <TESTCASE ID=3>
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   *** TEST STARTING
   ***
   *** Test Name:      2c_FilterReceive
   *** Test ID:        3
   *** Library Path:   \ndt_2c.dll
   *** Command Line:   -t AX88179_178A1 -s AX88179_178A2
   *** Kernel Mode:    No
   *** Random Seed:    10943
   *** Thread Count:   0
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "2c_FilterReceive", Threads=0, Seed=10943
      05be0212: ndt_2c Msg: Start 2c_FilterReceive test
      05be0212: ndt_2c Msg: The test adapter is AX88179_178A1
      05be0212: ndt_2c Msg: The support adapter is AX88179_178A2
      05be0212: ndt_2c Msg: Opening adapters
      05be0212: ndt_2c Msg: Binding adapters
      05be0212: ndt_2c Msg: Get basic adapters info
      05be0212: ndt_2c Msg: Possible filter settings:
      05be0212: ndt_2c Msg:   - Directed
      05be0212: ndt_2c Msg:   - Broadcast
      05be0212: ndt_2c Msg:   - Promiscuous
      05be0212: ndt_2c Msg:   - Multicast
      05be0212: ndt_2c Msg:   - All Multicast
      05be0212: ndt_2c Msg: Setting receiving filters
      05be0212: ndt_2c Msg: Set filter FILTER_NONE for instance 0
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+ for instance 1
      05be0212: ndt_2c Msg: Set filter FILTER_BROADCAST+ for instance 2
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+ for instance 3
      05be0212: ndt_2c Msg: Set filter FILTER_PROMISCUOUS+ for instance 4
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_PROMISCUOUS+ for instance 5
      05be0212: ndt_2c Msg: Set filter FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      05be0212: ndt_2c Msg: Start receiving
      05be0212: ndt_2c Msg: Sending 300 packets with size 128 bytes to Test NIC's directed Addr
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Instance 0 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 1 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 2 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 3 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 4 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 5 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 6 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 7 received expected 300 packets
      05be0212: ndt_2c Msg: Setting receiving filters
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+ for instance 0
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+ for instance 1
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+ for instance 2
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+ for instance 3
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      05be0212: ndt_2c Msg: Start receiving
      05be0212: ndt_2c Msg: Sending 300 packets with size 128 bytes to Test NIC's directed Addr
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Instance 0 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 1 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 2 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 3 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 4 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 5 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 6 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 7 received expected 300 packets
      05be0212: ndt_2c Msg: Setting receiving filters
      05be0212: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+ for instance 0
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+ for instance 1
      05be0212: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      05be0212: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      05be0212: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      05be0212: ndt_2c Msg: Start receiving
      05be0212: ndt_2c Msg: Sending 300 packets with size 128 bytes to Test NIC's directed Addr
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Instance 0 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 1 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 2 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 3 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 4 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 5 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 6 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 7 received expected 300 packets
      05be0212: ndt_2c Msg: Setting receiving filters
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 0
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 1
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      05be0212: ndt_2c Msg: Start receiving
      05be0212: ndt_2c Msg: Sending 300 packets with size 128 bytes to Test NIC's directed Addr
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Instance 0 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 1 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 2 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 3 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 4 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 5 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 6 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 7 received expected 300 packets
      05be0212: ndt_2c Msg: Setting receiving filters
      05be0212: ndt_2c Msg: Set filter FILTER_NONE for instance 0
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+ for instance 1
      05be0212: ndt_2c Msg: Set filter FILTER_BROADCAST+ for instance 2
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+ for instance 3
      05be0212: ndt_2c Msg: Set filter FILTER_PROMISCUOUS+ for instance 4
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_PROMISCUOUS+ for instance 5
      05be0212: ndt_2c Msg: Set filter FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      05be0212: ndt_2c Msg: Start receiving
      05be0212: ndt_2c Msg: Sending 300 packets with size 128 bytes to Broadcast Addr
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Instance 0 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 1 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 2 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 3 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 4 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 5 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 6 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 7 received expected 300 packets
      05be0212: ndt_2c Msg: Setting receiving filters
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+ for instance 0
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+ for instance 1
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+ for instance 2
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+ for instance 3
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      05be0212: ndt_2c Msg: Start receiving
      05be0212: ndt_2c Msg: Sending 300 packets with size 128 bytes to Broadcast Addr
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Instance 0 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 1 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 2 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 3 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 4 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 5 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 6 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 7 received expected 300 packets
      05be0212: ndt_2c Msg: Setting receiving filters
      05be0212: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+ for instance 0
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+ for instance 1
      05be0212: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      05be0212: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      05be0212: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      05be0212: ndt_2c Msg: Start receiving
      05be0212: ndt_2c Msg: Sending 300 packets with size 128 bytes to Broadcast Addr
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Instance 0 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 1 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 2 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 3 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 4 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 5 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 6 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 7 received expected 300 packets
      05be0212: ndt_2c Msg: Setting receiving filters
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 0
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 1
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      05be0212: ndt_2c Msg: Start receiving
      05be0212: ndt_2c Msg: Sending 300 packets with size 128 bytes to Broadcast Addr
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Instance 0 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 1 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 2 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 3 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 4 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 5 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 6 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 7 received expected 300 packets
      05be0212: ndt_2c Msg: Setting receiving filters
      05be0212: ndt_2c Msg: Set filter FILTER_NONE for instance 0
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+ for instance 1
      05be0212: ndt_2c Msg: Set filter FILTER_BROADCAST+ for instance 2
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+ for instance 3
      05be0212: ndt_2c Msg: Set filter FILTER_PROMISCUOUS+ for instance 4
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_PROMISCUOUS+ for instance 5
      05be0212: ndt_2c Msg: Set filter FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      05be0212: ndt_2c Msg: Start receiving
      05be0212: ndt_2c Msg: Sending 300 packets with size 128 bytes to Any directed Random Addr
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Instance 0 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 1 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 2 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 3 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 4 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 5 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 6 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 7 received expected 300 packets
      05be0212: ndt_2c Msg: Setting receiving filters
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+ for instance 0
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+ for instance 1
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+ for instance 2
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+ for instance 3
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      05be0212: ndt_2c Msg: Start receiving
      05be0212: ndt_2c Msg: Sending 300 packets with size 128 bytes to Any directed Random Addr
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Instance 0 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 1 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 2 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 3 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 4 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 5 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 6 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 7 received expected 300 packets
      05be0212: ndt_2c Msg: Setting receiving filters
      05be0212: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+ for instance 0
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+ for instance 1
      05be0212: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      05be0212: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      05be0212: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      05be0212: ndt_2c Msg: Start receiving
      05be0212: ndt_2c Msg: Sending 300 packets with size 128 bytes to Any directed Random Addr
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Instance 0 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 1 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 2 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 3 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 4 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 5 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 6 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 7 received expected 300 packets
      05be0212: ndt_2c Msg: Setting receiving filters
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 0
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 1
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      05be0212: ndt_2c Msg: Start receiving
      05be0212: ndt_2c Msg: Sending 300 packets with size 128 bytes to Any directed Random Addr
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Instance 0 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 1 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 2 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 3 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 4 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 5 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 6 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 7 received expected 300 packets
      05be0212: ndt_2c Msg: Setting receiving filters
      05be0212: ndt_2c Msg: Set filter FILTER_NONE for instance 0
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+ for instance 1
      05be0212: ndt_2c Msg: Set filter FILTER_BROADCAST+ for instance 2
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+ for instance 3
      05be0212: ndt_2c Msg: Set filter FILTER_PROMISCUOUS+ for instance 4
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_PROMISCUOUS+ for instance 5
      05be0212: ndt_2c Msg: Set filter FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      05be0212: ndt_2c Msg: Start receiving
      05be0212: ndt_2c Msg: Sending 300 packets with size 128 bytes to Multicast Addr
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Instance 0 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 1 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 2 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 3 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 4 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 5 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 6 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 7 received expected 300 packets
      05be0212: ndt_2c Msg: Setting receiving filters
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+ for instance 0
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+ for instance 1
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+ for instance 2
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+ for instance 3
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      05be0212: ndt_2c Msg: Start receiving
      05be0212: ndt_2c Msg: Sending 300 packets with size 128 bytes to Multicast Addr
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Instance 0 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 1 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 2 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 3 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 4 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 5 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 6 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 7 received expected 300 packets
      05be0212: ndt_2c Msg: Setting receiving filters
      05be0212: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+ for instance 0
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+ for instance 1
      05be0212: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      05be0212: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      05be0212: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      05be0212: ndt_2c Msg: Start receiving
      05be0212: ndt_2c Msg: Sending 300 packets with size 128 bytes to Multicast Addr
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Instance 0 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 1 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 2 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 3 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 4 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 5 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 6 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 7 received expected 300 packets
      05be0212: ndt_2c Msg: Setting receiving filters
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 0
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 1
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      05be0212: ndt_2c Msg: Start receiving
      05be0212: ndt_2c Msg: Sending 300 packets with size 128 bytes to Multicast Addr
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Instance 0 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 1 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 2 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 3 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 4 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 5 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 6 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 7 received expected 300 packets
      05be0212: ndt_2c Msg: Setting receiving filters
      05be0212: ndt_2c Msg: Set filter FILTER_NONE for instance 0
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+ for instance 1
      05be0212: ndt_2c Msg: Set filter FILTER_BROADCAST+ for instance 2
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+ for instance 3
      05be0212: ndt_2c Msg: Set filter FILTER_PROMISCUOUS+ for instance 4
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_PROMISCUOUS+ for instance 5
      05be0212: ndt_2c Msg: Set filter FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      05be0212: ndt_2c Msg: Start receiving
      05be0212: ndt_2c Msg: Sending 300 packets with size 128 bytes to Bad Multicast Addr
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Instance 0 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 1 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 2 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 3 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 4 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 5 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 6 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 7 received expected 300 packets
      05be0212: ndt_2c Msg: Setting receiving filters
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+ for instance 0
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+ for instance 1
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+ for instance 2
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+ for instance 3
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      05be0212: ndt_2c Msg: Start receiving
      05be0212: ndt_2c Msg: Sending 300 packets with size 128 bytes to Bad Multicast Addr
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Instance 0 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 1 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 2 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 3 properly didn't receive packets
      05be0212: ndt_2c Msg: Instance 4 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 5 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 6 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 7 received expected 300 packets
      05be0212: ndt_2c Msg: Setting receiving filters
      05be0212: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+ for instance 0
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+ for instance 1
      05be0212: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      05be0212: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      05be0212: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      05be0212: ndt_2c Msg: Start receiving
      05be0212: ndt_2c Msg: Sending 300 packets with size 128 bytes to Bad Multicast Addr
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Instance 0 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 1 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 2 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 3 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 4 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 5 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 6 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 7 received expected 300 packets
      05be0212: ndt_2c Msg: Setting receiving filters
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 0
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 1
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      05be0212: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      05be0212: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      05be0212: ndt_2c Msg: Start receiving
      05be0212: ndt_2c Msg: Sending 300 packets with size 128 bytes to Bad Multicast Addr
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Instance 0 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 1 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 2 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 3 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 4 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 5 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 6 received expected 300 packets
      05be0212: ndt_2c Msg: Instance 7 received expected 300 packets
      05be0212: ndt_2c Msg: Unbinding adapters
   END TEST: "2c_FilterReceive", PASSED, Time=283.014
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   *** TEST COMPLETED
   ***
   *** Test Name:      2c_FilterReceive
   *** Test ID:        3
   *** Library Path:   \ndt_2c.dll
   *** Command Line:   -t AX88179_178A1 -s AX88179_178A2
   *** Kernel Mode:    No
   *** Result:         Passed
   *** Random Seed:    10943
   *** Thread Count:   1
   *** Execution Time: 0:04:43.014
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   
   </TESTCASE RESULT="PASSED">
   <TESTCASE ID=4>
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   *** TEST STARTING
   ***
   *** Test Name:      2c_MulticastReceive
   *** Test ID:        4
   *** Library Path:   \ndt_2c.dll
   *** Command Line:   -t AX88179_178A1 -s AX88179_178A2
   *** Kernel Mode:    No
   *** Random Seed:    3005
   *** Thread Count:   0
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "2c_MulticastReceive", Threads=0, Seed=3005
      05be0212: ndt_2c Msg: Start 1c_MulticastReceive test
      05be0212: ndt_2c Msg: The test adapter is AX88179_178A1
      05be0212: ndt_2c Msg: The support adapter is AX88179_178A2
      05be0212: ndt_2c Msg: Opening adapters
      05be0212: ndt_2c Msg: Binding adapters
      05be0212: ndt_2c Msg: Get basic adapters info
      05be0212: ndt_2c Msg: AX88179_178A1 driver supports 64 multicast addresses
      05be0212: ndt_2c Msg: Add multicast addresses
      05be0212: ndt_2c Msg: Set multicast filter
      05be0212: ndt_2c Msg: Sending 10 packets on 8 unused multicast addresses
      05be0212: ndt_2c Msg: Sent 80 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly didn't receive packets
      05be0212: ndt_2c Msg: Sending 10 packets on 64 multicast addresses
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly received 640 packets
      05be0212: ndt_2c Msg: Removing randomly 8 multicast addresses
      05be0212: ndt_2c Msg: Sending 10 packets on 16 unused multicast addresses
      05be0212: ndt_2c Msg: Sent 160 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly didn't receive packets
      05be0212: ndt_2c Msg: Sending 10 packets on 56 multicast addresses
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly received 560 packets
      05be0212: ndt_2c Msg: Removing randomly 8 multicast addresses
      05be0212: ndt_2c Msg: Sending 10 packets on 24 unused multicast addresses
      05be0212: ndt_2c Msg: Sent 240 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly didn't receive packets
      05be0212: ndt_2c Msg: Sending 10 packets on 48 multicast addresses
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly received 480 packets
      05be0212: ndt_2c Msg: Removing randomly 8 multicast addresses
      05be0212: ndt_2c Msg: Sending 10 packets on 32 unused multicast addresses
      05be0212: ndt_2c Msg: Sent 320 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly didn't receive packets
      05be0212: ndt_2c Msg: Sending 10 packets on 40 multicast addresses
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly received 400 packets
      05be0212: ndt_2c Msg: Removing randomly 8 multicast addresses
      05be0212: ndt_2c Msg: Sending 10 packets on 40 unused multicast addresses
      05be0212: ndt_2c Msg: Sent 400 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly didn't receive packets
      05be0212: ndt_2c Msg: Sending 10 packets on 32 multicast addresses
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly received 320 packets
      05be0212: ndt_2c Msg: Removing randomly 4 multicast addresses
      05be0212: ndt_2c Msg: Sending 10 packets on 44 unused multicast addresses
      05be0212: ndt_2c Msg: Sent 440 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly didn't receive packets
      05be0212: ndt_2c Msg: Sending 10 packets on 28 multicast addresses
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly received 280 packets
      05be0212: ndt_2c Msg: Removing randomly 4 multicast addresses
      05be0212: ndt_2c Msg: Sending 10 packets on 48 unused multicast addresses
      05be0212: ndt_2c Msg: Sent 480 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly didn't receive packets
      05be0212: ndt_2c Msg: Sending 10 packets on 24 multicast addresses
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly received 240 packets
      05be0212: ndt_2c Msg: Removing randomly 4 multicast addresses
      05be0212: ndt_2c Msg: Sending 10 packets on 52 unused multicast addresses
      05be0212: ndt_2c Msg: Sent 520 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly didn't receive packets
      05be0212: ndt_2c Msg: Sending 10 packets on 20 multicast addresses
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly received 200 packets
      05be0212: ndt_2c Msg: Removing randomly 4 multicast addresses
      05be0212: ndt_2c Msg: Sending 10 packets on 56 unused multicast addresses
      05be0212: ndt_2c Msg: Sent 560 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly didn't receive packets
      05be0212: ndt_2c Msg: Sending 10 packets on 16 multicast addresses
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly received 160 packets
      05be0212: ndt_2c Msg: Removing randomly 1 multicast addresses
      05be0212: ndt_2c Msg: Sending 10 packets on 57 unused multicast addresses
      05be0212: ndt_2c Msg: Sent 570 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly didn't receive packets
      05be0212: ndt_2c Msg: Sending 10 packets on 15 multicast addresses
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly received 150 packets
      05be0212: ndt_2c Msg: Removing randomly 1 multicast addresses
      05be0212: ndt_2c Msg: Sending 10 packets on 58 unused multicast addresses
      05be0212: ndt_2c Msg: Sent 580 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly didn't receive packets
      05be0212: ndt_2c Msg: Sending 10 packets on 14 multicast addresses
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly received 140 packets
      05be0212: ndt_2c Msg: Removing randomly 1 multicast addresses
      05be0212: ndt_2c Msg: Sending 10 packets on 59 unused multicast addresses
      05be0212: ndt_2c Msg: Sent 590 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly didn't receive packets
      05be0212: ndt_2c Msg: Sending 10 packets on 13 multicast addresses
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly received 130 packets
      05be0212: ndt_2c Msg: Removing randomly 1 multicast addresses
      05be0212: ndt_2c Msg: Sending 10 packets on 60 unused multicast addresses
      05be0212: ndt_2c Msg: Sent 600 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly didn't receive packets
      05be0212: ndt_2c Msg: Sending 10 packets on 12 multicast addresses
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly received 120 packets
      05be0212: ndt_2c Msg: Removing randomly 1 multicast addresses
      05be0212: ndt_2c Msg: Sending 10 packets on 61 unused multicast addresses
      05be0212: ndt_2c Msg: Sent 610 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly didn't receive packets
      05be0212: ndt_2c Msg: Sending 10 packets on 11 multicast addresses
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly received 110 packets
      05be0212: ndt_2c Msg: Removing randomly 1 multicast addresses
      05be0212: ndt_2c Msg: Sending 10 packets on 62 unused multicast addresses
      05be0212: ndt_2c Msg: Sent 620 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly didn't receive packets
      05be0212: ndt_2c Msg: Sending 10 packets on 10 multicast addresses
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly received 100 packets
      05be0212: ndt_2c Msg: Removing randomly 1 multicast addresses
      05be0212: ndt_2c Msg: Sending 10 packets on 63 unused multicast addresses
      05be0212: ndt_2c Msg: Sent 630 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly didn't receive packets
      05be0212: ndt_2c Msg: Sending 10 packets on 9 multicast addresses
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly received 90 packets
      05be0212: ndt_2c Msg: Removing randomly 1 multicast addresses
      05be0212: ndt_2c Msg: Sending 10 packets on 64 unused multicast addresses
      05be0212: ndt_2c Msg: Sent 640 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly didn't receive packets
      05be0212: ndt_2c Msg: Sending 10 packets on 8 multicast addresses
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly received 80 packets
      05be0212: ndt_2c Msg: Removing randomly 1 multicast addresses
      05be0212: ndt_2c Msg: Sending 10 packets on 65 unused multicast addresses
      05be0212: ndt_2c Msg: Sent 650 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly didn't receive packets
      05be0212: ndt_2c Msg: Sending 10 packets on 7 multicast addresses
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly received 70 packets
      05be0212: ndt_2c Msg: Removing randomly 1 multicast addresses
      05be0212: ndt_2c Msg: Sending 10 packets on 66 unused multicast addresses
      05be0212: ndt_2c Msg: Sent 660 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly didn't receive packets
      05be0212: ndt_2c Msg: Sending 10 packets on 6 multicast addresses
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly received 60 packets
      05be0212: ndt_2c Msg: Removing randomly 1 multicast addresses
      05be0212: ndt_2c Msg: Sending 10 packets on 67 unused multicast addresses
      05be0212: ndt_2c Msg: Sent 670 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly didn't receive packets
      05be0212: ndt_2c Msg: Sending 10 packets on 5 multicast addresses
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly received 50 packets
      05be0212: ndt_2c Msg: Removing randomly 1 multicast addresses
      05be0212: ndt_2c Msg: Sending 10 packets on 68 unused multicast addresses
      05be0212: ndt_2c Msg: Sent 680 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly didn't receive packets
      05be0212: ndt_2c Msg: Sending 10 packets on 4 multicast addresses
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly received 40 packets
      05be0212: ndt_2c Msg: Removing randomly 1 multicast addresses
      05be0212: ndt_2c Msg: Sending 10 packets on 69 unused multicast addresses
      05be0212: ndt_2c Msg: Sent 690 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly didn't receive packets
      05be0212: ndt_2c Msg: Sending 10 packets on 3 multicast addresses
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly received 30 packets
      05be0212: ndt_2c Msg: Removing randomly 1 multicast addresses
      05be0212: ndt_2c Msg: Sending 10 packets on 70 unused multicast addresses
      05be0212: ndt_2c Msg: Sent 700 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly didn't receive packets
      05be0212: ndt_2c Msg: Sending 10 packets on 2 multicast addresses
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly received 20 packets
      05be0212: ndt_2c Msg: Removing randomly 1 multicast addresses
      05be0212: ndt_2c Msg: Sending 10 packets on 71 unused multicast addresses
      05be0212: ndt_2c Msg: Sent 710 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly didn't receive packets
      05be0212: ndt_2c Msg: Sending 10 packets on 1 multicast addresses
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly received 10 packets
      05be0212: ndt_2c Msg: Removing randomly 1 multicast addresses
      05be0212: ndt_2c Msg: Sending 10 packets on 72 unused multicast addresses
      05be0212: ndt_2c Msg: Sent 720 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Properly didn't receive packets
      05be0212: ndt_2c Msg: Closing adapters
   END TEST: "2c_MulticastReceive", PASSED, Time=218.843
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   *** TEST COMPLETED
   ***
   *** Test Name:      2c_MulticastReceive
   *** Test ID:        4
   *** Library Path:   \ndt_2c.dll
   *** Command Line:   -t AX88179_178A1 -s AX88179_178A2
   *** Kernel Mode:    No
   *** Result:         Passed
   *** Random Seed:    3005
   *** Thread Count:   1
   *** Execution Time: 0:03:38.843
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   
   </TESTCASE RESULT="PASSED">
   <TESTCASE ID=5>
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   *** TEST STARTING
   ***
   *** Test Name:      2c_StressSend
   *** Test ID:        5
   *** Library Path:   \ndt_2c.dll
   *** Command Line:   -t AX88179_178A1 -s AX88179_178A2
   *** Kernel Mode:    No
   *** Random Seed:    9851
   *** Thread Count:   0
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "2c_StressSend", Threads=0, Seed=9851
      05be0212: ndt_2c Msg: Start 2c_StressSend test
      05be0212: ndt_2c Msg: The test adapter is AX88179_178A1
      05be0212: ndt_2c Msg: The support adapter is AX88179_178A2
      05be0212: ndt_2c Msg: Opening adapters
      05be0212: ndt_2c Msg: Binding adapters
      05be0212: ndt_2c Msg: Get basic adapters info
      05be0212: ndt_2c Msg: Seting direct receive filters
      05be0212: ndt_2c Msg: Test Pass #0
      05be0212: ndt_2c Msg: Start sending 10000 packets
      05be0212: ndt_2c Msg: Sent 10000 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Test: Sent 10000 packets with total size 7631416 bytes in 12859 ms
      05be0212: ndt_2c Msg: Test: Recv 10000 packets with total size 500000 bytes in 12859 ms
      05be0212: ndt_2c Msg: Support: Recv 10000 packets with total size 7771416 bytes in 12859 ms
      05be0212: ndt_2c Msg: Support: Sent 10000 packets with total size 500000 bytes in 12859 ms
      05be0212: ndt_2c Msg: Test Pass #1
      05be0212: ndt_2c Msg: Start sending 10000 packets
      05be0212: ndt_2c Msg: Sent 10000 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Test: Sent 10000 packets with total size 7669960 bytes in 12873 ms
      05be0212: ndt_2c Msg: Test: Recv 10000 packets with total size 500000 bytes in 12873 ms
      05be0212: ndt_2c Msg: Support: Recv 10000 packets with total size 7809960 bytes in 12873 ms
      05be0212: ndt_2c Msg: Support: Sent 10000 packets with total size 500000 bytes in 12873 ms
      05be0212: ndt_2c Msg: Test Pass #2
      05be0212: ndt_2c Msg: Start sending 10000 packets
      05be0212: ndt_2c Msg: Sent 10000 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Test: Sent 10000 packets with total size 7678112 bytes in 12862 ms
      05be0212: ndt_2c Msg: Test: Recv 10000 packets with total size 500000 bytes in 12862 ms
      05be0212: ndt_2c Msg: Support: Recv 10000 packets with total size 7818112 bytes in 12863 ms
      05be0212: ndt_2c Msg: Support: Sent 10000 packets with total size 500000 bytes in 12863 ms
      05be0212: ndt_2c Msg: Test Pass #3
      05be0212: ndt_2c Msg: Start sending 100 packets
      05be0212: ndt_2c Msg: Sent 100 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Test: Sent 100 packets with total size 8650 bytes in 120 ms
      05be0212: ndt_2c Msg: Test: Recv 100 packets with total size 5000 bytes in 120 ms
      05be0212: ndt_2c Msg: Support: Recv 100 packets with total size 10050 bytes in 120 ms
      05be0212: ndt_2c Msg: Support: Sent 100 packets with total size 5000 bytes in 120 ms
      05be0212: ndt_2c Msg: Test Pass #4
      05be0212: ndt_2c Msg: Start sending 53 packets
      05be0212: ndt_2c Msg: Sent 53 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Test: Sent 53 packets with total size 3339 bytes in 60 ms
      05be0212: ndt_2c Msg: Test: Recv 53 packets with total size 4081 bytes in 60 ms
      05be0212: ndt_2c Msg: Support: Recv 53 packets with total size 4081 bytes in 60 ms
      05be0212: ndt_2c Msg: Support: Sent 53 packets with total size 4081 bytes in 60 ms
      05be0212: ndt_2c Msg: Test Pass #5
      05be0212: ndt_2c Msg: Start sending 10000 packets
      05be0212: ndt_2c Msg: Sent 10000 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Test: Sent 10000 packets with total size 1000000 bytes in 12490 ms
      05be0212: ndt_2c Msg: Test: Recv 10000 packets with total size 500000 bytes in 12490 ms
      05be0212: ndt_2c Msg: Support: Recv 10000 packets with total size 1140000 bytes in 12490 ms
      05be0212: ndt_2c Msg: Support: Sent 10000 packets with total size 500000 bytes in 12490 ms
      05be0212: ndt_2c Msg: Test Pass #6
      05be0212: ndt_2c Msg: Start sending 10000 packets
      05be0212: ndt_2c Msg: Sent 10000 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Test: Sent 10000 packets with total size 7608522 bytes in 12934 ms
      05be0212: ndt_2c Msg: Test: Recv 10000 packets with total size 500000 bytes in 12934 ms
      05be0212: ndt_2c Msg: Support: Recv 10000 packets with total size 7748522 bytes in 12934 ms
      05be0212: ndt_2c Msg: Support: Sent 10000 packets with total size 500000 bytes in 12934 ms
      05be0212: ndt_2c Msg: Test Pass #7
      05be0212: ndt_2c Msg: Start sending 10000 packets
      05be0212: ndt_2c Msg: Sent 10000 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Test: Sent 10000 packets with total size 7611942 bytes in 12490 ms
      05be0212: ndt_2c Msg: Test: Recv 0 packets with total size 0 bytes in 12490 ms
      05be0212: ndt_2c Msg: Support: Recv 10000 packets with total size 7751942 bytes in 12490 ms
      05be0212: ndt_2c Msg: Support: Sent 0 packets with total size 0 bytes in 12490 ms
      05be0212: ndt_2c Msg: Test Pass #8
      05be0212: ndt_2c Msg: Start sending 10000 packets
      05be0212: ndt_2c Msg: Sent 10000 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Test: Sent 10000 packets with total size 7772381 bytes in 12792 ms
      05be0212: ndt_2c Msg: Test: Recv 10000 packets with total size 7912381 bytes in 12792 ms
      05be0212: ndt_2c Msg: Support: Recv 10000 packets with total size 7912381 bytes in 12792 ms
      05be0212: ndt_2c Msg: Support: Sent 10000 packets with total size 7912381 bytes in 12792 ms
      05be0212: ndt_2c Msg: Test Pass #9
      05be0212: ndt_2c Msg: Start sending 10000 packets
      05be0212: ndt_2c Msg: Sent 10000 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Test: Sent 10000 packets with total size 600000 bytes in 12489 ms
      05be0212: ndt_2c Msg: Test: Recv 10000 packets with total size 740000 bytes in 12489 ms
      05be0212: ndt_2c Msg: Support: Recv 10000 packets with total size 740000 bytes in 12489 ms
      05be0212: ndt_2c Msg: Support: Sent 10000 packets with total size 740000 bytes in 12489 ms
      05be0212: ndt_2c Msg: Unbinding adapters
      05be0212: ndt_2c Msg: Closing adapters
   END TEST: "2c_StressSend", PASSED, Time=123.095
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   *** TEST COMPLETED
   ***
   *** Test Name:      2c_StressSend
   *** Test ID:        5
   *** Library Path:   \ndt_2c.dll
   *** Command Line:   -t AX88179_178A1 -s AX88179_178A2
   *** Kernel Mode:    No
   *** Result:         Passed
   *** Random Seed:    9851
   *** Thread Count:   1
   *** Execution Time: 0:02:03.095
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   
   </TESTCASE RESULT="PASSED">
   <TESTCASE ID=6>
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   *** TEST STARTING
   ***
   *** Test Name:      2c_StressReceive
   *** Test ID:        6
   *** Library Path:   \ndt_2c.dll
   *** Command Line:   -t AX88179_178A1 -s AX88179_178A2
   *** Kernel Mode:    No
   *** Random Seed:    32207
   *** Thread Count:   0
   *** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "2c_StressReceive", Threads=0, Seed=32207
      05be0212: ndt_2c Msg: Start 2c_StessReceive test
      05be0212: ndt_2c Msg: The test adapter is AX88179_178A1
      05be0212: ndt_2c Msg: The support adapter is AX88179_178A2
      05be0212: ndt_2c Msg: Opening adapters
      05be0212: ndt_2c Msg: Binding adapters
      05be0212: ndt_2c Msg: Get basic adapters info
      05be0212: ndt_2c Msg: Seting direct receive filters
      05be0212: ndt_2c Msg: Test Pass #0
      05be0212: ndt_2c Msg: Start sending 10000 packets
      05be0212: ndt_2c Msg: Sent 10000 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Support: Sent 10000 packets with total size 7628292 bytes in 12558 ms
      05be0212: ndt_2c Msg: Support: Recv 10000 packets with total size 500000 bytes in 12558 ms
      05be0212: ndt_2c Msg: Test: Recv 10000 packets with total size 7768292 bytes in 12559 ms
      05be0212: ndt_2c Msg: Test: Sent 10000 packets with total size 500000 bytes in 12559 ms
      05be0212: ndt_2c Msg: Test Pass #1
      05be0212: ndt_2c Msg: Start sending 10000 packets
      05be0212: ndt_2c Msg: Sent 10000 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Support: Sent 10000 packets with total size 7696761 bytes in 12550 ms
      05be0212: ndt_2c Msg: Support: Recv 10000 packets with total size 500000 bytes in 12550 ms
      05be0212: ndt_2c Msg: Test: Recv 10000 packets with total size 7836761 bytes in 12551 ms
      05be0212: ndt_2c Msg: Test: Sent 10000 packets with total size 500000 bytes in 12551 ms
      05be0212: ndt_2c Msg: Test Pass #2
      05be0212: ndt_2c Msg: Start sending 10000 packets
      05be0212: ndt_2c Msg: Sent 10000 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Support: Sent 10000 packets with total size 7682596 bytes in 12573 ms
      05be0212: ndt_2c Msg: Support: Recv 10000 packets with total size 500000 bytes in 12573 ms
      05be0212: ndt_2c Msg: Test: Recv 10000 packets with total size 7822596 bytes in 12573 ms
      05be0212: ndt_2c Msg: Test: Sent 10000 packets with total size 500000 bytes in 12573 ms
      05be0212: ndt_2c Msg: Test Pass #3
      05be0212: ndt_2c Msg: Start sending 100 packets
      05be0212: ndt_2c Msg: Sent 100 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Support: Sent 100 packets with total size 8650 bytes in 120 ms
      05be0212: ndt_2c Msg: Support: Recv 100 packets with total size 5000 bytes in 120 ms
      05be0212: ndt_2c Msg: Test: Recv 100 packets with total size 10050 bytes in 120 ms
      05be0212: ndt_2c Msg: Test: Sent 100 packets with total size 5000 bytes in 120 ms
      05be0212: ndt_2c Msg: Test Pass #4
      05be0212: ndt_2c Msg: Start sending 53 packets
      05be0212: ndt_2c Msg: Sent 53 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Support: Sent 53 packets with total size 3339 bytes in 60 ms
      05be0212: ndt_2c Msg: Support: Recv 53 packets with total size 4081 bytes in 60 ms
      05be0212: ndt_2c Msg: Test: Recv 53 packets with total size 4081 bytes in 60 ms
      05be0212: ndt_2c Msg: Test: Sent 53 packets with total size 4081 bytes in 60 ms
      05be0212: ndt_2c Msg: Test Pass #5
      05be0212: ndt_2c Msg: Start sending 10000 packets
      05be0212: ndt_2c Msg: Sent 10000 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Support: Sent 10000 packets with total size 1000000 bytes in 12490 ms
      05be0212: ndt_2c Msg: Support: Recv 10000 packets with total size 500000 bytes in 12490 ms
      05be0212: ndt_2c Msg: Test: Recv 10000 packets with total size 1140000 bytes in 12490 ms
      05be0212: ndt_2c Msg: Test: Sent 10000 packets with total size 500000 bytes in 12490 ms
      05be0212: ndt_2c Msg: Test Pass #6
      05be0212: ndt_2c Msg: Start sending 10000 packets
      05be0212: ndt_2c Msg: Sent 10000 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Support: Sent 10000 packets with total size 7727615 bytes in 12545 ms
      05be0212: ndt_2c Msg: Support: Recv 10000 packets with total size 500000 bytes in 12545 ms
      05be0212: ndt_2c Msg: Test: Recv 10000 packets with total size 7867615 bytes in 12546 ms
      05be0212: ndt_2c Msg: Test: Sent 10000 packets with total size 500000 bytes in 12546 ms
      05be0212: ndt_2c Msg: Test Pass #7
      05be0212: ndt_2c Msg: Start sending 10000 packets
      05be0212: ndt_2c Msg: Sent 10000 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Support: Sent 10000 packets with total size 7605615 bytes in 12490 ms
      05be0212: ndt_2c Msg: Support: Recv 0 packets with total size 0 bytes in 12490 ms
      05be0212: ndt_2c Msg: Test: Recv 10000 packets with total size 7745615 bytes in 12491 ms
      05be0212: ndt_2c Msg: Test: Sent 0 packets with total size 0 bytes in 12491 ms
      05be0212: ndt_2c Msg: Test Pass #8
      05be0212: ndt_2c Msg: Start sending 10000 packets
      05be0212: ndt_2c Msg: Sent 10000 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Support: Sent 10000 packets with total size 7681709 bytes in 12612 ms
      05be0212: ndt_2c Msg: Support: Recv 10000 packets with total size 7821709 bytes in 12612 ms
      05be0212: ndt_2c Msg: Test: Recv 10000 packets with total size 7821709 bytes in 12613 ms
      05be0212: ndt_2c Msg: Test: Sent 10000 packets with total size 7821709 bytes in 12613 ms
      05be0212: ndt_2c Msg: Test Pass #9
      05be0212: ndt_2c Msg: Start sending 10000 packets
      05be0212: ndt_2c Msg: Sent 10000 packets
      05be0212: ndt_2c Msg: Stop receiving and checking results
      05be0212: ndt_2c Msg: Support: Sent 10000 packets with total size 600000 bytes in 12490 ms
      05be0212: ndt_2c Msg: Support: Recv 10000 packets with total size 740000 bytes in 12490 ms
      05be0212: ndt_2c Msg: Test: Recv 10000 packets with total size 740000 bytes in 12490 ms
      05be0212: ndt_2c Msg: Test: Sent 10000 packets with total size 740000 bytes in 12490 ms
      05be0212: ndt_2c Msg: Unbinding adapters
      05be0212: ndt_2c Msg: Closing adapters
   END TEST: "2c_StressReceive", PASSED, Time=121.619
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   *** TEST COMPLETED
   ***
   *** Test Name:      2c_StressReceive
   *** Test ID:        6
   *** Library Path:   \ndt_2c.dll
   *** Command Line:   -t AX88179_178A1 -s AX88179_178A2
   *** Kernel Mode:    No
   *** Result:         Passed
   *** Random Seed:    32207
   *** Thread Count:   1
   *** Execution Time: 0:02:01.619
   *** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
   
   </TESTCASE RESULT="PASSED">
END GROUP: ndt_2c.dll
*** ==================================================================
*** MEMORY INFO
***
*** Memory Total:   746,651,648 bytes
*** Memory Used:     28,278,784 bytes
*** Memory Free:    718,372,864 bytes
***
*** Kernel Used:        761,856 bytes
*** Water Mark:         175,170 pages
***
*** Store Total:    133,971,968 bytes
*** Store Used:       1,314,816 bytes
*** Store Free:     132,657,152 bytes
*** ==================================================================

*** ==================================================================
*** SUITE SUMMARY
***
*** Passed:          6
*** Failed:          0
*** Skipped:         0
*** Aborted:         0
*** -------- ---------
*** Total:           6
***
*** Cumulative Test Execution Time: 0:18:47.338
*** Total Tux Suite Execution Time: 0:18:48.406
*** CPU Idle Time:                  0:18:36.074
*** ==================================================================
</TESTGROUP>
@@@@@@0

